

Recommendation for Space Data System Standards

|  |
| --- |
| CCSDS Global Spacecraft Identifier Field:Code Assignment Control Procedures |



MAGENTA Book

June 2016

AUTHORITY

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | Issue: | , 7 |  |
|  | Date: | 6 |  |
|  | Location: | Washington, DC, USA |  |
|  |  |  |  |

This document has been approved for publication by the Management Council of the Consultative Committee for Space Data Systems (CCSDS) and represents the consensus technical agreement of the participating CCSDS Member Agencies. The procedure for review and authorization of CCSDS documents is detailed in *Organization and Processes for the Consultative Committee for Space Data Systems* (CCSDS A02.1-Y-4), and the record of Agency participation in the authorization of this document can be obtained from the CCSDS Secretariat at the address below.

This document is published and maintained by:

CCSDS Secretariat

Space Communications and Navigation Office, 7L70

Space Operations Mission Directorate

NASA Headquarters

Washington, DC 20546-0001, USA

STATEMENT OF INTENT

The Consultative Committee for Space Data Systems (CCSDS) is an organization officially established by the management of its members. The Committee meets periodically to address data systems problems that are common to all participants, and to formulate sound technical solutions to these problems. Inasmuch as participation in the CCSDS is completely voluntary, the results of Committee actions are termed **Recommended Practice** and are not considered binding on any Agency.

This **Recommended Practice** is issued by, and represents the consensus of, the CCSDS members. Endorsement of this **Recommendation** is entirely voluntary. Endorsement, however, indicates the following understandings:

o Whenever a member establishes a CCSDS-related **practice** , this **practice** will be in accord with the relevant **Recommended Practice** . Establishing such a **practice** does not preclude other provisions which a member may develop.

o Whenever a member establishes a CCSDS-related **practice** , that member will provide other CCSDS members with the following information:

 -- The **practice** itself.

 -- The anticipated date of initial operational capability.

 -- The anticipated duration of operational service.

o Specific service arrangements shall be made via memoranda of agreement. Neither this **Recommended Practice** nor any ensuing **practice** is a substitute for a memorandum of agreement.

No later than three years from its date of issuance, this **Recommended Practice** will be reviewed by the CCSDS to determine whether it should: (1) remain in effect without change; (2) be changed to reflect the impact of new technologies, new requirements, or new directions; or (3) be retired or canceled.

In those instances when a new version of a **Recommended Practice** is issued, existing CCSDS-related member **practices** and implementations are not negated or deemed to be non-CCSDS compatible. It is the responsibility of each member to determine when such **practices** or implementations are to be modified. Each member is, however, strongly encouraged to direct planning for its new practices and implementations towards the later version of the Recommended **Practice** .

FOREWORD

This document is a Recommended **Practice** that establishes control procedures for Spacecraft Identifier (SCID) codes. As such, it defines the procedure governing assignment, relinquishment, and management of SCIDs.

To make the most efficient use of the available identification space in the several CCSDS-recommended data structures that contain a SCID field, all CCSDS-compatible missions are assigned SCIDs by the Space Assigned Numbers Authority (SANA).

As specified in this Recommended **Practice** , SANA accepts only requests from designated Agency Representatives and only when received via the approved Request web interface.

This Recommended **Practice** also describes a web interface to be used for requesting and relinquishing SCIDs.

Through the process of normal evolution, it is expected that expansion, deletion, or modification of this document may occur. This Recommended **Practice** is therefore subject to CCSDS document management and change control procedures, which are defined in the *Organization and Processes for the Consultative Committee for Space Data Systems* (CCSDS A02.1-Y-4). Current versions of CCSDS documents are maintained at the CCSDS Web site:

http://www.ccsds.org/

Questions relating to the contents or status of this document should be addressed to the CCSDS Secretariat at the address indicated on page i.

At time of publication, the active Member and Observer Agencies of the CCSDS were:

Member Agencies

* Agenzia Spaziale Italiana (ASI)/Italy.
* Canadian Space Agency (CSA)/Canada.
* Centre National d’Etudes Spatiales (CNES)/France.
* China National Space Administration (CNSA)/People’s Republic of China.
* Deutsches Zentrum für Luft- und Raumfahrt (DLR)/Germany.
* European Space Agency (ESA)/Europe.
* Federal Space Agency (FSA)/Russian Federation.
* Instituto Nacional de Pesquisas Espaciais (INPE)/Brazil.
* Japan Aerospace Exploration Agency (JAXA)/Japan.
* National Aeronautics and Space Administration (NASA)/USA.
* UK Space Agency/United Kingdom.

Observer Agencies

* Austrian Space Agency (ASA)/Austria.
* Belgian Federal Science Policy Office (BFSPO)/Belgium.
* Central Research Institute of Machine Building (TsNIIMash)/Russian Federation.
* China Satellite Launch and Tracking Control General, Beijing Institute of Tracking and Telecommunications Technology (CLTC/BITTT)/China.
* Chinese Academy of Sciences (CAS)/China.
* Chinese Academy of Space Technology (CAST)/China.
* Commonwealth Scientific and Industrial Research Organization (CSIRO)/Australia.
* Danish National Space Center (DNSC)/Denmark.
* Departamento de Ciência e Tecnologia Aeroespacial (DCTA)/Brazil.
* European Organization for the Exploitation of Meteorological Satellites (EUMETSAT)/Europe.
* European Telecommunications Satellite Organization (EUTELSAT)/Europe.
* Geo-Informatics and Space Technology Development Agency (GISTDA)/Thailand.
* Hellenic National Space Committee (HNSC)/Greece.
* Indian Space Research Organization (ISRO)/India.
* Institute of Space Research (IKI)/Russian Federation.
* KFKI Research Institute for Particle & Nuclear Physics (KFKI)/Hungary.
* Korea Aerospace Research Institute (KARI)/Korea.
* Ministry of Communications (MOC)/Israel.
* National Institute of Information and Communications Technology (NICT)/Japan.
* National Oceanic and Atmospheric Administration (NOAA)/USA.
* National Space Agency of the Republic of Kazakhstan (NSARK)/Kazakhstan.
* National Space Organization (NSPO)/Chinese Taipei.
* Naval Center for Space Technology (NCST)/USA.
* Scientific and Technological Research Council of Turkey (TUBITAK)/Turkey.
* South African National Space Agency (SANSA)/Republic of South Africa.
* Space and Upper Atmosphere Research Commission (SUPARCO)/Pakistan.
* Swedish Space Corporation (SSC)/Sweden.
* Swiss Space Office (SSO)/Switzerland.
* United States Geological Survey (USGS)/USA.

DOCUMENT CONTROL

|  |  |  |  |
| --- | --- | --- | --- |
| **Document** | **Title** | **Date** | **Status** |
| CCSDS 320.0-B-1 | CCSDS Global Spacecraft Identification Field: Code Assignment Control Procedures, Issue 1 | October 1993 | Original Issue (superseded) |
| CCSDS 320.0-B-2 | CCSDS Global Spacecraft Identification Field: Code Assignment Control Procedures, Issue 2 | November1998 | Superseded  |
| CCSDS 320.0-B-3 | CCSDS Global Spacecraft Identification Field: Code Assignment Control Procedures, Issue 3 | April2003 | Superseded |
| CCSDS 320.0-B-4 | CCSDS Global Spacecraft Identification Field: Code Assignment Control Procedures, Issue 4 | January 2006 | Superseded |
| CCSDS 320.0-B-5 | CCSDS Global Spacecraft Identification Field: Code Assignment Control Procedures, Issue 5 | September 2007 | Superseded |
| CCSDS 320.0-B-6 | ,  |  | Previous issue (note):* designates SANA as official registrar for SCIDs and ARs;
* reorganizes document for conformance with modern CCSDS publication requirements, rephrases some statements for clarity, and eliminates obsolete material.
 |
| Cor. 1 | Technical Corrigendum 1 |  | Clarifies procedure on page 3-3.NOTE – Changes from the previous issue are too extensive to permit markup. |
| CCSDS 320.0-M-7 | , 7 | 6 | Current issue:* changed to Magenta Book to align with CCSDS Org & Proc definitions
* aligned with CCSDS Registry Management Policy CCSDS 313.1-Y-0.1
* adopts use of CCSDS Organization and Contact registries from CCSDS 313.1-Y-0.1
* Adopts separate frequency bins for SCID assignment
 |

CONTENTS

Section Page

1 INTRODUCTION 1-1

1.1 Purpose 1-1

1.2 Background 2-1

1.3 Global Spacecraft Identifier (GSCID) 1-2

1.4 Applicability 1-1

1.5 REFERENCEs 1-3

2 SCID CODE ASSIGNMENT CONTROL PROCEDURES 3-1

2.1 CCSDS SCID Management System Duties and
Responsibilities 3-1

2.2 SCID Assignment Request Procedures 3-2

2.3 SCID Code Assignment Procedures 3-3

2.4 SCID Relinquishing Procedures 3-4

ANNEX A SCID REQUEST FORM (Normative) A-1

ANNEX B ACRONYMS AND ABBREVIATIONS (Informative) B-1

Table

1-1Bit Structure of Currently Defined VN Fields 1-2

# INTRODUCTION

## Purpose

This Recommended **Practice** establishes the procedures governing requesting, assigning, and relinquishing CCSDS Spacecraft Identifier (SCID) field codes, which are specified in the data unit formats defined in references [1], [2], [3], and [4]. It specifies the organizations and personnel authorized to participate in the performance of those procedures, the requirements for configuration management, and the acceptable use of SCIDs.

## Applicability

This Recommended **Practice** applies to users of the CCSDS protocols defined in references [1], [2], [3], and [4]. These procedures shall be followed by all organizations who require a spacecraft identifier to use CCSDS protocols for space communication and by the SANA, which registers these identifiers.

## NOMENCLATURE

### Normative Text

The following conventions apply for the normative specifications in this Recommended **Practice** :

1. the words ‘shall’ and ‘must’ imply a binding and verifiable specification;
2. the word ‘should’ implies an optional, but desirable, specification;
3. the word ‘may’ implies an optional specification;
4. the words ‘is’, ‘are’, and ‘will’ imply statements of fact.

NOTE – These conventions do not imply constraints on diction in text that is clearly informative in nature.

### Informative Text

In the normative sections of this document, informative text is set off from the normative specifications either in notes or under one of the following subsection headings:

* Overview;
* Background;
* Rationale;
* Discussion.

## Definitions

**Agency Representative, AR**: An individual designated by a CCSDS Agency Head of Delegation as the person authorized to request and relinquish SCIDs on behalf of the respective agency.

**CCSDS Agency**: A CCSDS Member or Observer Agency.

**CCSDS Agency Head of Delegation**: The individual who serves as principal representative of a CCSDS Agencyin dealings with the CCSDS. The CCSDS Agency HoD for a Member Agency is usually the CMC member.

NOTE - Affiliate organizations (Associates or Liaisons) make requests via the AR for their country. If there is no CCSDS agency for their country they may petition the Secretariat to be assigned the responsibility for their country.

**Frequency Band (FB):** The discrete sets of frequencies that have been identified as frequency bands (FB) by the International Telecommunications Union (ITU), with letter designations (derived from [IEEE Std 521-2002 *Standard Letter Designations for Radar-Frequency Bands*](http://standards.ieee.org/findstds/standard/521-2002.html)).

**Global Spacecraft Identifier, GSCID**: The concatenation of the 2-bit Version Number (VN) and the SCID. Thus,

GSCID = VN **.** SCID

Where ‘**.**’ refers to the concatenation operator.

**Object Identifier (OID)**: the unique ISO identifier assigned to every spacecraft registered in the CCSDS spacecraft registry. [9]

NOTE - while the SCID is only valid for the operational lifetime of the mission the OID is permanently assigned.

**Qualified Spacecraft Identifier, Q-SCID**: The concatenation of the frequency band (FB), 2-bit Version Number (VN) and the SCID. Thus,

Q-SCID = FB **.** VN **.** SCID

Where ‘**.**’ refers to the concatenation operator.

**Spacecraft Identifier, SCID**: A value used in specified fields of CCSDS-defined data structures.

NOTE – Other non-CCSDS-compatible data structures may also use this term; however, this document does not apply to the assignment and use of identification codes for non-CCSDS-compatible data structures. In such cases the potential for misinterpretation is negligible because of differences in the overall data structures.

**Version Number, VN**: A field value used to differentiate CCSDS-defined transfer frames. The valid range of the currently defined VN field is shown in table 1‑1.

NOTE –The association of the VN with the spacecraft is a managed parameter. Any spacecraft that uses more than one one protocol with a different VN may require that two (or more) completely separate and distinct SCIDs be assigned.

Table 1‑ : Bit Structure of Currently Defined VN Fields

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Version** | **Binary****Encoded****VN**  | **Range of SCID** | **No. of Bits****in SCID****Encoded** | **Relevant****CCSDS****Documents** |
| 1 | 00 | 0–1,023 | 10 | Ref. [1] & [2] |
| 23 | 0110 | 0–255 0–1,023 | 810 | Ref. [3]Ref. [4] |
| NOTE – The binary encoded VN value of ‘11’ is reserved for possible future use and should not be used for project-unique purposes prior to formal agreement within CCSDS for such use. |

 NOTE - There is, in effect, a separate set of Q-SCID registry entries for each protocol version number and each frequency bin that a spacecraft is assigned to use, such as X-band uplink, X and Ka-band downlink. While it is to be avoided if at all possible, one spacecraft may have more than one SCID assigned in these different VN & frequency bins. See Annex C which defines the characteristics of the registries that are to be used for this procedure.

## References

The following publications contain provisions which, through reference in this text, constitute provisions of this document. At the time of publication, the editions indicated were valid. All publications are subject to revision, and users of this document are encouraged to investigate the possibility of applying the most recent editions of the publications indicated below. The CCSDS Secretariat maintains a register of currently valid CCSDS publications.

[] *TC Space Data Link Protocol*. Issue 2. Recommendation for Space Data System Standards (Blue Book), CCSDS 232.0-B-2. Washington, D.C.: CCSDS, September 2010.

[] *TM Space Data Link Protocol*. Issue 1. Recommendation for Space Data System Standards (Blue Book), CCSDS 132.0-B-1. Washington, D.C.: CCSDS, September 2003

[] *AOS Space Data Link Protocol*. Issue 2. Recommendation for Space Data System Standards (Blue Book), CCSDS 732.0-B-2. Washington, D.C.: CCSDS, July 2006.

[4] *Proximity-1 Space Link Protocol—Data Link Layer*. Issue 4. Recommendation for Space Data System Standards (Blue Book), CCSDS 211.0-B-4. Washington, D.C.: CCSDS, July 2006.

[] “Agency Representatives.” Space Assigned Number Authority. <http://sanaregistry.org/r/agency_representatives>.

[] “Spacecraft Identifiers.” Space Assigned Number Authority. <http://sanaregistry.org/r/spacecraftid>

[] “CCSDS Organization Registry” Space Assigned Number Authority. http://sanaregistry.org/r/organizations

[] “CCSDS Contact Registry” Space Assigned Number Authority. <http://sanaregistry.org/r/contact>s

[] “CCSDS OID Registry” Space Assigned Number Authority. http://sanaregistry.org/r/oid

[10] *Space Assigned Numbers Authority (SANA)--Role, Responsibilities, Policies, and Procedures*, CCSDS 313.0-Y-2, May 2016

[11] *CCSDS Registry Management Policy,* CCSDS 313.1-Y-1, June 2016

# Overview

## Purpose of the CCSDS Q-SCID

The CCSDS Q-SCID serves as a mechanism for the identification of:

– a simple spacecraft having only one logical space-ground link in a single frequency band; or

– an association between space-based and ground-based application processes with complex spacecraft having more than one logical space-ground link operating at different frequencies. Therefore, a single spacecraft may be assigned more than one GSCID.

The procedures contained in this document are intended to eliminate the possibility that

* data from any given CCSDS-compatible vehicle will be falsely interpreted as being from another CCSDS-compatible vehicle during the periods of mission operations; and that
* commands sent to a CCSDS-compatible vehicle will be received and acted upon by application processes for which they were not intended.

Since the space link data structures (synchronization code and virtual channel data unit/transfer frame/telecommand frame) are common to many missions, misinterpretation of the identity of space vehicle is possible unless procedures are developed and followed to identify uniquely each vehicle or assembly during its active phases. Different missions also are assigned spectrum in one or more frequency bands, so this separation of frequency band use also provides effective isolation for what are treated as separate namespaces. This document defines the assignment procedures that ensure assignment of one (or more) unique qualified spacecraft identifiers (Q-SCID) based on the frequency band(s) in use.

Because the SCID field in the various CCSDS transfer frames is used to discriminate among operational spacecraft, and the fields are only eight or ten bits long, the SCID is not intended to provide a unique identifier for the spacecraft and its data for all times. Because of the increasing numbers of operational spacecraft there is a concern that, at any one time, the number of vehicles under active operational control not exceed the namespace in the available allocation domains. It is inevitable that the SCIDs will have to be reused and there is a procedure for relinquishing them.

In order to directly address these concerns the Q-SCID allocation domains address the following considerations:

1. Separate SCID number assignment tables for each different protocol Version Number (VN).
2. Separate Q-SCID number assignment tables for each frequency band / bin for each VN.
3. Any spacecraft using more than one protocol, and/or more than one frequency band, may have two, or more, separate Q-SCIDs assigned, potentially in different frequency bins.
4. The assignment process will attempt to allocate the same SCID in each allocation domain, but this is not guaranteed.

The SANA, which performs Q-SCID assignments and manages the namespaces, will no longer assign SCIDs for simulation and testing, nor for ground based simulators or assemblies. Since these activities do not involve free space radiation there is no possibility of confusion between an operating spacecraft and a simulator. Missions may wish to assign separate simulation and test SCIDs to manage their own internal datasets, but this must be done by the missions themselves, or an agency or center can define how to manage it internally as a local matter.

In addition to the assignment of Q-SCIDs during the active operational lifetime, the SCID assignment process also provides a separate unique and permanent identifier for each spacecraft. In order to provide a unique, unambiguous, persistent spacecraft identifier the Q-SCID registration process also assigns a globally unique object identifier (OID), reference [9]. The OID is a permanent identifier for each spacecraft that may be used as a persistent identification for the spacecraft and its data.

NOTE - it is possible for an organization to request an OID assignment for a spacecraft, simulator, or assembly that does not have a Q-SCID assigned. Any spacecraft that receives communication services from a CCSDS agency or other service provider may have an OID assigned.

## Background

SCID codes appear in many of the CCSDS-recommended data structures used for the space-ground links and other purposes. Typical of the space-ground data structures that incorporate the SCID are:

– the conventional mission telemetry frame (reference [2]);

– the conventional mission telecommand transfer frame (reference [1]);

– the Advanced Orbiting Systems Virtual Channel Data Unit (reference [3]);

* the Proximity-1 transfer frame (reference [4]);

The CCSDS Recommended Standards on Data Link Layer protocols (references [1], [2], [3], [4] provide a mechanism for establishing a link layer association (either temporary or permanent) between space-based application process(es) and corresponding ground-based application process(es).

The data streams transmitted between space and ground processes contain identifiers that specify the relevant association. These identifiers are managed parameters (i.e., the specific association implied by a given identifier must have been previously established by agreement between service user and service provider). The utilization of the SCID field on a global scale necessitates its concatenation with the FB and VN of the protocol data structure in which it is used; the concatenation of FB, VN, and SCID is the Qualified SCID or Q-SCID.

The International Telecommunications Union (ITU) is the United Nations specialized agency, that, among other responsibilities, allocates global radio frequency spectrum and facilitates international coordination/notification for space systems and their earth stations. The World Radiocommunication Conferences (WRC) are held periodically to recommend allocation of frequency bands to radio services.  Every space agency sends representatives, as part of their administration’s delegation, to the WRC in order to protect valuable spectrum required for space science.  Each agency also has a spectrum manager who is responsible for selection and coordination of frequencies for their agency’s spacecraft.

Table 2-1 has the discrete sets of frequencies that have been identified as frequency bands (FB), with the following letter designations (derived from [IEEE Std 521-2002 *Standard Letter Designations for Radar-Frequency Bands*](http://standards.ieee.org/findstds/standard/521-2002.html)).

**Table 2-1 ITU / IEEE Frequency Bands**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IEEE FB Name** | **Near Earth Downlink** | **Abrv** | **Deep Space Downlink** | **Abrv** |
| HF-band  **0-30 MHz**  | Same | HF | Same | HF |
| VHF-band  **30-300 MHz**  | Same | VHF | Same | VHF |
| UHF-band  **300-1000 MHz** | Same | UHF | Same | UHF |
| L-band  **1-2 GHz** | Same | L | Same | L |
| S-Band  **2-4 GHz** | 2200-2290 MHz | S-NE | 2290-2300 MHz | S-DS |
| C-Band  **4-7 GHz** | 3400-4200 MHz  | C | N/A | C |
| X-Band SRS **7-12 GHz** | 8450-8500 MHz | XS-NE | 8400-8450 MHz | XS-DS |
| X-Band EESS **7-12 GHz** | 8025-8400 MHz | XE-NE | N/A | XE-DS |
| Ku-Band **12-18 GHz**  | 13.4-15.35 GHz  | Ku | N/A | Ku |
| K-Band **18-27 GHz** |  | K |  | K |
| Ka-Band SRS or EESS **27-40 GHz** | 25.5 - 27 GHz | Ka-NE | 31.8 – 32.3 GHz | Ka-DS |
| V-Band **40-75 GHz** (future) |  | V |  | V |
| W-Band **75-110 GHz** (future) |  | W |  | W |
| Optical 1064 nm (future) |  | O1 |  | O1 |
| Optical 1550 nm (future) |  | O2 |  | O2 |

Only the downlink frequencies are shown. The uplink frequencies that are used for any given satellite may just be an offset in the same frequency band range, i.e. 2-4 GHz, or they may actually be in a different frequency band, i.e. Ka band downlink and K-band uplink. In some cases these may be called “Ka-band”, or “Ku-band” mission allocations but the actual frequency bands that are in use are, numerically, different than that. As a result the Q-SCID request must specify the actual frequency band name and frequency range separately for both uplink and downlink separately so as to avoid confusion. It is not required to specify the actual frequencies in use, but the correct band designator, for uplink and downlink, must be provided.

It is expected that every spacecraft, early in its development process, will acquire a frequency allocation for uplink and downlink. The Q-SCID assignment procedures require that each registered spacecraft specify the one (or more) frequency bands that they have been allocated by their agency spectrum manager. Spacecraft may also use different link layer protocols for uplink and downlink. The assignment of one or more Q-SCIDs will be done relative to the number of frequency bands that a spacecraft uses, but for operational convenience every attempt will be made to assign the same SCID in all bands if that is possible.

# SCID CODE ASSIGNMENT CONTROL PROCEDURES

## CCSDS SCID Management System Duties and Responsibilities

### Overview

CCSDS SCID assignment and management, on an international basis, must be viewed as a cooperative effort among the CCSDS Agencies, with each constituent acting as agent for the users under its cognizance. The management system comprises four elements:

* the CCSDS Secretariat;
* the CCSDS Agency Heads of Delegation;
* the Agency Representatives;
* the Space Assigned Numbers Authority (SANA).

### CCSDS Secretariat Responsibilities

The CCSDS Secretariat shall

* serve as the focal point for the resolution of any issues not adequately covered by these procedures;
* act as intermediary for SCID requests from organizations not affiliated with a CCSDS Agency by assigning an existing AR to handle the request.
* handle any necessary updates to the official lists of CCSDS Agencies and to the Agency Head’s of Delegation

NOTE – The official list of CCSDS Agencies may be viewed at reference [7]. The official list of CCSDS Agency Head’s of Delegation may be viewed at reference [8]. The Secretariat is also responsible for synchronizing these official registries with those maintained in the SANA.

### CCSDS Agency Head of Delegation Responsibilities

Each CCSDS Agency Head of Delegation shall appoint an official Agency Representative to handle all SCID requests from his or her Agency.

As needed, CCSDS Agency Heads of Delegation shall provide current AR name and contact information using a web form found at reference [5], or via e-mail to info@sanaregistry.org with CC to secretariat@mailman.ccsds.org.

NOTE – The official list of ARs may be viewed at reference [5].

The CCSDS Agency Heads of Delegation shall update the AR name and contact information in the SANA whenever there is a change. This may be done using a web form found at reference [5] or via e-mail to info@sanaregistry.org with CC to secretariat@mailman.ccsds.org.

NOTE - The SANA web pages include a web form requiring authenticated access for any registry changes. The SANA will verify correct permissions before making changes to any of these entries.

### Agency Representative Responsibilities

The Agency Representative shall:

– submit Q-SCID requests in accordance with the provisions of this Recommended Practice;

– interact directly with SANA with regard to any issues relating to a specific Q-SCID assignment request;

– monitor the life of those CCSDS missions within his or her agency and relinquish all Q-SCIDs at the earliest practical time, which shall not in any event be later than two months after the last communication with the spacecraft;

– inform the applicable agency personnel of any relevant actions (i.e., Q-SCID assignment, relinquishment) taken by SANA relating to that agency.

### SANA Responsibilities

SANAshall

* maintain the on-line list of Agencies [7];
* maintain the on-line list of Agency HoD [8];
* maintain the official list of ARs [5];
* serve as the Q-SCID assignment manager;
* accept, from authorized ARs, requests for Q-SCID assignments;
* review and log Q-SCID assignment requests;
* assign one or more Q-SCIDs in the assigned frequency bin in response to requests and notify the appropriate AR of the assignment(s) [6];
* assign a unique, persistent, OID for each spacecraft in response to the request and notify the appropriate AR of the assignment(s) [9];

– interact directly with the appropriate AR in matters dealing with a particular Q-SCID or OID assignment request;

– maintain complete and independent sets of Q-SCID assignments for each frequency bin (FB) and protocol version number (VN) as registries on the SANA site;

NOTE – The official list of Q-SCIDs is maintained at reference [6].

* maintain a reference to the spacecraft OID assignments for each protocol version number as a registry on the SANA site;
* optionally record, in the spacecraft OID registry, the name, abbreviation, and any aliases for the spacecraft;

NOTE – The official list of OID assignments is maintained at reference [9].

* work with the respective ARs to recover all Q-SCIDs, corresponding to those spacecraft whose operational phases have been completed, for subsequent reassignment.

### SANA REGISTRY EXTENSIONS

This document references registries, such as the Organization and Contact registries, that have been defined in other documents [5], [7], [8], [9]. Similarly, this document defines a registry [6] that may be referenced in other standards. Furthermore, the Agency Representative registry, in particular, may be extended by other standards as the means to unambiguously identify specific Agency Representatives who have roles and responsibilities for managing the registration of different types of information than Q-SCIDs.

## Q-SCID CODE Lifetime

An assigned Q-SCID may be used throughout a spacecraft’s active operational phases, e.g., prelaunch testing, launch, and on-orbit operations.

As quickly as practical after reception of telemetry data, the SCID should be replaced with the OID, a globally unique, unambiguous, permanent, label for the spacecraft and/or payload data set(s) that is independent of the SCID.

NOTE – A globally unique, persistent, OID is created and assigned to the spacecraft for this purpose. It may be used during the entire operational life of the spacecraft and persists after termination of active operations.

Thereafter, access to and identification of these data sets should be by means of this OID, or by some other agency assigned identifier, rather than the SCID field described in this document.

NOTE – Because CCSDS SCIDs are reused, and the same SCID may be used in different frequency bands, identification of archived data by SCID is problematic. The OID is permanent and unambiguous; it may be represented in several different, but inter-changeable, forms, as needed. See ISO/IEC 8825-1:2008, X.690, Sec 8.19 thru 8.22 for viable mappings from a character string-based OID to other digital forms.

## SCID Assignment Request Procedures

All Q-SCID Assignment Requests by an Agency shall be submitted by the designated AR (see reference [5]).

Organizations that are not affiliated with a CCSDS Agency shall contact the SANA for Q-SCID assignments.

All Q-SCID Assignment Requests shall be submitted using the approved request form located on the SANA website at <http://sanaregistry.org/r/spacecraftid/spacecraftid.html>.

The AR shall specify the protocol that is to be used (VN) and the uplink and downlink frequency band(s) (FB) that have been assigned.

NOTE - The form requests only the uplink and downlink frequency bands, it does not require the exact operating frequencies. As long as the same VN and FB is used for uplink and downlink only one SCID need be assigned. The correct FB, by actual numeric frequency range, must be selected.

A separate form shall be used for each Q-SCID request.

NOTE - The form supports the request for Q-SCIDs for different protocols (VN) and frequency bands (FB) for any given spacecraft and may support requests for more than one spacecraft, such as a constellation.

All Q-SCID Assignment Requests shall be submitted to the SANA using the on-line web form.

In exceptional circumstances the AR may fill out a copy of the on-line form and email it to info@sanaregistry.org.

## SCID Code Assignment Procedures

All CCSDS Q-SCID Assignments shall be made by SANA.

April 2015

SANA shall assign the specific Q-SCID codes based on availability.  Only in exceptional circumstances will user requests for specific numerical code assignments be honored.

Each Q-SCID Code Assignment shall be globally unique within the assigned VN and frequency band during its assignment period.

Q-SCID Code Assignments shall be made on a spacecraft-by-spacecraft basis.

Each request for a Q-SCID Code Assignment shall also return a unique, persistent, OID identifier for each spacecraft.

NOTE -- Each spacecraft gets a unique OID. Each aperture on the spacecraft, and the frequency band(s) for the aperture, may also be assigned a unique sub-OID within the spacecraft OID tree.

User requests for reservation of a sequence of ID numbers for unspecified spacecraft shall not be accepted; however, multiple Q-SCIDs may be assigned for those missions that have multiple spacecraft.

NOTE -- Agencies that desire separate designations for protoflight spacecraft or simulators may request a unique OID for each such instance, but not SCIDs.

NOTE -- Any assignment of an OID to a protoflight spacecraft, simulator, or other “flight-less bird” shall be treated as assignment of a Q-SCID with a VN of “non-radiating”. These Q-SCIDs are separate from, but may overlap, those assigned to real VNs. Alternatively, any agency may self-assign SCIDs for simulators as long as these are never used for RF radiation.

User requests for assignment of specific numerical codes may be accepted in exceptional circumstances and may be satisfied only if those numerical codes are available.

The user should refer to the catalog of existing Q-SCID assignments (reference [6]) to avoid requesting specific assignments that could result in duplication, and, therefore, denial of a request.

If a request for a specific numerical code cannot be honored the SANA shall assign another SCID based on availability.

If a spacecraft requires more than one Q-SCID, due to use of different uplink and downlink protocols (VN) or different assigned frequency bands (FB), the SANA shall attempt to assign the same numeric SCID in each bin based on availability.

All OID assignments shall be made in the OID sub-tree for Spacecraft [9].

## SCID Relinquishing Procedures

The AR shall determine, in conjunction with the mission manager, exactly when the operational phase of a mission is complete and when the related Q-SCIDs can be relinquished.

The AR shall use the approved Q-SCID form located on the SANA website at http://sanaregistry.org/r/spacecraftid/spacecraftid.html and mark ‘RELINQUISH current GSCID’ in the **AUTHORIZATION** section.

Only an authorized AR for the Agency shall be permitted to relinquish an assigned Q-SCID.

SANA shall place the relinquished SCID code number at the bottom of the stack of SCIDs available for assignment.

NOTE – The relinquished SCID code number is placed at the bottom of the stack of unassigned SCIDs in order to maximize the period of time before the relinquished number might be reassigned

SCID REQUEST FORM

(NON-Normative)

This annex provides an example, as of the date of publication, of the official, on-line, form that is to be used by Agency Representatives for requesting and relinquishing SCIDs. This is provided only as an example of the sort of information needed to make a SCID request. The on-line form, found at <http://sanaregistry.org/r/spacecraftid/spacecraftid.html>, may differ from this example and the website should be used for all official requests by the Agency Representative.



1. ACRONYMS AND ABBREVIATIONS

(Informative)

Term Meaning

AR Agency Representative

FB Frequency Band

GSCID Global Spacecraft Identifier

Hex Hexadecimal

HoD Head of Delegation

IEEE Institute of Electrical and Electronics Engineers

ITC International Telecommunications Union (UN organization)

OID Object Identifier (ISO)

Q-SCID Qualified Spacecraft Identifier

S/C Spacecraft

SANA Space Assigned Numbers Authority

SCID Spacecraft Identifier

TC Telecommand

TLM Telemetry

VN Version Number

WRC World Radiocommunications Conference

**(NORMATIVE)**

**SANA Considerations**

**Name**: CCSDS Spacecraft Identifier

**Structure**: Tabular (one table for each Q-SCID Version), 12 columns by the number of rows needed for the SCID count (8 or 10 bits). The data types in this table are provided only as an example of the field type and size. The actual fields will be determined when the tables are implemented.

|  |  |  |  |
| --- | --- | --- | --- |
| **Column Name** | **Data Type** | **Data Range** | **Notes** |
| **Spacecraft Name** | Character (64) | Any valid alpha-numeric | Assigned by the agency |
| **Channel** | Character (3) | TC, TLM, AOS, Other | TLM used for AOS |
| **Version Number (s)** | Integer (short), may be more than one | 1, 2, or 3 | May be extended by new protocols |
| **SCID** | Hex (3) | 001-max  | Max is maximum SCID value for each Version Number |
| **GSCID** | Hex (3) | 001-max | Per frequency band |
| **Object ID** | ISO OID | 1.3.112.4.7… | Unique OID is assigned to each spacecraft |
| **Requestor Name** | Character (64) | Valid person name in English | Name must be in AR registry |
| **Requestor Affiliation** | Character (64) | Valid organization name | Name must be in Organization registry |
| **Requestor Affiliation Country** | Character (2) | Valid 2 character country code | Name must be valid ISO country code |
| **Last Request Date** | Date | yyyy-mm-dd |  |
| **Registered by** | ISO OID | 1.3.112.4.2.1 … | Unique OID for the person who last changed the registry |
| **Status** | Enumerated | “Assigned”, “Returned”, OID only, NULL |  |
| **Spacecraft Name Abbreviation** | Character (8) | Any valid alpha-numeric | Agency assigned abbreviation or acronym |
| **Spacecraft Name Alias(es)** | Character (128) | Comma separated list of any valid alpha-numeric | Agency assigned alias list (pre/post launch, familiar) |
| **S/C Transmitting Frequency Band (s)** | Character (6), one per assigned band | Frequency Band designator abbreviation | Frequency band designators from Table 2-1, may be more than one. |
| **S/C Recieivng Frequency Band (s)** | Character (6), one per assigned band | Frequency Band designator abbreviation | Frequency band designators from Table 2-1, may be more than one. |
| **Expected Launch Date** | Date | yyyy-mm-dd | Assignment will typically be pre-launch |
| **Expected Mission End Date** | Date | yyyy-mm-dd | May be extended upon request to SANA |
| **Note** | Char (64) |  |  |

**Registration Authority: CCSDS Secretariat**

**Registration Rule:**

1. Request must come from an assigned Agency Representative. If there is no Agency Representative for the Agency, or if the Agency (or other organization) is not registered, then those registry entries must first be created.
2. Requestor may ask for specific SCID assignment, but this is not guaranteed.
3. Requestor may ask for ***only*** an OID assignment, not just SCID. This is of benefit to organizations that do not use CCSDS link layer protocols but still wish to have a unique, registered, designator. OIDs shall be assigned sequentially in the spacecraft sub-section of the OID tree.
4. Each request must separately specify the specific uplink and downlink frequency bands within which it is to operate (see Table 2-1). These are assigned by the agency spectrum manager.

**Name**: CCSDS Agency registry

**Structure**: This **practice** references the CCSDS Organization registry defined in CCSDS 313.1-Y-1 [11].

1. Every request for a SCID must come from an organization that has a “member agency”, “observer agency”, or “affiliate” Organization Type.
2. Any organization wishing to request a SCID that is not yet registered must first register with the SANA.
3. An organization may have any of the defined Role types.

**Name**: CCSDS Contact registry

**Structure**: This **practice** references the CCSDS Contact registry defined in CCSDS 313.1-Y-1 [11].

1. Every request for a SCID must come from a person identified by their Agency as being the official Agency Representative.
2. Only persons with the Contact registry Role of “Agency Representative for SCID Requests” set may request a SCID.
3. Any person wishing to request a SCID, and who is not yet registered, must first register with the SANA.
4. The Agency Head of Delegation or Organization PoC must appoint the “Agency Representative for SCID Requests”
5. Only persons with the Contact registry Role of “Agency HoD” or “Organization PoC” set may appoint an “Agency Representative for SCID Requests”.