Technical corrigendum for 211.2-B-3

**FROM**

**A white paper with black text

Description automatically generated**

**TO**

**3.3.2.3** When LDPC coding is used, octet synchronization shall be maintained between the PLTUs and LDPC codewords as follows.

1. The first LDPC message block shall start with the first bit of the Acquisition Sequence, and this shall be the first bit of the PN sequence defined in 3.3.2.2.
2. The Acquisition Sequence shall be an integer number of octets in length.
3. Idle data inserted between PLTUs shall start with the first bit of the PN sequence defined in 3.3.2.2, and shall be an integer number of octets in length.

NOTE – These synchronization requirements apply only when LDPC coding is used.