

Draft Recommendation for  
Space Data System Standards

|  |
| --- |
| Mission Operations  Mission Planning & Scheduling Services |

Draft Recommended Standard

CCSDS 529.1-W-0

WHITE Book

October 2020

AUTHORITY

|  |  |  |  |
| --- | --- | --- | --- |
|  | | | |
|  | Issue: | White Book, Issue 0 |  |
|  | Date: | October 2020 |  |
|  | Location: | Not Applicable |  |
|  | | | |

**(WHEN THIS RECOMMENDED STANDARD IS FINALIZED, IT WILL CONTAIN THE FOLLOWING STATEMENT OF AUTHORITY:)**

This document has been approved for publication by the Management Council of the Consultative Committee for Space Data Systems (CCSDS) and represents the consensus technical agreement of the participating CCSDS Member Agencies. The procedure for review and authorization of CCSDS documents is detailed in *Organization and Processes for the Consultative Committee for Space Data Systems* (CCSDS A02.1-Y-4), and the record of Agency participation in the authorization of this document can be obtained from the CCSDS Secretariat at the address below.

This document is published and maintained by:

CCSDS Secretariat

Space Communications and Navigation Office, 7L70

Space Operations Mission Directorate

NASA Headquarters

Washington, DC 20546-0001, USA

FOREWORD

[Foreword text specific to this document goes here. The text below is boilerplate.]

Attention is drawn to the possibility that some of the elements of this document may be the subject of patent rights. CCSDS shall not be held responsible for identifying any or all such patent rights.

Through the process of normal evolution, it is expected that expansion, deletion, or modification of this document may occur. This Recommended Standard is therefore subject to CCSDS document management and change control procedures, which are defined in *Organization and Processes for the Consultative Committee for Space Data Systems* (CCSDS A02.1-Y-4). Current versions of CCSDS documents are maintained at the CCSDS Web site:

http://www.ccsds.org/

Questions relating to the contents or status of this document should be addressed to the CCSDS Secretariat at the address indicated on page i.

At time of publication, the active Member and Observer Agencies of the CCSDS were:

Member Agencies

* Agenzia Spaziale Italiana (ASI)/Italy.
* Canadian Space Agency (CSA)/Canada.
* Centre National d’Etudes Spatiales (CNES)/France.
* China National Space Administration (CNSA)/People’s Republic of China.
* Deutsches Zentrum für Luft- und Raumfahrt (DLR)/Germany.
* European Space Agency (ESA)/Europe.
* Federal Space Agency (FSA)/Russian Federation.
* Instituto Nacional de Pesquisas Espaciais (INPE)/Brazil.
* Japan Aerospace Exploration Agency (JAXA)/Japan.
* National Aeronautics and Space Administration (NASA)/USA.
* UK Space Agency/United Kingdom.

Observer Agencies

* Austrian Space Agency (ASA)/Austria.
* Belgian Federal Science Policy Office (BFSPO)/Belgium.
* Central Research Institute of Machine Building (TsNIIMash)/Russian Federation.
* China Satellite Launch and Tracking Control General, Beijing Institute of Tracking and Telecommunications Technology (CLTC/BITTT)/China.
* Chinese Academy of Sciences (CAS)/China.
* Chinese Academy of Space Technology (CAST)/China.
* Commonwealth Scientific and Industrial Research Organization (CSIRO)/Australia.
* Danish National Space Center (DNSC)/Denmark.
* Departamento de Ciência e Tecnologia Aeroespacial (DCTA)/Brazil.
* European Organization for the Exploitation of Meteorological Satellites (EUMETSAT)/Europe.
* European Telecommunications Satellite Organization (EUTELSAT)/Europe.
* Geo-Informatics and Space Technology Development Agency (GISTDA)/Thailand.
* Hellenic National Space Committee (HNSC)/Greece.
* Indian Space Research Organization (ISRO)/India.
* Institute of Space Research (IKI)/Russian Federation.
* KFKI Research Institute for Particle & Nuclear Physics (KFKI)/Hungary.
* Korea Aerospace Research Institute (KARI)/Korea.
* Ministry of Communications (MOC)/Israel.
* National Institute of Information and Communications Technology (NICT)/Japan.
* National Oceanic and Atmospheric Administration (NOAA)/USA.
* National Space Agency of the Republic of Kazakhstan (NSARK)/Kazakhstan.
* National Space Organization (NSPO)/Chinese Taipei.
* Naval Center for Space Technology (NCST)/USA.
* Scientific and Technological Research Council of Turkey (TUBITAK)/Turkey.
* South African National Space Agency (SANSA)/Republic of South Africa.
* Space and Upper Atmosphere Research Commission (SUPARCO)/Pakistan.
* Swedish Space Corporation (SSC)/Sweden.
* Swiss Space Office (SSO)/Switzerland.
* United States Geological Survey (USGS)/USA.

PREFACE

This document is a draft CCSDS Recommended Standard. Its ‘White Book’ status indicates that its contents are not stable, and several iterations resulting in substantial technical changes are likely to occur before it is considered to be sufficiently mature to be released for review by the CCSDS Agencies.

Implementers are cautioned **not** to fabricate any final equipment in accordance with this document’s technical content.

Recipients of this draft are invited to submit, with their comments, notification of any relevant patent rights of which they are aware and to provide supporting documentation.

DOCUMENT CONTROL

|  |  |  |  |
| --- | --- | --- | --- |
| **Document** | **Title and Issue** | **Date** | **Status** |
| CCSDS 529.1-W-0 | Mission Operations Mission Planning & Scheduling Services, Proposed Draft Recommended Standard, Issue 0 | April 2021 | Current draft |
|  |  |  |  |
|  |  |  |  |

CONTENTS

Section Page

[1. Introduction 1-1](#_Toc68819140)

[1.1 General 1-1](#_Toc68819141)

[1.2 Purpose and Scope 1-1](#_Toc68819142)

[1.3 Applicability 1-2](#_Toc68819143)

[1.4 Rationale 1-2](#_Toc68819144)

[1.5 Document Structure 1-3](#_Toc68819145)

[1.6 Definitions 1-4](#_Toc68819146)

[1.7 Nomenclature 1-8](#_Toc68819147)

[1.7.1 Normative Text 1-8](#_Toc68819148)

[1.7.2 Informative Text 1-8](#_Toc68819149)

[1.8 Conventions 1-9](#_Toc68819150)

[1.8.1 Diagrams 1-9](#_Toc68819151)

[1.8.2 Tables 1-12](#_Toc68819152)

[1.9 References 1-15](#_Toc68819153)

[2. Overview 2-1](#_Toc68819154)

[2.1 General 2-1](#_Toc68819155)

[2.2 Mission Planning & Scheduling Concept 2-1](#_Toc68819156)

[2.3 Relationship To Mission Operations Services 2-5](#_Toc68819157)

[2.4 MPS Information Model Overview 2-7](#_Toc68819158)

[2.4.1 General 2-7](#_Toc68819159)

[2.4.2 Planning Request 2-9](#_Toc68819160)

[2.4.3 Plan 2-9](#_Toc68819161)

[2.4.4 Planning Activity 2-9](#_Toc68819162)

[2.4.5 Planning Event 2-10](#_Toc68819163)

[2.4.6 Planning Resource 2-11](#_Toc68819164)

[2.5 MPS Services Overview 2-12](#_Toc68819165)

[2.5.1 General 2-12](#_Toc68819166)

[2.5.2 Planning Request Service 2-12](#_Toc68819167)

[2.5.3 Plan Distribution Service 2-14](#_Toc68819168)

[2.5.4 Plan Execution Control Service 2-15](#_Toc68819169)

[2.5.5 Plan Information Management Service 2-17](#_Toc68819170)

[2.5.6 Plan Edit Service 2-18](#_Toc68819171)

[2.6 Optional Elements of the Standard 2-20](#_Toc68819172)

[3. MPS Information Model 3-1](#_Toc68819173)

[3.1 General 3-1](#_Toc68819174)

[3.1.1 Short Form Parts 3-2](#_Toc68819175)

[3.2 MPS Data Items 3-4](#_Toc68819176)

[3.2.1 General 3-4](#_Toc68819177)

[3.2.2 Planning Activities 3-7](#_Toc68819178)

[3.2.3 Planning Events 3-17](#_Toc68819179)

[3.2.4 Planning Resources [Optional] 3-23](#_Toc68819180)

[3.2.5 Planning Requests 3-31](#_Toc68819181)

[3.2.6 Plans 3-42](#_Toc68819182)

[3.2.7 Planning Configuration Data 3-59](#_Toc68819183)

[3.2.8 Functions [Optional] 3-60](#_Toc68819184)

[3.3 MPS Data Types 3-62](#_Toc68819185)

[3.3.1 MPS Base Data Types 3-62](#_Toc68819186)

[3.3.2 MPS Position and Direction Data Types [Optional] 3-66](#_Toc68819187)

[3.3.3 Expressions 3-72](#_Toc68819188)

[3.3.4 Additional MPS Data Types 3-76](#_Toc68819189)

[3.3.5 Arguments 3-79](#_Toc68819190)

[3.3.6 Constraints 3-82](#_Toc68819191)

[3.3.7 Triggers 3-102](#_Toc68819192)

[3.3.8 Repetitions 3-106](#_Toc68819193)

[3.4 MO Framework 3-112](#_Toc68819194)

[3.4.1 Message Abstraction Layer (MAL) 3-112](#_Toc68819195)

[3.4.2 MO Objects 3-113](#_Toc68819196)

[3.4.3 MO Object Patterns 3-115](#_Toc68819197)

[4. MPS Service Specifications 4-1](#_Toc68819198)

[4.1 General 4-1](#_Toc68819199)

[4.2 Service: Planning Request 4-2](#_Toc68819200)

[4.2.1 Summary 4-2](#_Toc68819201)

[4.2.2 MO Objects 4-5](#_Toc68819202)

[4.2.3 High-Level Requirements 4-6](#_Toc68819203)

[4.2.4 Functional Requirements 4-6](#_Toc68819204)

[4.2.5 Operation: submitRequest 4-7](#_Toc68819205)

[4.2.6 Operation: getRequestSummaries 4-8](#_Toc68819206)

[4.2.7 Operation: getRequestStatus 4-9](#_Toc68819207)

[4.2.8 Operation: cancelRequest 4-10](#_Toc68819208)

[4.2.9 Operation: updateRequest 4-10](#_Toc68819209)

[4.2.10 Operation: monitorRequestStatus 4-11](#_Toc68819210)

[4.2.11 Operation: getRequest 4-12](#_Toc68819211)

[4.3 Service: Plan Distribution Service 4-13](#_Toc68819212)

[4.3.1 Summary 4-13](#_Toc68819213)

[4.3.2 MO Objects 4-16](#_Toc68819214)

[4.3.3 High-Level Requirements 4-17](#_Toc68819215)

[4.3.4 Functional Requirements 4-17](#_Toc68819216)

[4.3.5 Operation: getPlanSummaries 4-18](#_Toc68819217)

[4.3.6 Operation: getPlan 4-18](#_Toc68819218)

[4.3.7 Operation: getPlanStatus 4-19](#_Toc68819219)

[4.3.8 Operation: monitorPlanStatus 4-19](#_Toc68819220)

[4.3.9 Operation: monitorPlan 4-20](#_Toc68819221)

[4.3.10 Operation: queryPlan 4-21](#_Toc68819222)

[4.3.11 Operation: getPartialPlan 4-22](#_Toc68819223)

[4.4 Service: Plan Execution Control Service 4-23](#_Toc68819224)

[4.4.1 Summary 4-23](#_Toc68819225)

[4.4.2 MO Objects 4-30](#_Toc68819226)

[4.4.3 High-Level Requirements 4-30](#_Toc68819227)

[4.4.4 Functional Requirements 4-30](#_Toc68819228)

[4.4.5 Operation: submitPlan 4-32](#_Toc68819229)

[4.4.6 Operation: revokePlan 4-33](#_Toc68819230)

[4.4.7 Operation: getPlanStatus 4-33](#_Toc68819231)

[4.4.8 Operation: activatePlan 4-34](#_Toc68819232)

[4.4.9 Operation: deactivatePlan 4-35](#_Toc68819233)

[4.4.10 Operation: monitorPlanExecution 4-36](#_Toc68819234)

[4.4.11 Operation: monitorPlanExecutionDetail 4-37](#_Toc68819235)

[4.4.12 Operation: activateSubPlan 4-38](#_Toc68819236)

[4.4.13 Operation: deactivateSubPlan 4-38](#_Toc68819237)

[4.4.14 Operation: getSubPlanStatus 4-39](#_Toc68819238)

[4.4.15 Operation: monitorSubPlanExecution 4-40](#_Toc68819239)

[4.4.16 Operation: suspendActivity 4-40](#_Toc68819240)

[4.4.17 Operation: ResumeActivity 4-42](#_Toc68819241)

[4.4.18 Operation: getActivityStatus 4-43](#_Toc68819242)

[4.5 Service: Plan Information Management Service 4-44](#_Toc68819243)

[4.5.1 Summary 4-44](#_Toc68819244)

[4.5.2 MO Objects 4-45](#_Toc68819245)

[4.5.3 High-Level Requirements 4-46](#_Toc68819246)

[4.5.4 Functional Requirements 4-46](#_Toc68819247)

[4.5.5 Operation: listRequestDefs 4-46](#_Toc68819248)

[4.5.6 Operation: getRequestDefs 4-47](#_Toc68819249)

[4.5.7 Operation: listEventDefs 4-48](#_Toc68819250)

[4.5.8 Operation: getEventDefs 4-48](#_Toc68819251)

[4.5.9 Operation: listActivityDefs 4-49](#_Toc68819252)

[4.5.10 Operation: getActivityDefs 4-50](#_Toc68819253)

[4.5.11 Operation: listResourceDefs 4-50](#_Toc68819254)

[4.5.12 Operation: getResourceDefs 4-51](#_Toc68819255)

[4.5.13 Operation: getSystemConfig 4-51](#_Toc68819256)

[4.6 Service: Plan Edit Service 4-53](#_Toc68819257)

[4.6.1 Summary 4-53](#_Toc68819258)

[4.6.2 MO Objects 4-54](#_Toc68819259)

[4.6.3 High-Level Requirements 4-55](#_Toc68819260)

[4.6.4 Functional Requirements 4-55](#_Toc68819261)

[4.6.5 Operation: updatePlanStatus 4-56](#_Toc68819262)

[4.6.6 Operation: insertActivity 4-57](#_Toc68819263)

[4.6.7 Operation: insertEvent 4-58](#_Toc68819264)

[4.6.8 Operation: deleteActivity 4-59](#_Toc68819265)

[4.6.9 Operation: deleteEvent 4-59](#_Toc68819266)

[4.6.10 Operation: updateActivity 4-60](#_Toc68819267)

[4.6.11 Operation: updateEvent 4-60](#_Toc68819268)

[4.6.12 Operation: updateResource 4-61](#_Toc68819269)

[4.6.13 Operation: updateResourceProfile 4-62](#_Toc68819270)

[4.6.14 Operation: applyTimeShift 4-62](#_Toc68819271)

[5. Error Codes 5-1](#_Toc68819272)

[6. Service Specification XML 6-1](#_Toc68819273)

[7. XML File Formats 7-1](#_Toc68819274)

[7.1 Planning Request XML File Format 7-1](#_Toc68819275)

[7.2 Plan XML File Format 7-1](#_Toc68819276)

[ANNEX A Implementation Conformance Statement (ICS) Proforma (normative) 1](#_Toc62658695)

[ANNEX B Security, SANA, and Patent Considerations (Informative) 1](#_Toc62658696)

[ANNEX C DEFINITION OF ACRONYMS (Informative) 1](#_Toc62658697)

[ANNEX D Informative References (Informative) 1](#_Toc62658698)

**Figures**

[Figure 1: Example Class Diagram 1-9](#_Toc68819277)

[Figure 2: Example State Machine Diagram 1-11](#_Toc68819278)

[Figure 3: Example Sequence Diagram 1-12](#_Toc68819279)

[Figure 4: Functions involved in Mission Planning 2-1](#_Toc68819280)

[Figure 5: Entities and Functions Involved in Mission Planning 2-3](#_Toc68819281)

[Figure 6: MO MPS Services Generic Protocol Stack 2-5](#_Toc68819282)

[Figure 7: MPS Data Items 2-7](#_Toc68819283)

[Figure 8: MPS Data Items and their Constituent MO Objects 3-5](#_Toc68819284)

[Figure 9: Planning Activities 3-7](#_Toc68819285)

[Figure 10: Activity State Model 3-10](#_Toc68819286)

[Figure 11: Activity Details and Nodes 3-12](#_Toc68819287)

[Figure 12: Activity Service Structures 3-14](#_Toc68819288)

[Figure 13: Planning Events 3-17](#_Toc68819289)

[Figure 14: Event State Model 3-20](#_Toc68819290)

[Figure 15: Event Service Structures 3-21](#_Toc68819291)

[Figure 16: Planning Resources 3-23](#_Toc68819292)

[Figure 17: Resource Profiles 3-26](#_Toc68819293)

[Figure 18: Resource Service Structures 3-30](#_Toc68819294)

[Figure 19: Planning Requests 3-31](#_Toc68819295)

[Figure 20: Planning Request State Model 3-35](#_Toc68819296)

[Figure 21: Plans 3-42](#_Toc68819297)

[Figure 22: Plan Details 3-44](#_Toc68819298)

[Figure 23: Plan State Model 3-50](#_Toc68819299)

[Figure 24: Plan Service Structures 3-52](#_Toc68819300)

[Figure 25: Planning Configuration Data 3-59](#_Toc68819301)

[Figure 26: Functions 3-60](#_Toc68819302)

[Figure 27: MPS Base Data Types 3-62](#_Toc68819303)

[Figure 28: Position Data Type 3-66](#_Toc68819304)

[Figure 29: Direction Data Type 3-68](#_Toc68819305)

[Figure 30: Physical Value Data Types 3-71](#_Toc68819306)

[Figure 31: MPS Expression Types 3-72](#_Toc68819307)

[Figure 32: MPS Additional Data Types 3-76](#_Toc68819308)

[Figure 33: Arguments 3-79](#_Toc68819309)

[Figure 34: Planning Constraints 3-82](#_Toc68819310)

[Figure 35: Conditional Constraints 3-84](#_Toc68819311)

[Figure 36: Geometric Constraints 3-93](#_Toc68819312)

[Figure 37: Effects 3-99](#_Toc68819313)

[Figure 38: Triggers 3-102](#_Toc68819314)

[Figure 39: Repetitions 3-106](#_Toc68819315)

[Figure 40: MO Objects 3-113](#_Toc68819316)

[Figure 41: MO Object Patterns 3-116](#_Toc68819317)

[Figure 42: Planning Request Submission Operations 4-3](#_Toc68819318)

[Figure 43: Planning Request Feedback Operations 4-4](#_Toc68819319)

[Figure 44: Plan Distribution Mandatory Operations 4-14](#_Toc68819320)

[Figure 45: Plan Distribution Monitoring Operations 4-15](#_Toc68819321)

[Figure 46: Plan Distribution Special Operations 4-16](#_Toc68819322)

[Figure 47: Plan Execution Control Operations 4-25](#_Toc68819323)

[Figure 48: Plan Execution Feedback Operations 4-26](#_Toc68819324)

[Figure 49: SubPlan Execution Control Operations 4-28](#_Toc68819325)

[Figure 50: Activity Execution Control Operations 4-29](#_Toc68819326)

[Figure 51: Plan Information Management Operations for Generic Data Item 4-45](#_Toc68819327)

[Figure 52: Plan Edit Operations for Generic Data Item (Activity or Event) 4-54](#_Toc68819328)

Tables

[Table 1: Example Data Structure Table 1-12](#_Toc68819329)

[Table 2: Example Enumeration Table 1-13](#_Toc68819330)

[Table 3: Example Service Table 1-13](#_Toc68819331)

[Table 4: Example Operation Template 1-14](#_Toc68819332)

[Table 5: Planning Request Service Capability Sets and Service Operations 2-13](#_Toc68819333)

[Table 6: Plan Distribution Service Capability Sets and Service Operations 2-14](#_Toc68819334)

[Table 7: Plan Execution Control Service Capability Sets and Service Operations 2-15](#_Toc68819335)

[Table 8: Plan Information Management Service Capability Sets and Service Operations 2-17](#_Toc68819336)

[Table 9: Plan Edit Service Capability Sets and Service Operations 2-19](#_Toc68819337)

[Table 10: Optional Elements of the Information Model 2-20](#_Toc68819338)

[Table 11: MPS Service Provider Standard Properties 2-21](#_Toc68819339)

[Table 12: Optional Service Capabilities 2-22](#_Toc68819340)

# Introduction

## General

This Recommended Standard defines the Mission Operations (MO) Mission Planning and Scheduling (MPS) services in conformance with the service framework specified in reference [D1], *Mission Operations Services Concept*.

The MPS services are a set of services that support: interaction with a Mission Planning system and its users at the level of planning requests, distribution of the plans generated, and control of the execution of those plans. It is expected, but not required, that these are used in conjunction with other mission operations services, such as Monitoring & Control [D5] and Automation, as identified in reference [D1].

The MPS services are defined in terms of the Message Abstraction Layer (MAL) (see reference [2], *Mission Operations Message Abstraction Layer*), but not the MO Common Object Model (COM) (see reference [D3]).

## Purpose and Scope

This Recommended Standard defines, in an abstract manner, the MPS services in terms of:

1. an information model that describes the structure of MPS data, including planning requests, plans and supporting information objects that are referenced by the MPS services.
2. service specifications that define the operations necessary to provide the services, together with their parameter data and required behaviour.
3. file-based message formats for the exchange of planning requests and plans, for use in mission deployments that do not require service-based interfaces

There is no expectation that an MPS system will implement all aspects of this Recommended Standard. Each service is optional and may include optional capability sets within it. Some aspects of the MPS information model are optional. A summary of the optional elements of the standard is provided in section 2.6.

This Recommended Standard does not specify:

1. individual implementations or products;
2. the implementation of entities or interfaces within real systems;
3. the methods or technologies required for communications;
4. how required MPS service configuration data is made available to deployed MPS functions;
5. the expression language used for representation of conditions and calculations embedded within MPS data.

## Applicability

This specification is applicable to any mission operations component that provides mission planning functionality or executes mission plans (schedules) and exposes mission planning and scheduling interfaces. This includes interfaces between:

* Mission users and the Mission Planning system;
* Hierarchical or distributed components of a Mission Planning system;
* Mission Planning and Plan Execution (Scheduler) components;
* Plan Execution and Mission Control.

Note that the terms plan and planning are used throughout this specification, but that this also encompasses schedule and scheduling.

This standard is intended to apply to interfaces wherever they may occur in a space system:

* between ground-based components across a terrestrial link;
* between ground-based and on-board components across a space link;
* and potentially between on-board components across an on-board interface.

## Rationale

The primary goal is to increase the level of interoperability for mission planning among agencies and space system users at the level of exchanged planning requests and plans.. The service specifications can also be used between systems within an agency and to promote the development of re-usable infrastructure for space systems and interoperability between missions.

The use of the underlying MO framework enables abstract services to be implemented using appropriate encoding and information transfer technologies (file and/or message based) for the deployment context. An extensible set of MAL technology bindings exist to support:

* encoding of the service messages;
* binding of the service operations to a specific messaging technology.

Note that security considerations are assumed to be handled at the MO framework layer or below.

## Document Structure

This Recommended Standard is organized in the following sections:

1. **Introduction**: provides purpose and scope, applicability, and rationale of this  
   Recommended Practice and lists the definitions, conventions, and references used  
   throughout the document;
2. **Overview**: describes the Mission Planning & Scheduling concept and how this relates to MO services, as well as giving a high-level overview of both the MPS Information Model and the set of MPS Services specified.
3. **MPS Information Model**: describes the MPS data items and their constituent information objects that can be referenced by MPS services. It also includes the formal specification of MPS data structures.
4. **MPS Service Specifications**: provides the formal specification of the MPS services.
5. **Error Codes**: provides the formal specification of MPS error codes.
6. **Service Specification XML**: specifies the internet location of the formal service specification eXtensible Markup Language (XML).
7. **XML File Formats**: specifies the internet location of the formal specification of XML file formats for the exchange of planning requests and plans.

## Definitions

The following table contains the definition of terms used in the document. Acronyms are to be found in ANNEX C.

| Term | Definition |
| --- | --- |
| action | A single executable task of an MO M&C service provider, a telecommand is an example of an action. |
| activity definition | The definition element of a planning activity. It forms part of the planning configuration data. |
| activity details | The information required to create an activity instance from an activity definition. It may be contained within a planning request to request inclusion of a planning activity, or an activity definition (to specify child activities). |
| activity instance | The instance element of a planning activity. Activity Instances are contained within plans. |
| argument | A run-time parameter provided to various control items on invocation. Arguments apply to planning requests, planning activities and planning events among other items. |
| constraint | see planning constraint. |
| definition | The statically declared information associated with an information object. This may, for example, include a description, set of defined arguments or any other information that applies to all occurrences of the information object. There may be multiple definitions [versions] over the mission lifetime associated with the same identity [definitionID]. |
| details | A details data structure is used to specify the information needed to create an instance from a definition for an information object that has multiple occurrences. An example is the activity details data structure. |
| direction | An MPS data type that is used to represent a pointing direction or attitude of a spacecraft, payload instrument, or other object. Directions may be represented using cartesian, spherical, or right ascension and declination coordinates, or as a named target object. |
| domain | A namespace that partitions separately addressable entities (e.g. planning activities, planning events or planning resources) in the space system. The space system is decomposed into a hierarchy of domains within which entity identifiers are unique |
| effect | A type of planning constraint, that specifies the impact that executing a planning activity will have on a planning resource. |
| event definition | The definition element of a planning event. It forms part of the planning configuration data. |
| event instance | The instance element of a planning event. Event Instances are contained within plans. |
| expression | A calculation to be performed at run time that supplies a value of a defined data type. These may be used to evaluate a planning constraint condition or to supply the value for an argument or attribute of a planning activity when it is instantiated. Expressions are specified as text strings, together with the identification of the expression language used. No standard expression language is specified in this document. |
| function | An ancillary MPS data item that allows access to built-in Boolean functions of a planning system, for example in the context of planning constraints. The function must be pre-defined to be references and the MPS Function Definition holds the declaration of an available function. |
| identity | A unique Identity that may be used to reference all occurrences of an information object (compound object) throughout the mission lifetime. This is a combination of the domain, unique definitionID within the domain, and version. Note that if the information object has multiple instances [occurrences] then these also have a unique instanceID. |
| information object | The set of information about a real-world entity that is exchanged across an interface between functions. This may include static definitions, dynamic status and metadata.  Mission planning information objects include: planning requests, plans, planning activities, planning events and planning resources. |
| instance | A dynamically created object representing each new occurrence of an information object. This includes a unique instanceID of the occurrence and any unchanging data associated with it as a set of static attributes. It also includes the current status of the object as a set of dynamic attributes.  An Instance has a reference to its Definition. |
| MO instance | An MO object pattern for an information object that has separate definition and instance objects, the latter representing an individual occurrence of the object with an evolving status. MPS examples include planning requests, planning activities and planning events.  Updates reference the instance object. Instances reference the definition object. |
| MO object | An MO Object is an entity defined within the information model of an MO compliant service specification that has a unique identity enabling it to be referenced by other MO Objects and in the body of MO service messages.  Information objects may comprise multiple MO objects, adhering to one of the following object patterns: MO Static Item, MO State and MO Instance. |
| MO state | An MO object pattern for an information object that has a single element comprising both statically declared information and dynamically evolving status. MPS examples are planning resources, and plans.  Updates reference the definition object directly. |
| MO static item | An MO object pattern for an information object that has a single element comprising statically declared information with no evolving status. An MPS example is the MPSSystemConfig object that contains configuration parameters for an MPS system.  Static Items comprise only a definition object, with no corresponding updates. |
| plan | The output of the planning process. It contains a set of selected planning activities associated to time, position or planning event. A Plan may contain additional related information.  NOTE - In the context of the Mission Planning and Scheduling standardization activity, there is no distinction between the terms Plan and Schedule and only the term Plan is used. |
| plan execution | The process of executing a Plan on-board or on the ground. |
| planning | The process of creating one or more Plans (output) from Planning Requests (input).  NOTE - In the context of the Mission Planning and Scheduling standardization activity, there is no distinction between the terms Planning and Scheduling and only the term Planning is used. |
| planning activity | A Planning Activity is a meaningful unit of what can be planned. The granularity of a Planning Activity depends on the use case, it may be hierarchical. In other words Planning Activities are the building block for Planning.  NOTE - The prefix Planning is used to disambiguate from other uses of the term Activity.  NOTE - In common usage this may also be referred to as “Task”. |
| planning configuration data | The set of configuration data required by MPS service providers and consumers. It includes activity definitions, event definitions, resource definitions, request definitions, and MPS system configuration parameters. |
| planning constraint | A Planning Constraint is something that limits or restricts the planning of planning activities. Different types of constraint exist, including: temporal constraints, sequential constraints between planning activities and/or planning events, resource constraints, and geometric constraints (position and pointing). |
| planning event | A Planning Event marks when a condition is met. Planning activities can be associated with a planning event and specify their start or end relative to the event time.  NOTE - The prefix Planning is used to disambiguate from other uses of the term Event. |
| planning request | A Planning Request constitutes an input to the planning process, which requests one or more planning activities. Each Planning Request contains all the information that the requester can provide.  NOTE - The prefix Planning is used to disambiguate from other uses of the term Request.  NOTE - Typically the planning process depends on other inputs, which is not provided through the Planning Requests, such as orbital information, or the previous plan. |
| planning resource | Any physical or virtual quantity that either impacts or is affected by the execution of the planned activities.  NOTE - The prefix Planning is used to disambiguate from other uses of the term Resource. |
| planning user | Any function that is responsible for submitting planning requests to a planning function and potentially receiving feedback on the status of planning requests and generated plans. This may be an external Principal Investigator (PI) or a mission operations function. |
| position | An MPS data type that is used to represent the physical location of a spacecraft, or other object. Positions may be represented using cartesian coordinates, a CCSDS Orbit Data Message, spherical, or right ascension and declination coordinates, or as a named object. |
| potential events | A type of planning event that is not predictable, but may still have a defined response within a plan. A virtual observatory Target of Opportunity (TOO) event is an example. |
| predicted events | A type of planning event that are expected to occur at a particular time or position that can be predicted as an input to planning and contained within a plan. Orbital events are an example of predicted events. |
| procedure | An executable process of an MO Automation service provider, on-board control procedures, or automated operations procedures are examples of a procedure. |
| repetition | A data structure used in the context of a planning request to request the repeated execution of a [set of] planning activities. Various sub-types of repetition are defined to support the specification of repeat cycles by different criteria, such as time, position or pointing. |
| request definition | The optional definition element of a planning request that contains the specification of a re-usable planning request template. It forms part of the planning configuration data. |
| request instance | The instance element of a planning request. This may change over time if the request is updated by the user, each comprising a separate version of the request. |
| resource definition | The definition element of a planning resource. This may omit dynamic attributes of the resource (its value) and forms part of the planning configuration data. |
| resource profile | Provides the evolution of the value of a planning resource over time as a set of points. |
| slider | Represents a relative position with respect to an MPS object, such as a planning activity, where 0 represents the start and 1 the end of the activity. The slider is a real number that can represent any point between these two extremes. |
| trigger | A construct that allows specification of the specific condition that marks the start or end of something. It is used in the context of both planning activities and plans to specify when an activity should start or end. Triggers may be defined in terms of time, position, pointing or a planning event. |
| update | A data structure used to report the changing status o an information objector a specific occurrence of it at a specific point in time. This may include a current value, current state, or a current set of values for defined arguments. |
| version | A data type used to specify a particular version of an information object, typically of its definition. A version of an object is uniquely identified by its ObjectID and version. |

## Nomenclature

### Normative Text

The following conventions apply for the normative specifications in this Recommended Standard:

1. the words ‘shall’ and ‘must’ imply a binding and verifiable specification;
2. the word ‘should’ implies an optional, but desirable, specification;
3. the word ‘may’ implies an optional specification;
4. the words ‘is’, ‘are’, and ‘will’ imply statements of fact.

NOTE – These conventions do not imply constraints on diction in text that is clearly informative in nature.

### Informative Text

In the normative sections of this document, informative text is set off from the normative specifications either in notes or under one of the following subsection headings:

* Overview;
* Background;
* Rationale;
* Discussion.

## Conventions

### Diagrams

Unified Modelling Language (UML) notation is used for diagrams representing the MPS Information Model in section 3, and illustrating the service specifications in section 4.

This section does not seek to provide a full description of the standard UML diagram types used, but defines the specific conventions applied in this document.

Class Diagrams



Figure : Example Class Diagram

In the MPS Information Model, UML class diagrams are used to illustrate data structures and their relationships. The above example diagram highlights specific colour coding and other conventions used in this document.

Classes are used to represent MPS data structures or types and nominally have a tan background. Where they are greyed out this indicates that the data structure is an optional element of the MPS information model. Data structure names begin with an upper case letter and are shown in bold type. Abstract data types have their names italicized.

Where a data structure corresponds to an MO Object (see 3.4.2), this is shown by the application of the <<MO Object>> stereotype and a thick purple border.

The attributes of a data structure define its content as a series of data fields. Ultimately these are composed of fields of a valid MAL::Attribute type, but they can also be any of the composite MPS data structures defined in this document, which ultimately extend the MAL::Composite type. An attribute may be optional, or correspond to a list of items. This is indicated by a multiplicity qualifier [0..1] (optional: zero or one item) or [0..\*] (list: zero to many items). The attributes of a data structure may or may not be shown in a given diagram, in the interest of conciseness (they will appear in another diagram focused on that data structure).

In the specific case of MO Objects, distinction is drawn between those attributes that are static (their value does not change over time) and those that are dynamic (their value can change over time). Static attributes of MO Objects are shown underlined. Those attributes that together constitute the unique identity of an MO Object are indicated by {id} following their type.

Data structures imported or referenced from outside the MPS information model are highlighted in other colours as indicated in the legend in the bottom left of the example diagram. These include MO MAL [2] and M&C Services [D5], and other CCSDS standards including the Navigation Event Message [D6] and Cross Support Services simple schedule [D8].

Relationships between data structures are shown by the connecting lines in the diagrams. The following UML class relationships are used:

* Association : shows a relationship between MO objects or data structures. References to an MO Object are shown in this way, where the source object will have an attribute of type MAL::ObjectRef (or MAL::Identifier) pointing to another object.
* Generalization or Inheritance : shows that a data structure is derived from a parent class (which may be *abstract*), inheriting its attributes and extending or modifying them with its own.
* Composition : shows that a data structure is contained within a parent class. Aggregation (with an unfilled diamond) is similar, but the parent only contains references to the child structures.

Enumerations are identified by the stereotype <<enumeration>> and have a green background. The set of allowed statuses/enumerations is listed as attributes, together with their corresponding integer values. By convention the name of an enumeration ends with “Enum”, and the names of the statuses/enumerations are all in upper case.

An ∞ symbol on a class indicates that more detail is to be found on this class in another diagram.

State Machine Diagrams

UML state machine diagrams are used in the MPS information model to represent allowed states and state transitions for MPS information objects. This is done for planning requests, plans, planning activities and planning events, and applies to the status attribute of the corresponding instance object.



Figure : Example State Machine Diagram

The blue dashed boundary frames indicate which function is responsible for initially asserting these states (planning or plan execution). State transitions that occur as a result of an MPS service operation are marked with an \*, other transitions occur automatically as a result of Planning or Plan Execution processes.

Sequence Diagrams

In the MPS Service Specifications, UML sequence diagrams are used to illustrate the sequence of operations and their constituent messages (following MAL interaction patterns).

Timelines show the service consumer and provider. Each service operation is shown as a set of messages, following the appropriate MAL interaction pattern, contained within a fragment box with the name of the operation. The fragment is of type “opt” and greyed out if the operation is an optional element of the service (non-mandatory capability set). Where there is a logical sequence of operations this can be indicated on the diagram.

A broker timeline may also be shown, but is only relevant for publish-subscribe pattern operations. In this case the broker function is itself optional (together with all messages between broker and provider), as a valid implementation is for the provider to act as its own broker.

Messages are labelled with the operation name, followed by the MAL interaction pattern message name in block capitals and the message body fields shown in parentheses by type.



Figure : Example Sequence Diagram

### Tables

The formal normative definitions of data structures, services and service operations are presented in an abstract tabular format in this document. This is derived from that specified in the MO MAL standard [2], but has a more compact layout. The table formats used are summarised here to aid in understanding their presentation in this document. A full description can be found in reference [2]

Purple cells (dark grey when printed on a monochrome printer) contain table headings, light  
grey cells contain fields that are fixed for a pattern, and white cells contain values that must  
are specific to the operation or structure.

Data Structures

Each data structure (or type) definition contained in the MPS information model (section 3) contains a table following the standard structure outlined below.

Table : Example Data Structure Table

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **<Data Structure name>** | **Extends** | <Parent name> | **SFP** | <#> |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| ­<name> | <data type> | Yes¦No | <Description> |
| … | … | … | … |

The first row of the table specifies the name of the MPS data structure (in bold), and that of the structure it extends, which may either be a MAL data type (typically MAL::Composite) or another MPS data type. The Short Form Part (SFP) gives the number used by the MAL to identify this structure within the area and service.

This is followed by a list of attributes or data fields that constitute the data structure. Attribute data types may either be a MAL::Attribute type, or another MPS data structure. The nullable column indicates whether the attribute is allowed to contain a null value.

By convention data structure names start with an upper case letter If the data structure is abstract (only used to define an inheritance hierarchy) then its name is italicized and the word “abstract” is substituted in the SFP. Attribute names start with a lower case letter. In the context of MPS MO Objects (definitions and instances), static and dynamic attributes are differentiated by underlining the name of the static attributes.

Enumerations

Enumerations are also contained in the MPS information model (section 3) and defined using tables of the following format.

Table : Example Enumeration Table

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **<Enumeration name>** | **SFP** | <#> |

| Status | Value | Description |
| --- | --- | --- |
| <STATE NAME> | <#> | <Description> |
| … | … | … |

The set of allowed statuses/enumerations is listed together with their corresponding integer values and a description.

By convention the name of an enumeration ends with “Enum”, and the names of the statuses/enumerations are all in upper case.

Services

A summary table is provided for each service specification in section 4. This defines the area, service and version numbers used in MAL message headers, and lists the service operations together with their MAL interaction patterns, operation numbers and the capability set to which they belong.

Table : Example Service Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Area Identifier | Service Identifier | Area Number | Service Number | Area Version |
| MPS | <Service name> | 42 | <#> | <#> |

| Interaction Pattern | Operation Identifier | Operation Number | Capability Set |
| --- | --- | --- | --- |
| REQUEST | submitRequest | <#> | <#> |
| … | … | … | … |

Service Operations

The definition of each MPS service operation in section 4 contains a table based on the appropriate interaction pattern template for the applicable MAL interaction pattern (see [2]).

Table : Example Operation Template

|  |  |
| --- | --- |
| **Operation Identifier** | <Operation name> |
| **Interaction Pattern** | <Interaction pattern name> |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| <Message direction> | <Message name> | List<Field name : (data type)> |
| … | … | … |

The message direction denotes the direction of the message relative to the provider of the  
service and is either IN or OUT. So all messages directed towards the provider are IN  
messages, and all messages directed away from the provider are OUT messages.

The body signature contains a list of message fields, often a single field referencing an MPS data structure, but in some cases there may be a series of fields each identified by a field name and data type.

Where services and types are required from other MO specifications, the following notation  
is used to denote the area and, optionally, service in which the referenced definition resides:

<area>::<service>::<type name>

## References

The following publications contain provisions which, through reference in this text, constitute provisions of this document. At the time of publication, the editions indicated were valid. All publications are subject to revision, and users of this Recommended Standard are encouraged to investigate the possibility of applying the most recent editions of the publications indicated below. The CCSDS Secretariat maintains a register of currently valid CCSDS publications.

1. *Mission Operations Reference Model,* Issue 1, CCSDS Recommended Practice (Magenta Book), CCSDS 520.1-M-1, Washington, D.C.: CCSDS, July 2010
2. *Mission Operations Message Abstraction Layer,* Issue 2, CCSDS Recommended Standard (Blue Book), CCSDS 521.0-B-2, Washington, D.C.: CCSDS, March 2013

NOTE – Informative references are listed in ANNEX D.

# Overview

## General

This chapter introduces the concepts behind the MPS services. It has the following main sections:

* Mission Planning & Scheduling Concept
* Relationship to Mission Operations Services
* MPS Information Model Overview
* MPS Services Overview
* Optional Elements of the Standard

## Mission Planning & Scheduling Concept




Figure : Functions involved in Mission Planning

Mission Planning & Scheduling encompasses application level functions of a Space Mission System that may be distributed across multiple organizations and physical nodes, both in the space and ground segments. The objective of standardization in this area is the interaction between these functions and others at application level, and not standardization of the Mission Planning functions themselves.

The scope of standardization includes both the format/model of data exchanged, as well as the semantics of the interactions for their exchange, captured by the associated service level interfaces. A generalized view of the functions involved in Mission Planning and their interactions with other functions is given in Figure 4. The entities shown in blue are in the functional area of Mission Planning. The entities shown in different colors belong to other functional areas of mission operations, such as Monitoring and Control, Navigation and the Ground Station and Communication Network.

The following Mission Planning functions are identified:

* **Planning User**: a generic function that is responsible for submitting requests to the Planning function. It may also receive feedback on the status of Planning Requests and the generated plans. It is not a Planning function itself, but is a user of Planning data and services. A real system may contain multiple types of Planning User function, some of which correspond to other mission operations functions within the space mission system.
* **Planning**: the function responsible for performing Mission Planning. Internally it may be hierarchically organized and/or distributed. Planning Requests are received from multiple Planning Users (or other Mission Planning functions) and feedback on their status provided. The output of the Planning function is plans, which may be retrieved by Planning Users and submitted to Plan Execution functions. Planning may also control the execution of Plans via the Plan Execution functions. Planning is itself a user of the Navigation function and may receive predicted Planning Events, as a Navigation Event Message (NEM) [D6], that are related to orbital information, attitude or slew times; and negotiates the scheduling of ground station support via Cross Support Services (CSS) services [D8].
* **Plan Execution**: the function responsible for executing a Plan (or part of it). There may be multiple Plan Execution functions distributed between space and ground segments. It is not a Planning function itself, but it does support a common model of the Plan in its interface with Planning. It receives or retrieves distributed plans; allows external control of the Plan Execution process; and provides feedback on execution status of the Plan. Plan Execution may use underlying Mission Control Services to effect the execution of planned activities. Mission Controllers may interact with Plan Execution functions to control the Plan Execution process and to edit Plans. External functions may also edit Plans, for example to update planning events or resources.

It should be noted that in an actual deployment, there may be multiple copies of all the functions identified in Figure 4.

The identified functions may be distributed over a number of distinct entities (organizations and systems) within a given space mission system. There is not a fixed set of such entities, but typical examples include:

* User Community / PIs;
* Science/Payload Operations Centre;
* Payload Processing Centre;
* Mission Operations Centre;
* Flight Dynamics / Navigation;
* Ground Tracking Network;
* Unmanned Spacecraft;
* Surface Lander / Rover;
* Manned Space Vehicle.




Figure : Entities and Functions Involved in Mission Planning

As an example, Figure 5 illustrates potential deployment of each of the functions identified in Figure 4 to the entities listed above. The circles indicate where the each of the functions are typically deployed in existing systems, or where they could potentially be deployed in the future. The arrows indicate the interactions in a typical current deployment, but the potential distribution of functions indicated by the circles shows that all the functional interfaces shown in Figure 4 can be exposed to the boundaries between entities. It is where the interactions between the functions are exposed across one or more boundaries between entities that there is a need for standardization within CCSDS as a potentially interoperable interface between agencies.

The interactions within the scope of Mission Planning and Scheduling standardization can be grouped into five services:

* **Planning Request**: submission of Planning Requests to a planning function, associated responses and their subsequent management and status feedback.
* **Plan Distribution**: distribution and access to Plans generated by the planning function.
* **Plan Execution Control**: submission of Plans to a plan execution function, management of the execution process and status feedback.
* **Plan Information Management**: access to planning data definitions.
* **Plan Edit**: direct manipulation of Plans outside the Planning process, either to update planning events and resources with the latest information or for emergency intervention.

Figure 4 shows these MPS services as blue lines. Interactions supported by other CCSDS standards are shown in other colours. The circle at one end indicates which function is the service provider: Planning is the service provider for Planning Request and Plan Distribution services. Plan Execution is the service provider for Plan Execution Control and Plan Edit services. Both functions can provide the Plan Information Management service. These services are introduced in section 2.5 below and formally defined in chapter 4.

A common MPS information model applies to the planning requests and plans transferred or referenced by these services and also to the common configuration data required by service providers and consumers to interpret the planning requests and plans. This information model is introduced in section 2.4 below and formally defined in chapter 3.

For those organizations that do not wish to standardize the service level interaction, but only to standardize the data format used for the exchange of planning requests and plans, standard XML-based file formats are defined in chapter 7.

## Relationship To Mission Operations Services

The CCSDS Mission Operations (MO) Services Concept provides a standard framework for the specification of end-to-end services between Mission Operations applications (reference **Error! Reference source not found.**). MO Services are defined in terms of a Message Abstraction Layer (MAL) (reference **Error! Reference source not found.**), which provides a means of specifying data and service interfaces in an implementation, encoding and communication agnostic manner.




Figure : MO MPS Services Generic Protocol Stack

The MO MAL defines:

* A set of MAL Attribute data types that can be used to represent the individual data fields of message structures.
* A set of MAL Interaction patterns that correspond to the message exchange behavior of individual service operations.

The abstract specification of the service interfaces and data can be mapped to a concrete implementation through:

1. a technology binding that defines how the abstract messages (composed of a sequence of MAL attributes) are encoded in a concrete format (e.g. binary, XML or ASCII).
2. a technology binding that defines how the resulting messages are carried over a concrete message transport protocol by mapping the standard MAL interaction patterns to that protocol;
3. a language binding that transforms the abstract service interface into a concrete API for a given programming language (e.g. Java, C++ or Python);

Figure 6 illustrates a generic deployment of MPS services using the MO service framework with service consumer and provider functions hosted on different deployment nodes. MPS specific functions and protocol layers are shown in blue; elements of the “vanilla” MO framework in yellow; and underlying communications infrastructure layers in tan. The application level MPS service interaction is shown by the direct interface between service provider and consumer functions, carrying MPS service messages defined in terms of data structures specified in the MPS information model.

The MAL technology binding used in a specific deployment ensures on-the-wire interoperability at communications protocol level. Transfer Protocol equates to the messaging or file transfer service used over the underlying transport and physical link layers. The diagram illustrates how different language bindings can be used by provider and consumer for the service API, as this does not affect the wire level protocol.

It is noted that while the MAL may be implemented as a specific software layer for reasons of maintainability and reusability, it is not a requirement to do so. The MAL may simply be used as an abstract specification that enables transformation of the service specification by the applied technology bindings into a concrete implementation of that service with no distinct MAL layer. The MO MPS, MO MAL and MAL technology binding layers in the diagram are effectively combined into a single software component. This is an important distinction for deployment contexts where the implementation is required to be both compact and efficient, such as on-board a spacecraft.

It is also noted that the MPS services are not defined in terms of the MO Common Object Model (COM) (reference [D3]). Instead a more generic concept of an MO Object is used. An MO Object is an entity defined within the information model of an MO compliant service specification that has a unique identity enabling it to be referenced by other MO Objects and in the body of MO service messages. The identity of an MO Object is defined by its Object ID, scoped by its domain, and optionally by a version. The specification of a service-specific MO Object class includes a custom set of references to other MO Objects that capture the relationships between those objects. In the context of the MPS services, MO Objects are defined to represent planning requests, plans and the planning activities, planning events and resources that they reference (see §3.4 for a more detailed explanation).

An MO application-level service specification comprises a set of operations that the service consumer may invoke on the service provider. Each operation is mapped to a standard interaction pattern defined by the MAL and provides the service-specific body of the constituent messages.

In addition to the MAL and technology bindings, the MO service framework includes a set of Common Services [D4] that can be used in conjunction with any MO application level service. These include a Directory, Login and Configuration services.

## MPS Information Model Overview

### General



Figure : MPS Data Items

A high-level overview of the MPS Information Model is given in Figure 7. This shows the principal MPS data items and their interrelationships using standard UML notation.

The rectangles in the diagram correspond to standard data items. The lines between them define the relationships between those data items. Data items are color-coded by functional area:

◼ Mission Planning data items defined in this document are shown in blue

◼ Mission Control data items (red) correspond to CCSDS MO Monitoring & Control and the proposed MO Automation standards.

◼ Navigation data item (magenta) correspond to the CCSDS Navigation Event Message standard.

◼ Cross Support Services data items (grey) correspond to CCSDS Cross Support Service Management standards.

Relationships shown in black are within the scope of Mission Planning standardization, others are color-coded by their respective area.

The following principal MPS data items are shown in the diagram:

* Planning Requests
* Plans
* Planning Activities
* Planning Events
* Planning Resources

These are introduced in the subsections below and fully defined in section 3.2. Each of these data items comprises a set of MO Objects (see §3.4.2) with its own Object ID and in some cases version, following one of the MO Object patterns defined in section 3.4.3.

The status of Planning Requests, Plans, Planning Activities and Planning Events can evolve over time and is reported through the defined MPS Services. State models are defined for each of these data items in section 3.2, but only the minimum set of states has been defined to work with the defined services: missions may effectively extend these with additional states using additional information fields.

Planning requests and plans are both container objects, whose content relates to a set of planning data items: planning events, planning activities, and planning resources. For each of these three types (or classes) of planning data, there is a defined set of items that can be referenced or instantiated within Planning Requests and Plans. Together these definitions comprise the planning configuration data.

Planning constraints are not self-standing data items, but can be attached to Planning Requests and Planning Activities. They are defined in §3.3.6. Section 3.3 also includes the definition of other MPS supporting data types, including:

* MPS Position and Direction Data Types
* Expressions
* Arguments
* Triggers
* Repetitions

Some aspects of the MPS Information Model are optional. These aspects are not required to be supported by a compliant MO MPS Service Provider, although this may limit the set of service capabilities and associated operations that can be supported. Optional aspects of the model include:

* Planning Resources
* Functions
* Planning Constraints, other than representation as a text expression using any defined expression syntax supported by the service provider.
* Position and Direction data types
* Repetitions (the representation of repetitive occurrences of planning activities)

### Planning Request

Planning Requests are the main input to the planning function. A Planning Request is a container for the information needed to be exchanged between the requester and the planner. It supports the specification of a request to plan one or more planning activities. Alternatively, it can support a request to use an existing Plan (already containing a number of planning activities) as an input to the planning process. It can constitute a one-off planning request, or request the repetitive planning of activities as a “standing order”.

The main characteristic of the Planning Request is that, being a container, it needs to hold references to, or instances of, the constituent information items that are required by the planner and agreed by the interacting parties for exchange at interface level. It has one or more planning activities as the basis of the request. In addition, the request may optionally reference planning events. Information about planning constraints on when a requested activity can or shall be planned may be exchanged as part of the Planning Request, by referencing constraints on the timing or position of Planning Activities, both absolute and relative to Planning Events or other Planning Activities, and on the state of planning resources.

### Plan

The Plan is the output of a planning process. The Plan is basically a container of one or more selected planning activities, optionally associated to planning events. In addition, the usage of planning resources may be contained in the Plan. The Plan may contain specific information from the planning process, which applies to the Plan as a whole. In the hierarchical and distributed planning concepts, the output of one planning function could be the input of another one. As such, a planning request could refer to an entire Plan.

Plans may be iterative, and therefore overlap with the previous Plan. This introduces the notion that a Plan may have an identified predecessor, and also that if a planning data item is contained in multiple iterations of the plan, then it should have the same unique identity in each successive iteration of the Plan to avoid ambiguity and duplication.

Plans comprise the following main elements:

* Plan Information: header data relating to the plan as a whole.
* Planned Items: the set of contained planning activities and planning events.
* Plan Revisions [optional]: summaries of the changes between this version of the Plan and another specified version of a Plan, usually its predecessor Plan.
* Plan Resources [optional]: value profiles covering the period of the Plan for a set of planning resources.

### Planning Activity

A Planning Activity is the basic building block for the planning: a meaningful unit of what can be planned. As such, it has to be understood by the planning function. It could eventually be translated to something that can be executed by a plan execution function – this includes CCSDS MO M&C actions (that may represent telecommands) and CCSDS MO Automation procedures (that may represent any automated telecommand sequence, operational procedure, on-board control procedure, or function).

Planning Activities support hierarchy: a Planning Activity may be composed of one or more subordinate Planning Activities. A Planning Activity may define arguments (parameters), which could be used to instantiate a specific Planning Activity in a Plan, based on its generic definitions. Arguments of a Planning Request or Planning Event can be passed through to the arguments of Planning Activities resulting from these. Arguments can then similarly cascade down through a hierarchy of Planning Activities. A plan execution function may then flow down these arguments to any action or automated procedure initiated.

Planning constraints can also be associated with a Planning Activity, either generic constraints applicable to all occurrences (or instances) of the Planning Activity that are contained within its definition, or specific constraints associated with a particular instance that are defined in the context of the planning request. These planning constraints can be expressed in terms of the timing or position of a Planning Activity, both absolute and relative to Planning Events or other Planning Activities, and on the state of planning resources.

### Planning Event

A Planning Event marks when a condition is being met. It is not envisaged to use it to express a condition itself, but rather to express the fact that it is fulfilled. Typical conditions, for which events are used to report their fulfilment, are temporal or positional. They may be used to represent predicted or planned events, such as predicted orbital events or planned periods of contact with a spacecraft, that are typically received as an input by the mission planning function, from an external function, such as Navigation.

Planning Events may be grouped hierarchically to represent a compound event, such as the start and end of a satellite pass over a ground station (AOS/LOS), or a satellite passing through eclipse (penumbra entry, umbra entry, umbra exit, penumbra exit). A Planning Event may define arguments (parameters) to convey additional information relevant to the planning process.

Planning activities may be linked to a related planning event. The start or end of the planning activity can be relative to the planning event, and the arguments of the event can be flowed down to the planning activity. Planning requests may also reference planning events, associating them with requested planning activities.

Planning Events may be classified as predicted events or potential events:

* Predicted events are those that are expected to occur at a particular time or position that is known at the time of planning and can be contained within a plan. Uncertainty in the timing of predicted events may be refined closer to their time of occurrence. This can either be handled by re-planning, or by updating the events within an executing plan.
* Potential events are not predictable, but may still have a defined response within a plan: virtual observatory Target Of Opportunity (TOO) events are an example. Such events can be inserted into an executing plan.

### Planning Resource

A Planning Resource is an abstract status modelling the state of the system being planned. It may be necessary to model some aspects of system state in order to:

* trigger the execution of a Planning Activity;
* constrain the execution of a Planning Activity.
* define the effect that the execution of a Planning Activity has on the Planning Resource

A Planning Resource is in effect a value of defined type that can evolve over time. A Resource Profile can be used to capture and communicate that evolution over time in the context of a Plan.

If an event or constraint on a Planning Activity needs to be expressed in terms of the state of the system (rather than just time or position) then this corresponds to the state of Planning Resources. This is considered not internal to the Planning function, if it forms part of the Planning Request or Plan.

A Planning Resource could in principle be considered as information that is internal to the planning system. However, some resources may be shared across multiple planning entities. As such, information regarding a resource may need to be communicated between entities, and therefore has to be referenced as part of a Planning Request or of the Plan, in terms of requested or consumed resources respectively. This may include the initialization or synchronization of Planning Resource values at specific points in the Plan.

Planning Resources are an optional element of the MPS Information Model. There is no requirement for a compliant MPS system to support them.

## MPS Services Overview

### General

This document specifies standards for the following MPS Services, which are introduced in the following subsections:

* Planning Request Service [PRS]
* Plan Distribution Service [PDS]
* Plan Execution Control Service [PECS]
* Plan Information Management Service [PIMS]
* Plan Edit Service [PES]

A compliant MPS system may support only a subset of these services.

Each service comprises a set of service operations that the service consumer can invoke on the service provider. Service operations reference the MO Objects defined in the MPS Information Model. Each service operation follows one of the standard MO MAL interaction patterns that may comprise multiple messages flowing in both directions between service consumer and provider. Where not fully defined within the MAL, the body of these messages forms part of the service specification and are defined in terms of MAL Attribute data types and/or data structures defined in the MPS Information Model.

Service operations are grouped into capability sets. A compliant MPS system may only support a subset of capability sets for each supported service.

### Planning Request Service

The Planning Request Service is offered by the planning function of an MPS system to enable its users to submit, cancel and modify planning requests, as well as to receive feedback on their status. The service may be used by another planning function in a hierarchical or distributed MPS system, or by an MPS system user.

Planning Requests are defined in §3.2.5 and may include a set of requested Planning Activities or a reference to an existing Plan (the output of a Planning function in a hierarchical or distributed MPS system).

The following capability sets and service operations are defined:

Table : Planning Request Service Capability Sets and Service Operations

| Capability Set | Mandatory | Description |
| --- | --- | --- |
| 1 | Yes | Submit Planning Request, obtain a list of Planning Request Summaries and retrieve Planning Request Status. |
| 2 | No | Cancel Planning Request |
| 3 | No | Update (modify) Planning Request |
| 4 | No | Subscribe to Planning Request Status Updates |
| 5 | No | Retrieve Planning Requests |

|  |  |  |
| --- | --- | --- |
| Operation | Description | Capability Set |
| submitRequest | Send planning request to service provider, optionally based on a planning request definition. The ID of the planning request instance created is returned. | 1 |
| getRequestSummaries | Request a list of available planning requests from the service provider, subject to a specified filter. The returned list is provided as a set of summaries comprising identity, descriptive header fields and status for each planning request instance passing the filter. |
| getRequestStatus | Obtain the current status of one or more specified planning requests. The response is a list of planning request status updates, containing the status and other dynamic attributes of each requested planning request instance. |
| cancelRequest | Send cancellation of a previously submitted planning request to service provider. | 2 |
| updateRequest | Send update of a previously submitted planning request to service provider. A new version of the planning request instance is created and its identity (ID and version) is returned . | 3 |
| monitorRequestStatus | Subscribe to receive planning request status updates for a filtered set of planning request instances. The consumer is notified of updates to the status and other dynamic attributes of subscribed planning request instances. | 4 |
| getRequest | Retrieve the full content of one or more specified planning request instances. | 5 |

### Plan Distribution Service

The Plan Distribution Service is offered by the planning function of an MPS system to enable its users to obtain the Plans output by it, as well as to receive feedback on their status. The service may be used by another planning function in a hierarchical or distributed MPS system, or by an MPS system user. Plans are defined in §3.2.6.

The service does not provide the capability to control the planning function itself or to generate plans. This capability can be supported if the planning function exposes a standard set of MO Monitoring & Control services. Submission of Plans to a plan execution function is supported by the Plan Execution Control Service (see §2.5.4)

The following capability sets and service operations are defined:

Table : Plan Distribution Service Capability Sets and Service Operations

| Capability Set | Mandatory | Description |
| --- | --- | --- |
| 1 | Yes | List available Plans and their latest status, obtain specified Plans or their latest status. |
| 2 | No | Subscribe to updates in Plan status. |
| 3 | No | Subscribe to receive new Plans |
| 4 | No | Query to retrieve filtered set of Plans |
| 5 | No | Retrieve a partial Plan, based on specified criteria |

|  |  |  |
| --- | --- | --- |
| Operation | Description | Capability Set |
| getPlanSummaries | Request a list of available plans from the service provider, subject to a specified filter. The returned list is provided as a set of summaries comprising identity, descriptive header fields and status for each plan passing the filter. | 1 |
| getPlan | Retrieve the full content of one or more specified plans. |
| getPlanStatus | Obtain the current status of one or more specified plans. The response is a list of plan updates, containing the status and other dynamic attributes of each requested plan. |
| monitorPlanStatus | Subscribe to receive plan updates for a filtered set of plans. The consumer is notified of updates to the status and other dynamic attributes of subscribed plans. | 2 |
| monitorPlan | Subscribe to receive a filtered set of plans, receiving the full content of the plan when published by the Provider. | 3 |
| queryPlan | Query to receive a filtered set of plans, based on an extended set of filter criteria, including on the planning activities and events contained within a plan. | 4 |
| getPartialPlan | Retrieve a subset of a plan, covering a more restricted period or only containing selected planning activities. | 5 |

### Plan Execution Control Service

The Plan Execution Control Service is offered by an MPS system’s plan execution function to enable its users to submit (and revoke) Plans for execution; to control their execution at Plan, Sub-Plan and Activity levels; and to receive feedback on their execution status.

The Plan Execution Control Service may be used by a planning function, or by an MPS system user responsible for mission operations.

Plans are defined in §3.2.6, including the state model for Plans to which the operations of the service correlate.

Sub-plans are not defined as an MO Object in the MPS Information Model, but are specified by an Identifier associated with the constituent ActivityInstances contained in a Plan. This can be used to sub-divide a Plan based on domain (spacecraft or subsystem), operational responsibility, or another criterion. Each ActivityInstance can only be associated with a single Sub-plan. Control may be exercised via the service at the level of sub-plans.

The following capability sets and service operations are defined:

Table : Plan Execution Control Service Capability Sets and Service Operations

| Capability Set | Mandatory | Description |
| --- | --- | --- |
| 1 | Yes | Submit Plan for execution; revoke Plan previously submitted; and retrieve execution status of Plans. |
| 2 | No | Activate and deactivate execution of Plans. |
| 3 | No | Subscribe to receive execution status of Plans (at the level of the Plan). |
| 4 | No | Subscribe to receive detailed execution status of Plans (at the level of contained planning activities, events and resources). |
| 5 | No | Activate and deactivate execution of Sub-plans, and retrieve execution status of Sub-plans. |
| 6 | No | Subscribe to receive execution status of Sub-plans. |
| 7 | No | Suspend and resume execution of ActivityInstances. |
| 8 | No | Retrieve a detailed report on the execution status of ActivityInstances. |

|  |  |  |
| --- | --- | --- |
| Operation | Description | Capability Set |
| submitPlan | Send a Plan to a plan execution function, making it available for execution.  Note: A plan may be a patch plan. | 1 |
| revokePlan | Instructs a plan execution function to revoke a previously submitted Plan, making it unavailable for execution. |
| getPlanStatus | Retrieve the current execution status of Plans. |
| activatePlan | Enables the execution of specified Plans. | 2 |
| deactivatePlan | Disables the execution of a specified Plans, subject to an implementation specific deactivationMode. |
| monitorPlanExecution | Subscribe to receive plan updates for a filtered set of plans. The consumer is notified of updates to the status and other dynamic attributes of subscribed plans. | 3 |
| monitorPlanExecutionDetail | Subscribe to receive updates that report changes in the detailed execution status for a filtered set of Plan contents at the level of planning activities, events and resources. | 4 |
| activateSubPlan | Enables the execution of planning activities associated with specified Sub-plans. | 5 |
| deactivateSubPlan | Disables the execution of planning activities associated with specified Sub-plans, subject to an implementation specific deactivationMode. |
| getSubPlanStatus | Retrieves the current status of Sub-plans. |
| monitorSubPlanExecution | Subscribe to receive updates on execution status of Sub-plans. | 6 |
| SuspendActivity | Request suspension of the execution of selected activities in one or more plans without changing the state of the plan(s), subject to an implementation specific suspensionMode. | 7 |
| ResumeActivity | Requests the resumption of previously suspended activities in one or more plans without changing the state of the plan(s). |
| getActivityStatus | Requests a detailed Report on the status of Activities at Activity, Sub-plan or Tag level | 8 |

### Plan Information Management Service

The Plan Information Management Service is offered by the planning function of an MPS system to enable its users to list and retrieve available definitions for MPS data items, including: planning requests, planning events, planning activities, planning resources and MPS system configuration data. The service may also be offered by a plan execution function.

The service does not support the transfer of planning configuration data to planning or plan execution functions, which is outside the scope of the current MPS services. Nor does it support the insertion or modification of MPS data item definitions.

The structure of the various MPS data item definitions is given in §3.2.

The following capability sets and service operations are defined, each pertaining to a specific type of MPS data item:

Table : Plan Information Management Service Capability Sets and Service Operations

| Capability Set | Mandatory | Description |
| --- | --- | --- |
| 1 | No | List and retrieve planning RequestDefinitions |
| 2 | No | List and retrieve planning EventDefinitions |
| 3 | No | List and retrieve planning ActivityDefinitions |
| 4 | No | List and retrieve planning ResourceDefinitions |
| 5 | No | Retrieve MPS system configuration data [MPSSystemConfig] |

|  |  |  |
| --- | --- | --- |
| Operation | Description | Capability Set |
| listRequestDefs | Request a filtered list of available RequestDefinitions. | 1 |
| getRequestDefs | Retrieve a set of available RequestDefinitions. |
| listEventDefs | Request a filtered list of available EventDefinitions | 2 |
| getEventDefs | Retrieve a set of available EventDefinitions. |
| listActivityDefs | Request a filtered list of available ActivityDefinitions | 3 |
| getActivityDefs | Retrieve a set of available ActivityDefinitions. |
| listResourceDefs | Request a filtered list of available Resource definitions | 4 |
| getResourceDefs | Retrieve a set of available Resource definitions |
| getSystemConfig | Retrieves system configuration data relating to the MPS System. | 5 |

### Plan Edit Service

The Plan Edit Service is offered by an MPS system’s plan execution function to enable its users to modify Plans that have already been submitted for execution. It allows an external user or function to update the status of the Plan; insert, modify or delete planning activity and event instances; update the value of resources; and apply a time shift to a Plan.

This may be used by expert mission operations users in a non-nominal operational scenario to modify a Plan that is executing or about to execute in order to avert or recover from a failure. Where there is sufficient time, it is recommended to re-plan using the nominal planning process rather than to edit the Plan directly, as this circumvents any constraint checking performed by the planning function.

Another use of the service is for a third party functions to update elements of the plan to reflect information available in near-real-time. Examples are:

* Update of the input arguments of a planned activity instance to fine tune its behavior in response to currently observed status.
* Update of a predicted planning event instance that is already contained within a Plan, with refined timing or other details.
* The injection of instances of planning events. These may be detected in real-time and correlate to potential (rather than predicted) events for which a planned response is available. An example is a “Target of Opportunity” event that may be notified to an astronomical observatory mission.
* Update of a resource value by an external modelling function to more accurately reflect currently observed status.

Plans are defined in §3.2.6, while their constituent planned items are defined in §3.2.2 (Planning Activities), §3.2.3 (Planning Events) and §3.2.4 (Planning Resources).

The following capability sets and service operations are defined:

Table : Plan Edit Service Capability Sets and Service Operations

| Capability Set | Mandatory | Description |
| --- | --- | --- |
| 1 | Yes | Update Plan status. |
| 2 | Yes | Insert or Delete ActivityInstances or EventInstances. |
| 3 | No | Update ActivityInstances or EventInstances. |
| 4 | No | Update Resource value. |
| 5 | No | Update Resource profile. |
| 6 | No | Apply a time shift to a Plan. |

|  |  |  |
| --- | --- | --- |
| Operation | Description | Capability Set |
| updatePlanStatus | Update Plan status or isAlternate flag. | 1 |
| insertActivity | Insert a new ActivityInstance into a Plan. | 2 |
| insertEvent | Inject a new EventInstance into a Plan. |
| deleteActivity | Delete a specified ActivityInstance from a Plan. |
| deleteEvent | Delete a specified EventInstance from a Plan. |
| updateActivity | Update a specified ActivityInstance in a Plan. | 3 |
| updateEvent | Update a specified EventInstance in a Plan. |
| updateResource | Make a discrete update to the value of a specified Resource at a specified time. | 4 |
| updateResourceProfile | Update the profile of a specified Resource over time. | 5 |
| applyTimeShift | Apply a time shift to a specified Plan or its sub-plans. | 6 |

## Optional Elements of the Standard

The MPS services specification defines a substantial MPS information model and five services. Compliance of an individual mission planning system deployment to the MPS service specification does not imply that the either the complete set of services specified here or the full MPS information model has to be supported.

The level of compliance of a specific deployment to the standard can be selected as follows:

1. The set of MPS Services supported
2. The capability sets supported within each MPS Service
3. The optional elements of the MPS Information Model supported

The supported capabilities of a service provider can be made available to consumers via the MO Common Directory Service [D4]. An entry in the directory is made for each MPS service supported by each MPS service provided, which lists the supported capability sets for that service.

Table : Optional Elements of the Information Model

| # | Information Model Element | MO Objects | MPS Data Types | Constraints |
| --- | --- | --- | --- | --- |
| 1 | Core Features | Planning Requests Plans Planning Activities Planning Events MPSSystemConfig | Base Data Types (excl. Position & Direction) Expressions Additional MPS Data Types Arguments Time & Event Triggers Time & Event Repetitions | Constraint Expression |
| 2 | Basic Constraints |  |  | Temporal Constraints Sequential Constraint Exclusion Constraint |
| 3 | Plan Revisions | Patch Plans | Plan Revisions |  |
| 4 | Resources | Resources | Resource Profiles Plan Resources |  |
| 5 | Resource Constraints (requires Resources) |  | Resource Constraints Argument Constraint Effects |
| 6 | Position & Direction |  | Position & Direction Types Location, Pointing and Angle Triggers Location, Pointing and Angle Repetitions |  |
| 7 | Geometric Constraints (requires Pos. & Dir.) |  | Geometric Constraints |
| 8 | Functions | Functions |  | Function Constraint |

The optional elements of the MPS Information Model are themselves grouped into optional element sets detailed in Table 10 above. Of these, only the Core Features are mandatory, subject to the further caveat that only those MPS Information Model elements exposed by supported capability sets of MPS services need to be implemented. Other optional elements are shown with a grey background.

Note that support for Resource Constraints is dependent on support for Resources, and that support for Geometric Constraints is dependent on support for Position & Direction types.

The optional element sets of the MPS Information Model are orthogonal to the capability sets of the MPS Services. For example, a Planning Request Service provider may support the submission of planning requests, but not the representation of Basic Constraints within those planning constraints. This is represented in the Directory Service by the use of service provider properties as detailed in the following table:

Table : MPS Service Provider Standard Properties

| Property ID | Property Type | Description |
| --- | --- | --- |
| ES2\_CONSTR | BOOLEAN | Flag indicating support for Basic Constraints |
| ES3\_REVISION | BOOLEAN | Flag indicating support for Plan Revisions |
| ES4\_RESOURCE | BOOLEAN | Flag indicating support for Planning Resources |
| ES5\_RESCONSTR | BOOLEAN | Flag indicating support for Resource Constraints |
| ES6\_POSDIR | BOOLEAN | Flag indicating support for Position and Direction Types |
| ES7\_GEOCONSTR | BOOLEAN | Flag indicating support for Geometric Constraints |
| ES8\_FUNCTION | BOOLEAN | Flag indicating support for Functions and Function Constraints |

The following table summarises the optional capability sets and information model elements for all MPS Services. Optional capabilities and elements are shown with a grey background. For each service capability set, applicability of information model element sets are shown as follows:

✓ Required

O Optional

- Not Applicable

An indication is also given of which service specific data structures are relevant to the operation. Note this is shown at the level of the MPS object type: only the specific data structures used in the messages of the associated service operations are required.

Table : Optional Service Capabilities

| Services | | Information Model | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Service | Capability Set | Core Features | Basic Constraints | Plan Revisions | Resources | Position & Direction | Functions | Service Data Structures |
| PRS | 1: Submit Request / Status | ✓ | O | - | O | O | O | Request |
| 2: Cancel Request | ✓ | - | - | - | - | - |  |
| 3: Update Request | ✓ | O | - | O | O | O | Request |
| 4: Subscribe to Status | ✓ | - | - | - | - | - | Request |
| 5: Retrieve Request | ✓ | O | - | O | O | O |  |
| PDS | 1: List & Obtain Plans | ✓ | O | O | O | O | O | Plan |
| 2: Subscribe to Status | ✓ | - | - | - | - | - | Plan |
| 3: Subscribe to Plans | ✓ | O | O | O | O | O |  |
| 4: Query Plans | ✓ | O | O | O | O | O | Plan |
| 5: Retrieve Partial Plan | ✓ | O | O | O | O | O | Plan |
| PECS | 1: Submit Plan / Status | ✓ | O | O | O | O | O | Plan |
| 2: Plan Activation | ✓ | - | O | - | - | - | Plan |
| 3: Subscribe to Status | ✓ | - | - | - | - | - | Plan |
| 4: Subscribe to Detail | ✓ | - | - | O | O | - | Plan, Activity, Event, Resource |
| 5: SubPlan Activation | ✓ | - | - | - | - | - | Plan, SubPlan |
| 6: Subscribe to SubPlans | ✓ | - | - | - | - | - | Plan, SubPlan |
| 7: Activity Suspension | ✓ | - | - | - | - | - | Activity |
| 8: Activity Status | ✓ | - | - | - | - | - | Activity |
| PIMS | 1: Request Definitions | ✓ | O | - | O | O | O |  |
| 2: Event Definitions | ✓ | - | - | - | - | - |  |
| 3: Activity Definitions | ✓ | O | - | O | O | O |  |
| 4: Resource Definitions | ✓ | - | - | ✓ | - | - |  |
| 5: MPSSystemConfig | ✓ | - | - | - | O | - |  |
| PES | 1: Update Plan Status | ✓ | - | - | - | - | - |  |
| 2: Insert/Delete Activity/Event | ✓ | O | - | O | O | O | Activity, Event |
| 3: Update Activity/Event | ✓ | - | - | - | O | - | Activity, Event |
| 4: Update Resource | ✓ | - | - | ✓ | - | - | Resource |
| 5: Update Resource Profile | ✓ | - | - | ✓ | - | - |  |
| 6: Apply Time Shift | ✓ | - | - | - | - | - |  |

# MPS Information Model

## General

This chapter defines the Information Model applicable to the Mission Planning and Scheduling standard, introducing and defining major data elements in line with the terminology used throughout this document. An overview of the MPS Information Model has been given in section 2.4 above.

The MPS Information Model has been defined in terms of the CCSDS Mission Operations [MO] framework, specifically the MO Message Abstraction Layer [MAL] and the associated set of MAL Attribute types. This is to enable the specification of MO compliant data formats and services that reference elements of the information model.

The MPS Information Model is not defined in terms of the MO Common Object Model [COM], as it is anticipated that this will be deprecated in the next version of the MO framework. Instead the structure of MPS Objects is fully defined within this document, together with their relationships, on the assumption that the following data types will be directly supported by the MAL:

* Object ID
* Version
* Object Reference (including both Object ID and Version)

While the information model itself is not normative, the data formats and services derived from it and specified in this document are normative. It describes both the data actively exchanged by MPS Services and that required as common configuration data by service providers and users.

The information model diagrams contained in this section are expressed in UML and are informative, while the associated tables that define MPS data structures are consistent with the MO framework and normative. The diagrams and tables follow the conventions introduced in §1.7.1.

As previously introduced in §2.4, some elements of the MPS Information Model are optional. This is the case for individual data elements where:

* They may not be required by the supported capability sets of supported services.
* They form an optional element of a required data structure.

Where this is the case, this is indicated in the description of each element in the body of this chapter.

The chapter is organized into the following main sections:

1. This Introduction
2. MPS Data Items
3. MPS Data Types
4. MO Framework and Object Patterns

The principle MPS Data Items defined in are those introduced in §2.4 that correspond to a set of MO Objects that can be directly referenced in the context of the MPS Services:

* Planning Requests
* Plans
* Planning Activities
* Planning Events
* Planning Resources [Optional]
* Planning Configuration Data
* Functions [Optional]

MPS Data Types are supporting data structures used in the context of MPS Data Items and MPS Service messages:

* MPS Base Data Types
* MPS Position and Direction Types [Optional]
* Expressions
* Additional MPS Data Types
* Arguments
* Constraints
* Triggers
* Repetitions

Section 3.4 gives an overview of how the MO Framework is applicable to the MPS standard and introduces the concept of a generic MO Object and a set of common MO Object Patterns to which MPS Data Items conform. Three such MO Object Patterns are identified:

* MO Static Item: a singleton object containing static definitions only.
* MO State: a singleton object containing both static definitions and dynamic state.
* MO Instance: a Definition object containing static definitions from which a set of dynamically instantiated objects may be derived. The associated Instance objects contain static information specific to the instance and dynamic state.

### Short Form Parts

As required by the MO MAL, each concrete MPS data type is defined with a numerical Short Form Part (SFP) that is expected to be used by efficient encodings when required to hold type information. Short Form Numbers (SFN) are scoped by Area [MPS] and Service, and are formed by combining Area number (as a UShort), Service number (as a UShort) and the Short Form Part (SFP) taken from the type definition (as an Integer). As the MPS Data Items are not specific to a particular service, a convention has been adopted for the numbers used to ensure that all data types associated with a given MPS data item are contiguous.

All MPS Data Types defined in §3.3 are allocated SFPs at MPS Area level, starting from 0 (42-0-SFP).

For MPS Data Items defined in §3.2, the following approach is adopted:

* Planning Requests are defined at MPS Planning Request Service Level (42-1-SFP)
* Plans are defined at MPS Plan Distribution Service Level (42-2-SFP)
* Planning Activities are defined at MPS Area Level, with SFP from 101 (42-0-SFP)
* Planning Events are defined at MPS Area Level with SFP from 201 (42-0-SFP)
* Planning Resources are defined at MPS Area Level with SFP from 301 (42-0-SFP)
* MPS SysConfig is defined at MPS Area Level with SFP 401 (42-0-SFP)
* Functions are defined at MPS Area Level with SFP from 501 (42-0-SFP)

## MPS Data Items

### General

MPS Data Items are the principal elements of the MPS Information Model that are represented as MO Objects, following one of the MO Object Patterns described in §3.4.3. These have been introduced in §2.4 of this chapter and shown in Figure 7. The following Data Items are defined in the MPS Information Model:

MPS Core Objects

* **Planning Activities**
* **Planning Events**
* **Planning Resources** [Optional]

MPS Container Objects

* **Planning Requests**
* **Plans**
* **Planning Configuration Data**

MPS Ancillary Items

* **Functions** [Optional]

Each of these is described in turn in the following subsections.

The MPS Core Objects are those which are referenced in the context of Planning Requests and Plans, and for which there must be a set of definitions shared between communicating Mission Planning functions for those Planning Requests and Plans to be interpreted.

The MPS Container Objects are those that contain a set of references to the Core Objects. Planning Requests and Plans are dynamically created as part of the Planning process and exchanged between communicating Mission Planning functions. The Planning Configuration Data corresponds to the set of definitions shared between those functions to enable interpretation of the Planning Requests and Plans.

Functions are an MPS Ancillary Item that enable references to externally defined functions.




Figure : MPS Data Items and their Constituent MO Objects

Figure 8 shows how each of the MPS Data Items comprises multiple MO Objects following a 1, 2 or 3 element MO Object Pattern (see §3.4.3 for details). MO Objects are shown with a bold purple border.

Each MO Object has a unique Object ID. When a Definition object is updated, it retains the same Object ID, but it also has a Version attribute to uniquely identify a specific version of the definition. Planning Request Instances and Plans also have an associated Version.

The Definition objects associated with Planning Activities, Planning Events, Planning Resources and Planning Requests all form part of the Planning Configuration Data that must be available to both communicating parties that exchange Planning Requests and Plans. Planning Configuration Data also includes a single MPS SystemConfig object that defines overall configuration parameters for the entire MPS system. Definition objects comprise only static attributes. The MPS services defined in this standard do not address the bulk transfer of MPS Configuration Data between communicating parties, but individual definitions can be accessed using the Plan Information Management Service.

The Instance objects associated with all MPS data items, are the Live Planning Data created by and exchanged between communicating parties during planning and plan execution. Instance objects may comprise both static and dynamic attributes. For Planning Resources and MPS SystemConfig, the live instance has the same Object ID as the associated Definition, the only distinction being that the live instance may include dynamically updating attributes, such as the value of a Planning Resource.

Changes in state of the dynamic attributes of live planning data Instance objects may be notified through an Update structure exchanged through MPS service messages and optionally stored in Planning History. These updates are not themselves MO objects, but reference the corresponding Instance and the timestamp of the update as well as the value of dynamic attributes.

Planning Requests may reference Planning Activities, Planning Events and Planning Resources but do not contain Instances of Planning Activities or Planning Events. Instead they specify the Activity Details for the requested Planning Activities.

Plans contain Instances of planned activities, and optionally of planning events. They may also optionally contain planning resource profiles that express their planned evolution over time.

The following subsections contain the definition of each MPS Data Item and are structured as follows:

1. MO Objects defined for the Data Item
2. State Model for the Data Item (if relevant)
3. Subordinate Data Types defined for the Data Item (if relevant)
4. Service-specific Data Types defined for the Data Item (these may be used in the context of MPS Service messages).

### Planning Activities

#### Activity Objects



Figure : Planning Activities

Planning Activities follow the MO Instance Object Pattern, comprising Definition and Instance classes of MO Object.

Activity Definitions define the set of activities that may be planned and form part of the Planning Configuration Data for a mission planning system. The definition includes the specification of any arguments associated with the activity, as well as any constraints that apply to all occurrences of the activity.

Activity Instances are created to represent a specific occurrence of the activity within a Plan and include dynamic attributes that represent the changing status of the activity instance over time, including the value of any arguments and the current status of the activity. Plans contain activity instances to represent the current status of the activity within the plan.

Planning Activities may be hierarchical, with parent activities containing multiple child activities. The Activity Definition contains Activity Details (in an Activity Node) to specify each child activity. Each ActivityDetails points to the ActivityDefinition for the specified child activity. The Activity Instance maintains a set of pointers to its child ActivityInstances.

Activity Details hold the information required to create an Activity Instance and may be contained within another object, such as a Planning Request or a parent Activity Definition. This is further defined in §3.2.2.3 below.

ActivityDefinition

An ActivityDefinition is an MO Object that contains static configuration data relating to multiple occurrences of a Planning Activity. Its identity is defined by a constant definitionID and an evolving version, which is updated each time the definition is revised. ActivityDefinitions form part of the Planning Configuration Data.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ActivityDefinition** | **Extends** | MAL::Composite | **SFP** | 101 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| definitionID | MAL::ObjectID | No | ID of the ActivityDefinition. |
| version | MAL::Version | No | Version of the ActivityDefinition. |
| description | MAL::String | No | Description of the Activity. |
| argDefs | List <ArgDef> | Yes | List of Argument Definitions. |
| constraints | ConstraintNode | Yes | Set of Constraints applicable to all instances of the Activity. |
| execDef | MAL::Identifier | Yes | Reference to the definition of an executable body for the Activity (procedure, action sequence, etc.) [external to the MPS Information Model]. |
| durationSpec | DurationExpression | Yes | Supports calculation of an estimated duration of an Activity Instance. |
| children | ActivityNode | Yes | Set of Activity Details specifying child activities, optionally with repetition. |
| displayType | MAL::String | Yes | Enables a planning system to customise presentation of the Activity in displays. |
| defaultTags | List <MAL::String> | Yes | Default set of Tags that may be used to associate the Activity with others, grouping activities by operational responsibility (controller/group/system) or other criteria. |

ActivityInstance

An ActivityInstance is an MO Object that contains the identity of a specific occurrence of a Planning Activity, together with both static and dynamic information associated with that occurrence. It supports relationships to its definition, source, a related planning event and any child activities.

Activity Instances may be contained within a Plan.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ActivityInstance** | **Extends** | MAL::Composite | **SFP** | 102 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| instanceID | MAL::ObjectID | No | ID of the ActivityInstance |
| definition | MAL::ObjectRef | No | Reference to the ActivityDefinition |
| source | MAL::ObjectRef | No | Reference to the source of the ActivityInstance, which is either its parent ActivityInstance or a RequestInstance if it is a root Activity. |
| relatedEvent | MAL::ObjectRef | Yes | Optional reference to an EventInstance that is specifically associated with this instance of the Activity. Typically the Activity is placed in response to the Event. |
| children | List <MAL::ObjectRef> | Yes | References to any child ActivityInstances. |
| comments | MAL::String | Yes | Any notes associated with this instance of the Activity. |
| constraints | ConstraintNode | Yes | Set of Constraints applicable to this instance of the Activity. |
| arguments | List <Argument> | Yes | Argument values for each Argument defined in the Activity Definition. |
| start | Trigger | Yes | Optionally specifies the trigger that initiates the Activity: may be Time, Position or Event based. |
| end | Trigger | Yes | Optionally specifies the trigger that ends the Activity |
| duration | MAL::Duration | Yes | Optional duration of the Activity (estimated until execution, actual post execution). |
| subPlan | MAL::Identifier | Yes | Optional association of the Activity with a defined sub-plan. |
| tags | List <MAL::String> | Yes | Set of Tags that may be used to associate the Activity with others, grouping activities by operational responsibility (controller/group/system) or other criteria. |
| status | ActivityStatusEnum | No | Current Status of the Activity Instance (see Activity State Model in §3.2.2.2) |
| execInst | MAL::Identifier | Yes | Reference to the instance of an executable body for the Activity (procedure, action sequence, etc.) [external to the MPS Information Model]. |
| terminationInfo | MAL::String | Yes | TerminationInfo provides the reason for entering the Terminated State and is customisable, but includes:  - Completed (nominal)  - Expired (prior to Activation or during plan Supension)  - Deleted  - Failed (see ErrCode/ErrInfo) |
| errCode | MAL::Integer | Yes | Error Code relevant in the case of a failure status for the planning activity. |
| errInfo | MAL::String | Yes | Supplementary Error Information |

#### Activity State Model



Figure : Activity State Model

The following states are defined for **ActivityStatus**:

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **ActivityStatusEnum** | **SFP** | 103 |

| Status | Value | Description |
| --- | --- | --- |
| PLANNED | 1 | The Activity Instance has been included in the Plan |
| ACTIVATED | 2 | The Plan including the Activity Instance has been Activated within the Plan Execution function. |
| EXECUTING | 3 | Execution of the Activity Instance has been initiated |
| SUSPENDED | 4 | Execution of the Activity Instance has been suspended |
| TERMINATED | 5 | Execution of the Activity Instance has been terminated (further information is provided in terminationInfo) |

The blue dashed boundary frames indicate which of Planning or Plan Execution functions is responsible for asserting these states. State transitions that occur as a result of an MPS service operation are marked with an \*, other transitions occur automatically as a result of Planning or Plan Execution processes.

When an ActivityInstance is created within the context of a Plan by the Planning function, it has the initial status of Planned.

Plans may be submitted to a Plan Execution function, but before they will execute they must be activated. Once a Plan has been activated, all contained Activities will also become Activated.

When an Activity reaches its execution time or other trigger and is initiated by the Plan Execution function, then its status is changed to Executing.

During execution, an Activity may be Suspended. If resumed, its status returns to Executing.

The status of the Activity is set to Terminated once execution has ended, or it will no longer be executed. TerminationInfo provides the reason for termination and is customisable, but includes:

* Completed (nominal)
* Expired (the trigger condition passed before the Plan was activated or while the Activity was suspended)
* Deleted
* Failed (see ErrCode/ErrInfo)

If an Activity that failed to execute is subsequently re-planned, its status may be returned to Planned. It is implementation dependent whether a re-planned Activity re-uses the same ObjectID or is assigned a new one.

#### Activity Details and Nodes



Figure : Activity Details and Nodes

ActivityDetails is a structure that holds the information required to create an Activity Instance and may be contained within another object, such as a Planning Request or a parent Activity Definition.

There are two concrete sub-classes of ActivityDetails:

* **ActivityNode**: that allows details for multiple activities to be specified, as well as for those activities to be instantiated repeatedly through an optionally contained Repetition (see §3.3.8) that specifies the number and separation of the repeat instances.
* **SimpleActivityDetails**: that provides the details required to instantiate a single Activity.

As ActivityNodes can be nested, it is possible to specify complex repetitive sequences of activities.

*ActivityDetails*

Contains the information required to create one or more Activity Instances, including the specification of argument values and constraints.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***ActivityDetails*** | **Extends** | MAL::Composite | **SFP** | Abstract |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| activityRef | Slider | No | Specifies how the Activity Instance is placed with respect to any defined Repetition (0=Start; 1=End). Default is Start. |
| activityOffset | DurationExpression | No | Specifies an offset in time for the Activity Instance from any defined Repetition. Default is no offset. |
| relatedEvent | ObjectExpression | Yes | Specifies a related Event (or Event Group) for the Activity Instance. Argument specifications and constraints may reference arguments and attributes of the RelatedEvent. |
| comments | MAL::String | Yes | Any notes associated with the Activity Details. |

ActivityNode

A concrete sub-type of ActivityDetails, an Activity Node is a container node for a set of Activity Details together with an optional Repetition specification. An Activity Node is used as the root node of any Activity Details specification within a Planning Request or parent Activity Definition.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ActivityNode** | **Extends** | *ActivityDetails* | **SFP** | 104 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| Repetition | Repetition | Yes | Optional Repetition specification. |
| Activities | List <Activity Details> | No | Set of ActivityDetails. |

SimpleActivityDetails

A concrete sub-type of ActivityDetails, a Simple Activity Details provides the information required to instantiate a single ActivityInstance.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **SimpleActivityDetails** | **Extends** | *ActivityDetails* | **SFP** | 105 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| activityDef | MAL::ObjectRef | No | Reference to the ActivityDefinition. |
| argSpecs | List <ArgSpec> | Yes | Set of Argument Specifications for each Argument Definition contained in the referenced Activity Definition. These supply a value for each argument, or an expression to enable the value to be derived. |
| constraints | ConstraintNode | Yes | Set of Constraints specific to the Activity Instance to be created. |
| subPlan | MAL::Identifier | Yes | Optional association of the Activity with a defined sub-plan. |
| tags | List <MAL::String> | Yes | Set of Tags that may be used to associate the Activity with an identified sub-plan, grouping activities by operational responsibility (controller/group/system) or other criteria. |

#### Activity Service Structures



Figure : Activity Service Structures

This section defines data structures specific to Planning Activities that are used in the context of MPS service operations and their associated messages.

ActivityUpdate

ActivityUpdate is a data structure that is used to report the dynamic status of an ActivityInstance in the context of the MPS Plan Execution Control service monitorPlanExecutionDetail and getActivityStatus operations.

Activity Updates may be distributed to subscribing applications, including status displays, to inform them of the latest status of the activity. This may be particularly relevant in conjunction with a Plan Execution function. Activity Updates may be stored in Activity History to provide a complete record of evolving status over time.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ActivityUpdate** | **Extends** | MAL::Composite | **SFP** | 106 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| activityInstance | MAL::ObjectRef | No | Reference to the Activity Instance to which the status update relates. |
| timestamp | MAL::Time | Yes | Time of status update.  Only nullable in the context of an updateActivity operation: the timestamp must be provided when reporting ActivityInstance status. |
| plan | MAL::ObjectRef | Yes | Optional reference to the Plan containing the Activity Instance to which this update pertains. |
| arguments | List <Argument> | Yes | Argument values. |
| start | Trigger | Yes | Optionally specifies the trigger that initiates the Activity: may be Time, Position or Event based. |
| end | Trigger | Yes | Optionally specifies the trigger that ends the Activity |
| duration | MAL::Duration | Yes | Optional duration of the Activity (estimated until execution, actual post execution). |
| subPlan | MAL::Identifier | Yes | Optional association of the Activity with a defined sub-plan. |
| tags | List <MAL::String> | Yes | Set of Tags that may be used to associate the Activity with an identified sub-plan, grouping activities by operational responsibility (controller/group/system) or other criteria. |
| status | ActivityStatusEnum | No | Current Status of the Activity Instance |
| execInst | MAL::Identifier | Yes | Reference to the instance of an executable body for the Activity (procedure, action sequence, etc.) [external to the MPS Information Model]. |
| terminationInfo | MAL::String | Yes | TerminationInfo provides the reason for entering the Terminated State and is customisable, but includes:  - Completed (nominal)  - Expired (prior to Activation or during plan Supension)  - Deleted  - Failed (see ErrCode/ErrInfo) |
| errCode | MAL::Integer | Yes | Error Code relevant in the case of a failure status for the planning activity. |
| errInfo | MAL::String | Yes | Supplementary Error Information |

InsertedActivityDetails

A concrete sub-type of SimpleActivityDetails (see §3.2.2.3) that extends the latter to provide additional details for a single ActivityInstance to be inserted into a Plan using the MPS Plan Edit service.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **InsertedActivityDetails** | **Extends** | SimpleActivityDetails | **SFP** | 107 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| plan | MAL::ObjectRef | No | Reference to the Plan into which the Activity is to be inserted. |
| start | Trigger | Yes | Optionally specifies the trigger that initiates the Activity: may be Time, Position or Event based. |
| end | Trigger | Yes | Optionally specifies the trigger that ends the Activity |

ActivitySuspensionStatus

A data structure that returns the status and supplementary suspension information for an ActivityInstance affected by an MPS Plan Execution Control service SuspendActivity or ResumeActivity operation.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ActivitySuspensionStatus** | **Extends** | MAL::Composite | **SFP** | 108 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| activityInstance | MAL::ObjectRef | No | Reference to an Activity Instance. |
| plan | MAL::ObjectRef | Yes | Optional reference to the Plan containing the Activity Instance. |
| status | ActivityStatusEnum | No | Current Status of the Activity Instance |
| suspensionInfo | MAL::String | Yes | Supplementary information on the suspension/resumption status of the Activity Instance.  This may detail the point of suspension, which may be specific to the suspension mode; or a reason why resumption was not possible. |

### Planning Events

#### Event Objects



Figure : Planning Events

Planning Events follow the MO Instance Object Pattern, comprising Definition and Instance classes of MO Object.

Event Definitions define the set of planning events that may be referenced in planning requests and plans and form part of the Planning Configuration Data for a mission planning system. The definition includes the specification of any arguments associated with the event.

Event Instances are created to represent a specific occurrence of the event within a Plan and include dynamic attributes that represent the changing status of the event instance over time, including the value of any arguments and the current status of the event. Plans include event instances to represent the current status of the event within the plan.

Planning Events may correspond to either a single event, or an event group. Event groups provide a means to reference a set of related events together. An example might be Acquisition and Loss of Signal (AOS and LOS) for the same contact period between a spacecraft and ground station. There is no sub-typing of Event Definitions and Event Instances to differentiate single events and event groups; an event group is simply an event that has an associated set of child Event Definitions.

EventDefinition

An EventDefinition is an MO Object that contains static configuration data relating to multiple occurrences of a Planning Event. Its identity is defined by a constant definitionID and an evolving version, which is updated each time the definition is revised. Event Definitions form part of the Planning Configuration Data.

Events may be either Predicted or Potential. Events that are predictable either by time or position can have specific instances included in a Plan. Potential Events are those that may occur during the execution of a Plan, but the specific time or position is not predicted.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **EventDefinition** | **Extends** | MAL::Composite | **SFP** | 201 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| definitionID | MAL::ObjectID | No | ID of the EventDefinition. |
| version | MAL::Version | No | Version of the EventDefinition. |
| description | MAL::String | No | Description of the Event. |
| eventType | EventTypeEnum | No | Enumeration: one of {Predicted, Potential} indicating the type of Event. |
| displayType | MAL::String | Yes | Enables a planning system to customise presentation of the Event in displays. |
| argDefs | List <ArgDef> | Yes | List of Argument Definitions. |
| eventDefs | List <MAL::ObjectRef> | Yes | List of child Event Definitions. For a single Event, this list shall be empty; for a group Event, the list shall be populated. |

EventInstance

An EventInstance is an MO Object that contains the identity of a specific occurrence of a Planning Event, together with both static and dynamic information associated with that occurrence. It supports relationships to its definition and source.

The source of an EventInstance may be an external event, corresponding to a NAV Predicted Event or a CSS Contact Event.

EventInstances may be contained within a Plan.

EventInstances may be referenced as a related event by an ActivityInstance, so that the ActivityInstance can reference the timing and arguments of the related EventInstance.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **EventInstance** | **Extends** | MAL::Object | **SFP** | 202 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| instanceID | MAL::ObjectID | No | ID of the EventInstance |
| definition | MAL::ObjectRef | No | Reference to the EventDefinition |
| sourceEvent | MAL::Identifier | Yes | Reference to an external source event (e.g. NAV predicted event, or CSS contact event) |
| events | List <MAL::ObjectRef> | Yes | List of references to child EventInstances. For a single Event, this list is empty; for a group Event, the list will be populated. |
| eventTime | MAL::FineTime | Yes | Predicted or actual time of the Event. EventTime is nullable: it can be predicted without an EventTime (e.g. if Position based) |
| arguments | List <Argument> | Yes | Argument values for each Argument defined in the Event Definition. |
| eventStatus | EventStatusEnum | No | Current Status of the Event Instance (see Event State Model in §0) |
| terminationInfo | MAL::String | Yes | TerminationInfo provides the reason for entering the Terminated State and is customisable, but includes:  - Occurred (Event has been triggered)  - Did Not Occur (Event expired or did not occur within validity period)  - Deleted (Event was deleted) |

EventTypeEnum

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **EventTypeEnum** | **SFP** | 203 |

| Enumeration | Value | Description |
| --- | --- | --- |
| PREDICTED | 1 | Events that are predictable either by time or position can have specific instances included in a Plan. |
| POTENTIAL | 2 | Potential Events are those that may occur during the execution of a Plan, but the specific time or position is not predicted. |

#### Event State Model



Figure : Event State Model

The following states are defined for **EventStatus**:

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **EventStatusEnum** | **SFP** | 204 |

| Status | Value | Description |
| --- | --- | --- |
| GROUP | 1 | The Event is a Group Event |
| PLANNED | 2 | The Event Instance has been included in the Plan |
| ACTIVATED | 3 | The Plan including the Event Instance has been Activated within the Plan Execution function. |
| TERMINATED | 4 | The Event Instance has reached a terminal status (further information is provided in terminationInfo) |

The blue dashed boundary frames indicate which of Planning or Plan Execution functions is responsible for asserting these states. State transitions that occur as a result of an MPS service operation are marked with an \*, other transitions occur automatically as a result of Planning or Plan Execution processes.

When an EventInstance is created within the context of a Plan by the Planning function, it has the initial status of Planned if it is a single event, or Group if it is an event group.

Plans may be submitted to a Plan Execution function, but before they will execute they must be activated. Once a Plan has been activated, all contained Events that are single events will also become Activated.

The status of the Event is set to Terminated once it has occurred, or it will no longer occur. TerminationInfo provides the reason for termination and is customisable, but includes:

* Occurred (Event has been triggered)
* Did Not Occur (Event expired or did not occur within validity period)
* Deleted (Event was deleted)

#### Event Service Structures



Figure : Event Service Structures

This section defines data structures specific to Planning Events that are used in the context of MPS service operations and their associated messages.

EventUpdate

EventUpdate is a data structure that is used to report the dynamic status of an EventInstance in the context of the MPS Plan Execution Control service monitorPlanExecutionDetail operation.

EventUpdates may be distributed to subscribing applications, including status displays, to inform them of the latest status of the event. This may be particularly relevant in conjunction with a Plan Execution function. EventUpdates may be stored in Event History to provide a complete record of evolving status over time.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **EventUpdate** | **Extends** | MAL::Composite | **SFP** | 205 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| eventInstance | MAL::ObjectRef | No | Reference to the Event Instance to which the status update relates. |
| timestamp | MAL::Time | No | Time of status update. |
| eventTime | MAL::FineTime | No | Predicted or actual time of the Event. EventTime is nullable: it can be predicted without an EventTime (e.g. if Position based) |
| arguments | List <Argument> | Yes | Argument values. |
| eventStatus | EventStatusEnum | No | Current Status of the Event Instance. |
| terminationInfo | MAL::String | Yes | TerminationInfo provides the reason for entering the Terminated State and is customisable, but includes:  - Occurred (Event has been triggered)  - Did Not Occur (Event expired or did not occur within validity period)  - Deleted (Event was deleted) |

InsertedEventDetails

A data structure that provides the information required to create the EventInstance to be inserted into a Plan using the MPS Plan Edit service.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **InsertedEventDetails** | **Extends** | MAL::Composite | **SFP** | 206 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| plan | MAL::ObjectRef | No | Reference to the Plan into which the Event is to be inserted. |
| eventDef | MAL::ObjectRef | No | Reference to the EventDefinition |
| eventTime | MAL::FineTime | No | Specifies the predicted or actual time of the Event. For an inserted Event this must be present. |
| arguments | List <Argument> | Yes | Argument values. |

### Planning Resources [Optional]

Planning Resources are an optional element of the MPS Information Model. Support for Planning Resources is not a requirement for compliance of an MPS system with the MPS service interfaces.

#### Resource Objects



Figure : Planning Resources

Planning Resources follow the MO State Object Pattern, comprising a single class of MO Object. The resource definitions form part of the Planning Configuration Data for a mission planning system, but the same object identity is used to reference the value of the resource in a mission planning system.

Planning Resources can be of any MAL Attribute data type. The value of the Resource does not inherently require sub-types, as all data types can be represented by an attribute of type MAL::Attribute. However, as the attributes required to support data validation are type-specific, four distinct Resource Definition MO Object types are defined:

* Resource: the base type where data validation is not applicable.
* Numeric Resource: applicable for any numeric data type where a min-max range is defined for the Resource (including Durations).
* String Resource: applicable for Resources of type String.
* Status Resource: applicable for enumerated status Resources (of type Integer, but with interpreted status text strings).

The “x-axis” of a Resource is always Time: in other words it records the evolution of the value of the Resource over time, and not other dimensions (such as position).

Resource

A Resource is an MO Object that contains both the static attributes that define a Planning Resource and a dynamic attribute that holds its current value. Its identity is defined by a constant resourceID and evolving version, which is updated each time the definition is revised. Resource definitions form part of the Planning Configuration Data and in practice the value attribute may be omitted in this context, although it may also be used to provide an initial or default value.

As previously described, depending on the Resource DataType, the Resource definition may require additional type specific attributes to support data validation. SubTypes are defined for Numeric, String and enumerated Status type Resources. The base Resource MO Object type can be used where no data validation is applicable. The following attributes are applicable to the base type and all sub-types.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **Resource** | **Extends** | MAL::Composite | **SFP** | 301 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| resourceID | MAL::ObjectID | No | ID of the Resource. |
| version | MAL::Version | No | Version of the Resource definition. |
| description | MAL::String | No | Description of the Resource. |
| dataType | MAL::AttributeType | No | Specifies the data type of the Resource, which must be a supported MAL Attribute type. |
| units | MAL::String | Yes | Optional. Specifies the units the value of the Resource is expressed in. |
| value | MAL::Attribute | Yes | Value of the resource. MAL Attribute type must match the DataType of the Resource definition.  The value is only nullable in the context of a Resource Definition (Planning Configuration Data). |

NumericResource

Sub-type of Resource applicable to Resources of any numeric type, including Duration, that provides additional attributes for the specification of numeric data validation.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **NumericResource** | **Extends** | Resource | **SFP** | 302 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| minimum | ResourceProfile | No | Defines the permitted minimum value over time. |
| maximum | ResourceProfile | No | Defines the permitted maximum value over time. |

StringResource

Sub-type of Resource applicable to Resources of type String, that provides additional attributes for the specification of string data validation.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **StringResource** | **Extends** | Resource | **SFP** | 303 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| maxLength | MAL::Integer | No | Maximum length of the string (characters). |
| regex | MAL::String | No | A “regular expression” or sequence of characters defining a character pattern that the string value must match. |

StatusResource

Sub-type of Resource that provides additional attributes to support data validation and interpretation for integer type arguments that are effectively enumerated Statuses.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **StatusResource** | **Extends** | Resource | **SFP** | 304 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| allowedValues | List <StateDef> | No | Set of allowed State definitions (see §3.3.4), comprising the enumerated value and an associated text label. |

#### Resource Profiles



Figure : Resource Profiles

Resource Profiles provide the evolution of a value over time as a set of points.

They are used in both Resource Definitions where they can represent time-variant minimum and maximum values for the Resource; and in Plans where they represent the predicted evolution of a Resource value over the duration of the Plan.

The Profile comprises a series of profile segments, each of which identifies the time range covered, the interpolation method to be used between points, whether the start and end time are included in the segment, and a set of profile entries, each of which corresponds to a Time-Value pair.

The values in the Profile Entries are represented as MAL Attributes, the data type of which must match the defined DataType in the corresponding Resource definition.

It is noted that Interpolation methods are only relevant for resources of Numeric type.

Resource Profiles use absolute timestamps, but the derived Relative Resource Profile uses relative timestamps of type Duration (indicating an offset from a reference time, such as the start time of an Activity). Relative Resource Profiles are used in the context of a Complex Resource Constraint.

ResourceProfile

A Resource Profile provides the evolution of a value for a single Planning Resource over time as a set of Profile Segments.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ResourceProfile** | **Extends** | MAL::Composite | **SFP** | 305 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| resource | MAL::ObjectRef | No | Reference to a Resource |
| profileSegments | List <ProfileSegment> | No | Set of Profile Segments |

ProfileSegment

A Profile Segment defines the time range and interpolation method for a set of Profile Entries.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ProfileSegment** | **Extends** | MAL::Composite | **SFP** | 306 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| interpolation | InterpolationTypeEnum | No | Interpolation method to be applied for values lying between points defined in the Profile Segment.  Default = Step. |
| start | TimeExpression | No | Start of time range covered by the Profile Segment. |
| end | TimeExpression | No | End of time range covered by the Profile Segment |
| startIncluded | MAL::Boolean | No | Indicates whether the Start time is included in the Profile Segment.  Default = True. |
| endIncluded | MAL::Boolean | No | Indicates whether the End time is included in the Profile Segment. This allows the same Time to be used as the end of one segment and the start of another.  Default = False. |
| profileEntries | List <ProfileEntry> | No | Set of Profile Entries (resource value points). |

InterpolationTypeEnum

The following InterpolationTypes are defined:

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **InterpolationTypeEnum** | **SFP** | 307 |

| Enumeration | Value | Description |
| --- | --- | --- |
| STEP | 1 | No interpolation: resource values remain unchanged between defined points. |
| LINEAR | 2 | Linear interpolation: resource values follow a straight line between defined points. |
| POLYNOMIAL | 3 | Polynomial interpolation: resource values follow a curve fitting the defined points. |

ProfileEntry

Defines the value [or minimum/maximum value] of a resource at a particular point in time.

The data type of the Value can be any valid MAL Attribute type, but must match the defined DataType in the corresponding Resource definition.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ProfileEntry** | **Extends** | MAL::Composite | **SFP** | 308 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| time | TimeExpression | No | Time of resource data point |
| value | MAL::Attribute | No | Value of resource data point |

RelativeResourceProfile

A variation on Resource Profile, the Relative Resource Profile uses relative timestamps of type Duration (indicating an offset from a reference time, such as the start time of an Activity). Relative Resource Profiles are used in the context of a Complex Resource Constraint.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RelativeResourceProfile** | **Extends** | MAL::Composite | **SFP** | 309 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| resource | MAL::ObjectRef | No | Reference to a Resource |
| profileSegments | List <RelativeProfileSegment> | No | Set of Relative Profile Segments |

RelativeProfileSegment

A Relative Resource Segment defines the time range and interpolation method for a set of Relative Profile Entries.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RelativeProfileSegment** | **Extends** | MAL::Composite | **SFP** | 310 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| interpolation | InterpolationTypeEnum | No | Interpolation method to be applied for values lying between points defined in the Profile Segment.  Default = Step. |
| start | DurationExpression | No | Relative Start of time range covered by the Relative Profile Segment. |
| end | DurationExpression | No | Relative End of time range covered by the Relative Profile Segment |
| startIncluded | MAL::Boolean | No | Indicates whether the Start time is included in the Profile Segment.  Default = True. |
| endIncluded | MAL::Boolean | No | Indicates whether the End time is included in the Profile Segment. This allows the same Time to be used as the end of one segment and the start of another.  Default = False. |
| profileEntries | List <RelativeProfileEntry> | No | Set of Relative Profile Entries (resource value points). |

RelativeProfileEntry

Defines the value [or minimum/maximum value] of a resource at a relative point in time.

Specific sub-types exist for each allowed data type for a Resource. These replace the Variant type Value attribute with one of concrete data type.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RelativeProfileEntry** | **Extends** | MAL::Composite | **SFP** | 311 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| time | DurationExpression | No | Relative time of resource data point |
| value | MAL::Attribute | No | Value of resource data point |

#### Resource Service Structures



Figure : Resource Service Structures

This section defines data structures specific to Planning Resources that are used in the context of MPS service operations and their associated messages.

ResourceUpdate

ResourceUpdate is a data structure that is used to report the value of a Resource at a given point in time in the context of the MPS Plan Execution Control service monitorPlanExecutionDetail operation, or to supply an updated value for a Resource in the context of the MPS Plan Edit service.

Resource Updates may be distributed to subscribing applications, including status displays, to inform them of the latest value of the Resource. This may be particularly relevant in conjunction with a Plan Execution function. Resource Updates may be stored in Resource History to provide a complete record of evolving value over time.

Resource Updates are also effectively contained within a Plan to describe the predicted evolution of Resources over the duration of that Plan. However, in this context the Resource Profile construct is used (see 3.2.4.2 above).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ResourceUpdate** | **Extends** | MAL::Composite | **SFP** | 312 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| resource | MAL::ObjectRef | No | Reference to the Resource to which the value update relates. |
| timestamp | MAL::Time | No | Time of Resource value update. |
| value | MAL::Attribute | No | Value of the resource. MAL Attribute type must match the DataType of the Resource Definition. |

### Planning Requests

#### Planning Request Objects



Figure : Planning Requests

Planning Requests follow the MO Instance Object Pattern, comprising Definition and Instance classes of MO Object, although in this case Planning Request instances can be created without reference to a Planning Request Definition.

Request Definitions provide a re-usable template for common Planning Requests from which specific Request Instances can be created and form part of the Planning Configuration Data for a mission planning system. They include the details of a planning request that are generic to multiple invocations of the request, including the set of Planning Activities to be requested and any planning constraints specific to the request. Arguments may be specified to parameterise the planning request and referred to within the requested planning activities or specified constraints. They differ from Activity and Event definitions in two regards:

* RequestInstances can be created without reference to any RequestDefinition.
* Any aspect of a RequestInstance created from a RequestDefinition can be modified, including the set of requested Planning Activities and the constraints applicable. Once created a RequestInstance is independent from any initial RequestDefinition, although a reference is retained.

Request Instances specify the details of a planning request, including the set of Planning Activities being requested and any planning constraints specific to the request. Arguments may be specified to parameterise the planning request and referred to within the requested planning activities or specified constraints.

The ID of the Request Instance are assigned by the planning function and returned to the requester as part of the MPS Planning Request service SubmitRequest operation. A user supplied reference may also be included in the body of the request. Where a planning request is updated by the user and resubmitted to a planning function, a new version of the RequestInstance is created, but retains the same ID.

Planning requests may also reference or include an existing Plan as the body of the request. In this case the referenced Plan corresponds to the output of one planning process, but is being requested as the input to another.

RequestDefinition

A RequestDefinition is an MO Object that contains the specification of a re-usable planning request template.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RequestDefinition** | **Extends** | MAL::Composite | **SFP** | 1 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| definitionID | MAL::ObjectID | No | ID of the RequestDefinition |
| version | MAL::Version | No | Version of the RequestDefinition |
| description | MAL::String | No | Description of the re-usable RequestDefinition. |
| argDefs | List <ArgDef> | Yes | List of Argument Definitions. Arguments may be referenced in ActivityDetails and constraints. |
| standingOrder | MAL::Boolean | No | A flag that indicates whether the planning request is for a repetitive standing order (unbounded other than by the validity period), or is a one-off request. If it is a standing order, then the ActivityNode must include specification of the repetition criteria. Note that a one-off request can still include repetition. |
| constraints | ConstraintNode | Yes | Set of Constraints applicable to the whole planning request. Note that constraints specific to a Planning Activity can be specified within the ActivityDetails for that activity within the ActivityNode. |
| activities | ActivityNode | No | Set of Activity Details specifying requested activities, optionally with repetition. |

RequestInstance

A RequestInstance is an MO Object that contains the specification of a planning request. This may change over time if the request is updated by the user, each comprising a separate version of the request with the same Object ID.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RequestInstance** | **Extends** | MAL::Composite | **SFP** | 2 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| instanceID | MAL::ObjectID | No | ID of the RequestInstance |
| version | MAL::Version | No | Version of the RequestInstance |
| userReference | MAL::Identifier | Yes | Optional user supplied reference for the planning request. This is distinct from the instancetID of the RequestInstance that is assigned by the planning function. |
| creationDate | MAL::Time | No | Creation date-time of the RequestInstance version. |
| definition | MAL::ObjectRef | Yes | Reference to the RequestDefinition from which the RequestInstance was created, if a planning request template was used. |
| planningPeriod | MAL::Identifier | No | Specifies which planning period the planning request applies to. Planning period IDs are mission specific, but can be used to indicate mission phase; planning cycle; or “semester” in observatory missions. |
| validityTime | List <TimeWindow> | Yes | Validity period for the planning request, expressed as one or more time windows. The planning request must be satisfied within this period.  Only one of validityTime or validityEvent should be present in a planning request. |
| validityEvent | List <EventWindow> | Yes | Validity period for the planning request, expressed as one or more event windows. The planning request must be satisfied within this period.  Only one of validityTime or validityEvent should be present in a planning request. |
| timeReference | TimeReferenceEnum | Yes | Specifies the Time reference used for all Time attributes within the planning request.  If Null, default Time Reference for the system is used. |
| user | MAL::ObjectRef | No | The User ID for the person or organisation raising the planning request. |
| description | MAL::String | No | Description of the Request. |
| arguments | List <Argument> | Yes | List of named Argument values. If created from a template planning request , this will include the arguments defined in the RequestDefinition. |
| standingOrder | MAL::Boolean | No | A flag that indicates whether the planning request is for a repetitive standing order (unbounded other than by the validity period), or is a one-off request. If it is a standing order, then the ActivityNode must include specification of the repetition criteria. Note that a one-off request can still include repetition. |
| constraints | ConstraintNode | Yes | Set of Constraints applicable to the whole planning request. Note that constraints specific to a Planning Activity can be specified within the ActivityDetails for that activity within the ActivityNode. |
| activities | ActivityNode | No | Set of Activity Details specifying requested activities, optionally with repetition. |
| inputPlanRef | MAL::ObjectRef | Yes | Optional. Reference to an existing Plan (output of one planning function) submitted as a planning request to another planning function in the context of a distributed or hierarchical planning system.  Only one of inputPlanRef and inputPlan should be present within the planning request. |
| inputPlan | Plan | Yes | Optional. An existing Plan (output of one planning function) submitted as a planning request to another planning function in the context of a distributed or hierarchical planning system. The plan is embedded within the planning request.  Only one of inputPlanRef and inputPlan should be present within the planning request. |
| comments | MAL::String | Yes | Free text for any additional user comments about the request. |
| status | RequestStatusEnum | No | Current Status of the Activity Instance (see Planning Request State Model in §3.2.5.2) |
| outputPlanRef | List<MAL::ObjectRef> | Yes | Optional. Reference to the output Plan(s) that contains the activities resulting from the planning request. Where multiple alternate plans have been generated, these may be listed here. |
| terminationInfo | MAL::String | Yes | TerminationInfo provides the reason for termination and is customisable, but includes:  - Completed (all constituent activities completed successfully)  - Expired (constituent activities expired prior to execution)  - Failed (constituent activities failed during execution)  - Deleted (constituent activities were deleted) |
| errCode | MAL::Integer | Yes | Error Code relevant in the case of a failure status for the planning request. |
| errInfo | MAL::String | Yes | Supplementary Error Information |

#### Planning Request State Model



Figure : Planning Request State Model

The following states are defined for **RequestStatus**:

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **RequestStatusEnum** | **SFP** | 3 |

| Status | Value | Description |
| --- | --- | --- |
| REQUESTED | 1 | The Planning Request has been submitted to the Planning function |
| ACCEPTED | 2 | The Planning Request has been accepted by the Planning function |
| REJECTED | 3 | The Planning Request has been rejected by the Planning function |
| CANCELLED | 4 | The Planning Request has been cancelled by the User |
| PLANNED | 5 | The Planning Request has been incorporated into a Plan (see outputPlanRef) |
| ACTIVATED | 6 | The corresponding Plan has been activated within PlanExecution |
| EXECUTING | 7 | Execution of the first constituent Activity of the Planning Request has been initiated |
| TERMINATED | 8 | Execution of all constituent Activities of the Planning Request have been terminated (further information is provided in terminationInfo) |

All states are asserted by the Planning function. The blue dashed boundary frame indicates those states which require status feedback from the Plan Execution function.

When a planning request is first received by a Planning function from a user (via an MPS Planning Request Service SubmitRequest operation) the RequestInstance is created with an initial state of Requested. The Planning function may then accept or reject the request, setting its status to Accepted or Rejected accordingly.

Once the Planning function has included the planning activities associated with the request in a Plan, the RequestInstance status is set to Planned.

An UpdateRequest service operation may be used to modify a planning request in the Accepted, Rejected or Planned state, in which case the RequestInstance version is updated and its status reverts to Requested.

A CancelRequest service operation may be used to cancel a planning request in the Accepted or Planned state, in which case the RequestInstance status is set to Cancelled.

Once a Plan containing the requested planning activities has been submitted to a Plan Execution function, further status updates are dependent on feedback received by the Planning function from Plan Execution. It is implementation dependent at what point the RequestInstance status is updated, but the following execution stages are defined:

* Activated once the containing Plan has been activated
* Executing once the first constituent Activity has been initiated
* Terminated once all constituent Activities have been terminated

An MPS system may support re-planning of failed activities without requiring a new Planning Request. To support this, the transition of the RequestInstance from Terminated to Planned is permitted.

TerminationInfor provides more detailed information on reason for termination of the planning request and is customisable, but includes:

* Completed (all constituent activities completed successfully)
* Expired (constituent activities expired prior to execution)
* Failed (constituent activities failed during execution)
* Deleted (constituent activities were deleted)

#### Planning Request Service Structures



RequestStatusUpdate

RequestStatusUpdate is a data structure that is used to report changes in status of the RequestInstance as it proceeds through both planning and plan execution functions. Reporting is the responsibility of the planning function.

Planning request status updates may be distributed to subscribing applications, including both Users and status displays, to inform them of the latest status of the planning request. This may be particularly relevant in conjunction with a Plan Execution function. Status updates may be stored in Planning Request History to provide a complete record of evolving status over time.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RequestStatusUpdate** | **Extends** | MAL::Composite | **SFP** | 4 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| requestInstance | MAL::ObjectRef | No | Reference to the Planning Request Instance to which the status update relates. |
| timestamp | MAL::Time | No | Time of status update. |
| status | RequestStatusEnum | No | Current status of the planning request. |
| outputPlanRef | MAL::ObjectRef | Yes | Reference to the Plan that contains the planned activities resulting from the planning request. Note that this is only available once the planning request has been processed and successfully planned. The outputPlanRef may be updated following iterative planning cycles or re-planning. |
| terminationInfo | MAL::String | Yes | TerminationInfo provides the reason for termination and is customisable, but includes:  - Completed (all constituent activities completed successfully)  - Expired (constituent activities expired prior to execution)  - Failed (constituent activities failed during execution)  - Deleted (constituent activities were deleted) |
| errCode | MAL::Integer | Yes | Error Code relevant in the case of a failure status for the planning request. |
| errInfo | MAL::String | Yes | Supplementary Error Information. |

PlanningRequestDetails

PlanningRequestDetails is a data structure used in the context of the MPS Planning Request service SubmitRequest and UpdateRequest operations, where the RequestInstance MO object cannot be used as the full identity of the resulting RequestInstance (ID and Version) is not yet known.

Its structure is equivalent to that of RequestInstance, but omitting the identity attributes and dynamic attributes used to report its status.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanningRequestDetails** | **Extends** | MAL::Composite | **SFP** | 5 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| userReference | MAL::Identifier | No | User supplied reference for the planning request. This is distinct from the instancetID of the RequestInstance that is assigned by the planning function. |
| definition | MAL::ObjectRef | Yes | Reference to the RequestDefinition from which the RequestInstance was created, if a planning request template was used. |
| planningPeriod | MAL::Identifier | No | Specifies which planning period the planning request applies to. Planning period IDs are mission specific, but can be used to indicate mission phase; planning cycle; or “semester” in observatory missions. |
| validityTime | List <TimeWindow> | Yes | Validity period for the planning request, expressed as one or more time windows. The planning request must be satisfied within this period.  Only one of validityTime or validityEvent should be present in a planning request. |
| validityEvent | List <EventWindow> | Yes | Validity period for the planning request, expressed as one or more event windows. The planning request must be satisfied within this period.  Only one of validityTime or validityEvent should be present in a planning request. |
| timeReference | TimeReferenceEnum | Yes | Specifies the Time reference used for all Time attributes within the planning request.  If Null, default Time Reference for the system is used. |
| user | MAL::ObjectRef | No | The User ID for the person or organisation raising the planning request. |
| description | MAL::String | No | Description of the Request. |
| arguments | List <Argument> | Yes | List of named Argument values. If created from a template planning request , this will include the arguments defined in the RequestDefinition. |
| standingOrder | MAL::Boolean | No | A flag that indicates whether the planning request is for a repetitive standing order (unbounded other than by the validity period), or is a one-off request. If it is a standing order, then the ActivityNode must include specification of the repetition criteria. Note that a one-off request can still include repetition. |
| constraints | ConstraintNode | Yes | Set of Constraints applicable to the whole planning request. Note that constraints specific to a Planning Activity can be specified within the ActivityDetails for that activity within the ActivityNode. |
| activities | ActivityNode | No | Set of Activity Details specifying requested activities, optionally with repetition. |
| inputPlanRef | MAL::ObjectRef | Yes | Optional. Reference to an existing Plan (output of one planning function) submitted as a planning request to another planning function in the context of a distributed or hierarchical planning system.  Only one of inputPlanRef and inputPlan should be present within the planning request. |
| inputPlan | Plan | Yes | Optional. An existing Plan (output of one planning function) submitted as a planning request to another planning function in the context of a distributed or hierarchical planning system. The plan is embedded within the planning request.  Only one of inputPlanRef and inputPlan should be present within the planning request. |
| comments | MAL::String | Yes | Free text for any additional user comments about the request. |

PlanningRequestResponse

PlanningRequestResponse is a data structure used in the context of the MPS Planning Request service SubmitRequest and UpdateRequest operations, in response to the submitted PlanningRequestDetails defined above. It contains a reference to the created RequestInstance and the supplied userReference to allow the user to correlate the two.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanningRequestResponse** | **Extends** | MAL::Composite | **SFP** | 6 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| instance | MAL::ObjectRef | No | Reference to the RequestInstance created in response to a SubmitRequest operation, or the updated version of the RequestInstance following an UpdateRequest operation. |
| userReference | MAL::Identifier | No | User supplied reference for the planning request. This is distinct from the instancetID of the RequestInstance that is assigned by the planning function. |

RequestSummaryStatus

RequestSummaryStatus is a data structure used in the context of the MPS Planning Request service getRequestSummaries operation, where a list of these structures is returned. It contains header fields of the planning request and its status, but not the request content (arguments, activities and constraints).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RequestSummaryStatus** | **Extends** | MAL::Composite | **SFP** | 7 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| requestInstance | MAL::ObjectRef | No | Reference to the RequestInstance (ID and Version). |
| userReference | MAL::Identifier | Yes | Optional user supplied reference for the planning request. This is distinct from the instancetID of the RequestInstance that is assigned by the planning function. |
| creationDate | MAL::Time | No | Creation date-time of the RequestInstance version. |
| definition | MAL::ObjectRef | Yes | Reference to the RequestDefinition from which the RequestInstance was created, if a planning request template was used. |
| planningPeriod | MAL::Identifier | No | Specifies which planning period the planning request applies to. Planning period IDs are mission specific, but can be used to indicate mission phase; planning cycle; or “semester” in observatory missions. |
| validityTime | List <TimeWindow> | Yes | Validity period for the planning request, expressed as one or more time windows. The planning request must be satisfied within this period.  Only one of validityTime or validityEvent should be present in a planning request. |
| validityEvent | List <EventWindow> | Yes | Validity period for the planning request, expressed as one or more event windows. The planning request must be satisfied within this period.  Only one of validityTime or validityEvent should be present in a planning request. |
| user | MAL::ObjectRef | No | The User ID for the person or organisation raising the planning request. |
| description | MAL::String | No | Description of the Request. |
| standingOrder | MAL::Boolean | No | A flag that indicates whether the planning request is for a repetitive standing order (unbounded other than by the validity period), or is a one-off request. If it is a standing order, then the ActivityNode must include specification of the repetition criteria. Note that a one-off request can still include repetition. |
| comments | MAL::String | Yes | Free text for any additional user comments about the request. |
| status | RequestStatusEnum | No | Current Status of the Activity Instance (see Planning Request State Model in §3.2.5.2) |
| outputPlanRef | MAL::ObjectRef | Yes | Optional. Reference to the output Plan that contains the activities resulting from the planning request. |
| terminationInfo | MAL::String | Yes | TerminationInfo provides the reason for termination and is customisable, but includes:  - Completed (all constituent activities completed successfully)  - Expired (constituent activities expired prior to execution)  - Failed (constituent activities failed during execution)  - Deleted (constituent activities were deleted) |

RequestFilter

RequestFilter is a data structure used in the context of MPS Planning Request Service operations to specify a filtered set of Planning Requests. All filter criteria specified are applied (logical AND, not OR).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RequestFilter** | **Extends** | MAL::Composite | **SFP** | 8 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| domain | MAL::Identifier | Yes | Domain of the RequestInstance |
| instanceID | MAL::ObjectRef | Yes | instanceID (and Version) of the RequestInstance |
| creationDate | MAL::Time | Yes | Creation date-time of the RequestInstance version. |
| definitionID | MAL::ObjectRef | Yes | definitionID (and Version) of the RequestInstance (the RequestDefinition from which it was created) |
| userID | MAL::ObjectRef | Yes | userID of the User who initiated the RequestInstance |
| userReference | MAL::Identifier | Yes | Reference supplied by User when submitting the RequestInstance. |
| status | RequestStatusEnum | Yes | Current status (enum) of the RequestInstance |
| outputPlanRef | MAL::ObjectRef | Yes | Reference to the output Plan generated in response to the RequestInstance |

### Plans

#### Plan Object



Figure : Plans

Plans follow the MO State Object Pattern, comprising a single class of MO Object. Plans are dynamically created and do not form part of the Planning Configuration Data. They specify the details of a generated plan that is the output of a Planning function. Plans are versioned: the same planID can be used for successive iterations of a Plan, each differentiated by the version of the Plan.

The major part of a Plan is a static data structure that effectively comprises general header information followed by four sections, as shown in Figure 22 below:

* Plan Information
* Planned Items (contains planned activities and events)
* Plan Revisions (details changes from a predecessor plan)
* Plan Resources (contains planning resource profiles)

Each of these sections is represented by its own data structure, defined in the following subsections. Both Plan Revisions and Plan Resources are optional elements of the Plan. It is also optional whether planning events are included within the Planned Items section.

The evolving status of a Plan is represented by a set of dynamic attributes that can be updated during the lifetime of a version of a Plan.

Plans can represent a Full Plan (contains all elements of the plan) or a Patch Plan (contains the delta from a predecessor plan only).

A Full Plan may have a predecessor Plan with which it overlaps and specifies changes in the Plan Revisions. If there is no predecessor, then it is a self-standing plan. The specification of Plan Revisions in a Full Plan allows a plan execution function to merge the successor plan into an already loaded predecessor plan by applying only the changes identified. Alternatively the already loaded plan can be discarded and the entire plan loaded from the Full Plan.

A Patch Plan must have a predecessor Plan to which it is the delta. It contains only the differences between the predecessor Plan and a target Plan. If a Patch Plan is used in the context of a Planning Request it will not have a target Plan. If the Patch Plan is a distributed output of a planning function, it must also have the reference to the target Plan. It is only possible for a plan execution function to merge a Patch Plan into an already loaded predecessor plan by applying the changes identified – it does not include the full specification of the plan to be loaded from scratch.



Figure : Plan Details

The component parts are the same for Full and Patch Plans.

For a Patch Plan, only Planned Items that are new or modified with respect to the Predecessor Plan Version are included. Unchanged items should not be present, while a Full Plan will include any unchanged items.

A Patch Plan must have a Plan Revision, and only one Plan Revision can be present - relative to the Predecessor Plan Version. Updated Resource Profiles may also be included. This is unlikely to be relevant for a Patch Plan that is a request.

Several plans may share the same predecessor, representing alternative options. Plans may be released as Operational or Alternate plans. An Operational plan is the default to be applied, while Alternate plans may be provided to allow for a last-minute operational choice or to handle predicted contingency situations. Whether a Plan is Operational or Alternate can be modified after it has been generated and this status is therefore a dynamic attribute.

Plan

A Plan is an MO Object that contains both the static attributes that define a version of a Plan and dynamic attributes that hold its current state. Its identity is defined by a constant planID and an evolving version, which is updated each time the plan is revised.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **Plan** | **Extends** | MAL::Composite | **SFP** | 1 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| planID | MAL::ObjectID | No | ID of the Plan |
| version | MAL::Version | No | Version of the Plan |
| hasPrecursor | MAL::Boolean | No | Flag indicating if the plan has a predecessor Plan from which the changes are detailed in Plan. This may be used if there is an iterative re-planning cycle in which successive plans overlap, or where a previous plan has been updated through re-planning. If there is no predecessor, then the Plan must be a self-standing Full Plan. |
| isPatchPlan | MAL::Boolean | No | Flag indicating if the plan is a Patch Plan that only contains details of the changes from the predecessor Plan. A Patch Plan must have a predecessor and the hasPrecursor flag must be set to True. It must also include a single PlanRevision relative to the predecessor Plan. |
| precursorPlan | MAL::ObjectRef | Yes | Reference to the predecessor Plan, nullable only if the hasPrecursor flag is set to False. |
| targetPlan | MAL::ObjectRef | Yes | Applicable only for Patch Plans, this is a reference to the target Plan. This target Plan is the result of applying the PatchPlan to the predecessor Plan and is distinct from the identity of the PatchPlan itself. For a Patch Plan used in the context of a planning request, this is set to null. |
| information | PlanInformation | No | Contains header information relating to the Plan, including its originator and validity period. |
| items | PlannedItems | No | Contains the planned activities and events that constitute the plan. |
| revisions | PlanRevisions | Yes | Details the changes between this Plan and other Plans (or other versions of the same Plan), usually the predecessor Plan. Optional, but must be present in a Patch Plan. |
| resources | PlanResources | Yes | Optional. Contains resource profiles for planning resources covering the period of the plan. |
| isAlternate | MAL::Boolean | No | Flag indicating if the Plan has currently been released as an Operational or Alternate plan. |
| status | PlanStatusEnum | No | Current status of the Plan. |
| terminationInfo | MAL::String | Yes | Supplementary information for a plan in the Terminated state. This is customisable, but includes:  - Completed (nominal)  - Superseded (by a successor Plan)  - Revoked  - Expired |

##### Plan Information

PlanInformation

The Plan Information section of a Plan contains administrative and validity details associated with the plan as a whole.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanInformation** | **Extends** | MAL::Composite | **SFP** | 2 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| originator | MAL::Identifier | No | Identity of the entity or system responsible for the production of the Plan. |
| productionDate | MAL::Time | No | Date and time of production of the Plan. |
| description | MAL::String | No | Description of the Plan. |
| comments | MAL::String | Yes | Field for additional comments or notes to the operations team regarding the plan. |
| validityStart | MAL::Time | No | Start of validity period for the Plan.  The validity period defines when the Plan is available for operational use. It cannot be used outside its validity period. |
| validityEnd | MAL::Time | No | End of validity period for the Plan. |
| planPeriodStart | Trigger | No | Start of the plan period.  The plan period defines the start and end points of the plan. Planned items (planning activities and events) contained within the plan must at least partially overlap the plan period. The use of the trigger structure allows this to be specified in terms of Time, Position, Pointing or Planning Events. Examples are:  - a specified period of time  - an orbital repeat cycle  - a period between two events |
| planPeriodEnd | Trigger | No | End of the plan period. |
| timeReference | TimeReferenceEnum | Yes | Specifies the Time reference used for all Time attributes within the plan.  If Null, default Time Reference for the system is used. |

##### Planned Items

The PlannedItems section of the Plan specifies the set of planning activities and planning events contained within the plan. It comprises two lists of contained MO objects: one of EventInstances and one of ActivityInstances. Both lists can be empty.

If the Plan is a Full Plan, then there must be an entry in the list for all planned items contained within the plan, whether changed or not. If the Plan is a Patch Plan, then there is only an entry in the list for those planned items that have changed (new or modified).

PlannedItems

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlannedItems** | **Extends** | MAL::Composite | **SFP** | 3 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| plannedEvents | List <EventInstance> | Yes | List of Planned Events contained within the Plan. |
| plannedActivities | List <ActivityInstance> | Yes | List of Planned Activities contained within the Plan. |

##### Plan Revisions [Optional]

The optional PlanRevisions section details the changes between this Plan and another Plan. PlanRevisions comprise a collection of PlanRevision structures, each of which details the changes with respect to one version of a Plan (the revised plan).

In the typical case, there is only one PlanRevision corresponding to the changes between the Plan and its predecessor. However, it is possible to include multiple PlanRevision structures documenting the differences with any other version of a Plan. This can be used to provide a change history for successive versions of the same Plan, or to document the differences between alternate Plans.

In the case of a Patch Plan, the Plan must include a single PlanRevision relative to the predecessor Plan.

Each PlanRevision comprises an ordered set of ItemRevisions that document the change to individual planned items (planning events and activities). The order should be from earliest to latest within the plan period. Each ItemRevision references an individual EventInstance or ActivityInstance and indicates whether the planned item is new, modified or deleted in the current plan. New or modified items must also exist within the PlannedItems section of the Plan, but deleted items are not contained within the current Plan. Note that unmodified items do not appear in the PlanRevision.

PlanRevisions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanRevisions** | **Extends** | MAL::Composite | **SFP** | 4 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| planRevisions | List <PlanRevision> | No | Set of PlanRevision structures, each detailing the change with respect to an identified Plan. |

PlanRevision

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanRevision** | **Extends** | MAL::Composite | **SFP** | 5 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| revisedPlan | MAL::ObjectRef | No | Reference to the Plan (ID and version) with respect to which the plan revisions are detailed. Typically this is the predecessor plan, but any other Plan can be used. |
| revisionStart | MAL::Time | No | Start time of the earliest revision. |
| revisionEnd | MAL::Time | No | End time of the latest revision. |
| itemRevisions | List <ItemRevision> | Yes | Ordered list (earliest to latest) of revisions to planned items (activity and event instances). |

ItemRevision

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ItemRevision** | **Extends** | MAL::Composite | **SFP** | 6 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| itemRef | MAL::ObjectRef | No | Reference to a planned ActivityInstance or EventInstance that is new or modified in the current Plan, or has been deleted with respect to the referenced revisedPlan. |
| revisionStatus | RevisionStatusEnum | No | Revision status of the referenced item. May be one of New, Modified or Deleted. Default = Undefined. |

RevisionStatusEnum

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **RevisionStatusEnum** | **SFP** | 7 |

| Status | Value | Description |
| --- | --- | --- |
| NEW | 1 | The item is new in this revision of the Plan. |
| MODIFIED | 2 | The item has been modified in this revision of the Plan. |
| DELETED | 3 | The item has been deleted in this revision of the Plan. |
| UNDEFINED | 4 | The item is unchanged in this revision of the Plan, or its revision status is undefined. |

##### Plan Resources [Optional]

The optional PlanResources section allows the projected values of Planning Resources to be communicated between distributed planning and plan execution functions as part of a Plan.

This is provided as a set of ResourceProfiles (see §3.2.4.2), one per Planning Resource included. Resource profiles can provide the projected evolution of the value of a planning resource over the period of the plan. Alternatively it can provide a single value at the start of the plan to enable synchronisation between planning systems. It is a deployment choice which approach is used.

PlanResources

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanResources** | **Extends** | MAL::Composite | **SFP** | 8 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| resourceProfiles | List <ResourceProfile> | No | Set of resource profiles, one per planning resource, containing the initial value of the resource and optionally the projected evolution of the resource value over the period of the plan. |

#### Plan State Model



Figure : Plan State Model

The following states are defined for **PlanStatus**:

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **PlanStatusEnum** | **SFP** | 9 |

| Status | Value | Description |
| --- | --- | --- |
| DRAFT | 1 | The Plan has been saved by the Planning function |
| RELEASED | 2 | The Plan has been released for operational use by the Planning function |
| SUBMITTED | 3 | The Plan has been submitted to the Plan Execution function and is available for use, but will not execute until activated. |
| ACTIVATED | 4 | The Plan has been activated by the Plan Execution function |
| TERMINATED | 5 | The Plan has reached a terminal state, as detailed in the terminationInfo. This includes the following cases:  - Completed (nominal)  - Superseded by a successor Plan  - Revoked by a user  - Expired (reached the end of its validity period without being activated) |

The blue dashed boundary frames indicate which of Planning or Plan Execution functions is responsible for asserting these states. State transitions that occur as a result of an MPS service operation are marked with an \*, other transitions occur automatically as a result of Planning or Plan Execution processes.

Draft and Released states are asserted by the planning function with the transition normally being under user control.

Submitted, Activated and Terminated states are asserted by the plan execution function.

A Plan may be submitted to a Plan Execution function using the MPS Plan Execution Control service SubmitPlan operation, upon which it enters the Submitted state. The Plan and its contained Activities will not execute until the Plan has been activated using the ActivatePlan operation, when its state becomes Activated. The Plan enters the Terminated state when its execution has been completed, or it has been superseded by the activation of a successor Plan.

A Plan in the Activated state may be deactivated using the DeactivatePlan operation, but remains available for re-activation.

A Plan in the Submitted or Activated states may be made permanently unavailable for execution using the RevokePlan operation, in which case it is placed in the Terminated state. A Plan may also move to the Terminated state if its validity period has expired.

#### Plan Service Structures



Figure : Plan Service Structures

This section defines data structures specific to Plans that are used in the context of MPS service operations and their associated messages.

PlanUpdate

PlanUpdate is a data structure that is used to report changes in status of the Plan as it proceeds through both planning and plan execution functions. It is returned in the context of the MPS Plan Distribution service GetPlanStatus and MonitorPlanStatus operations, and also the MPS Plan Execution Control service MonitorPlanExecution and GetPlanStatus operations.

PlanUpdates may be distributed to subscribing applications, including status displays, to inform them of the latest status of a Plan. PlanUpdates may be stored in Plan History to provide a complete record of evolving status over time.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanUpdate** | **Extends** | MAL::Composite | **SFP** | 10 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| plan | MAL::ObjectRef | No | Reference to the Plan (ID and version) to which the status update relates. |
| timestamp | MAL::Time | No | Time of status update. |
| isAlternate | MAL::Boolean | No | Flag indicating if the Plan has currently been released as an Operational or Alternate plan. |
| status | PlanStatusEnum | No | Current status of the Plan. |
| terminationInfo | MAL::String | Yes | Supplementary information for a plan in the Terminated state. This is customisable, but includes: - Completed (nominal)  - Superseded (by a successor Plan)  - Revoked  - Expired |

PlanSummaryStatus

PlanSummaryStatus is a data structure that provides an summary view of a Plan that includes the PlanInformation section and current status, but not the full details of the plan. It is returned in the context of the MPS Plan Distribution service GetPlanSummaries operation.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanSummaryStatus** | **Extends** | MAL::Composite | **SFP** | 11 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| plan | MAL::ObjectRef | No | Reference to the Plan (ID and version) to which the Summary Status relates. |
| hasPrecursor | MAL::Boolean | No | Flag indicating if the plan has a predecessor Plan from which the changes are detailed in Plan. This may be used if there is an iterative re-planning cycle in which successive plans overlap, or where a previous plan has been updated through re-planning. If there is no predecessor, then the Plan must be a self-standing Full Plan. |
| isPatchPlan | MAL::Boolean | No | Flag indicating if the plan is a Patch Plan that only contains details of the changes from the predecessor Plan. A Patch Plan must have a predecessor and the hasPrecursor flag must be set to True. It must also include a single PlanRevision relative to the predecessor Plan. |
| precursorPlan | MAL::ObjectRef | Yes | Reference to the predecessor Plan, nullable only if the hasPrecursor flag is set to False. |
| targetPlan | MAL::ObjectRef | Yes | Applicable only for Patch Plans, this is a reference to the target Plan. This target Plan is the result of applying the PatchPlan to the predecessor Plan and is distinct from the identity of the PatchPlan itself. For a Patch Plan used in the context of a planning request, this is set to null. |
| information | PlanInformation | No | Contains header information relating to the Plan, including its originator and validity period. |
| isAlternate | MAL::Boolean | No | Flag indicating if the Plan has currently been released as an Operational or Alternate plan. |
| status | PlanStatusEnum | No | Current status of the Plan. |
| terminationInfo | MAL::String | Yes | Supplementary information for a plan in the Terminated state. |

PlanActivationStatus

PlanActivationStatus is a data structure that returns the activation status of a Plan in the context of the MPS Plan Execution Control service ActivatePlan and DeactivatePlan operations.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanActivationStatus** | **Extends** | MAL::Composite | **SFP** | 12 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| plan | MAL::ObjectRef | No | Reference to the Plan (ID and version) to which the status relates. |
| status | PlanStatusEnum | No | Current status of the Plan. |
| activationInfo | MAL::String | No | ActivationInfo provides customisable detailed information on the result of the activation/deactivation request for the referenced Plan. |

SubPlanUpdate

SubPlanUpdate is a data structure that is used to report changes in status of a SubPlan during Plan Execution. It is returned in the context of the MPS Plan Execution Control service MonitorSubPlanExecution and GetSubPlanStatus operations.

Sub-plans are not defined as objects within the MPS model. Individual activities within a Plan may be associated with a single sub-plan via its Identifier. The Plan Execution function is responsible for managing and reporting sub-plan status associated with relevant Plan Execution Control service operations, if supported.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **SubPlanUpdate** | **Extends** | MAL::Composite | **SFP** | 13 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| subPlan | MAL::Identifier | No | Identifier of the SubPlan to which the update relates. |
| timestamp | MAL::Time | No | Time of status update. |
| status | SubPlanStatusEnum | No | Current status of the SubPlan, which may be Activated or Deactivated.. |

SubPlanStatusEnum

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **SubPlanStatusEnum** | **SFP** | 14 |

| Status | Value | Description |
| --- | --- | --- |
| ACTIVATED | 1 | The SubPlan is active. |
| DEACTIVATED | 2 | The SubPlan is not active. |

SubPlanActivationStatus

SubPlanActivationStatus is a data structure that returns the activation status of a SubPlan in the context of the MPS Plan Execution Control service ActivateSubPlan and DeactivateSubPlan operations.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanActivationStatus** | **Extends** | MAL::Composite | **SFP** | 15 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| plan | MAL::ObjectRef | No | Identifier of the SubPlan to which the status relates. |
| status | SubPlanStatusEnum | No | Current status of the SubPlan, which may be Activated or Deactivated. |
| activationInfo | MAL::String | No | ActivationInfo provides customisable detailed information on the result of the activation/deactivation request for the referenced SubPlan. |

PlanQuery

PlanQuery is a data structure used in the context of queryPlan operation of the MPS Plan Distribution Service. It is used to specify search criteria for querying the available set of Plans. All fields are nullable, in which case they do not apply as a search criteria.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanQuery** | **Extends** | MAL::Composite | **SFP** | 16 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| planID | MAL::ObjectID | Yes | Query for Plans with the specified PlanID. |
| hasPrecursor | MAL::Boolean | Yes | Query for Plans with or without a precursor. |
| isPatchPlan | MAL::Boolean | Yes | Query for Plans that are or are not Patch Plans |
| precursorPlan | MAL::ObjectRef | Yes | Query for Plans with the specified precursor Plan. |
| targetPlan | MAL::ObjectRef | Yes | Applicable only for Patch Plans. Query for Patch Plans that have the specified target Plan. |
| originator | MAL::Identifier | Yes | Query for Plans with the specified originator. |
| productionDate | TimeWindow | Yes | Query for Plans with a production date in the specified range. |
| validityPeriod | TimeWindow | Yes | Query for Plans with a validity period within (overlapping with) the specified range. |
| isAlternate | MAL::Boolean | Yes | Query for Plans that are or are not Alternate plans. |
| status | List <PlanStatusEnum> | Yes | Query for Plans that have a current status matching one of the specified list of Plan statuses. |
| containedEvents | List <MAL::ObjectRef> | Yes | Query for Plans that contain EventInstances whose definition matches one of the specified list of EventDefinitions. |
| containedActivities | List <MAL::ObjectRef> | Yes | Query for Plans that contain ActivityInstances whose definition matches one of the specified list of ActivityDefinitions. |

PartialPlan

A PartialPlan is a data structure returned from the getPartialPlan operation of the Plan Distribution Service that contains a reference to the source Plan, the criteria used to select the partial plan, and the partial plan itself. The partial plan uses the same structure as a normal Plan, with header fields matching those of the SourcePlan, but only containing the subset of ActivityInstances that matches the selection criteria. Whether EventInstances and Resources are included is implementation specific, but it might be assumed that any Events and Resources related to the selected ActivityInstances would be included in the returned partial plan.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PartialPlan** | **Extends** | MAL::Composite | **SFP** | 17 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| sourcePlan | MAL::ObjectRef | No | Reference to the Plan of which the partial plan is a selected subset. |
| domain | MAL::Identifier | Yes | Selection criterion based on the domain of contained ActivityInstances. |
| subPlan | MAL::Identifier | Yes | Selection criterion based on the subPlan of contained ActivityInstances. |
| tags | List <MAL::String> | Yes | Selection criterion based on tags associated with contained ActivityInstances |
| partialPlanStart | Trigger | Yes | Selection criterion indicating the start of a range of time, position or events associated with contained ActivityInstances. |
| partialPlanEnd | Trigger | Yes | Selection criterion indicating the end of a range of time, position or events associated with contained ActivityInstances. |
| partialPlan | Plan | No | The returned Partial Plan. |

PlanFilter

PlanFilter is a data structure used in the context of MPS Plan Distribution Service operations to specify a filtered set of Plans. All filter criteria specified are applied (logical AND, not OR).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PlanFilter** | **Extends** | MAL::Composite | **SFP** | 18 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| domain | MAL::Identifier | Yes | Domain of the Plan |
| planID | MAL::ObjectRef | Yes | ID (and Version) of the Plan |
| precursorPlan | MAL::ObjectRef | Yes | ID (and Version) of the precursor Plan |
| status | PlanStatusEnum | Yes | Current status (enum) of the Plan |
| originator | MAL::Identifier | Yes | Originator of the Plan |
| validityPeriod | TimeWindow | Yes | Period of time with which the validity period of the Plan overlaps. |

PartialPlanFilter

PartialPlanFilter is a data structure input to the getPartialPlan operation of the Plan Distribution Service that contains a reference to the source Plan, and specifies the criteria used to select the partial plan.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PartialPlanFilter** | **Extends** | MAL::Composite | **SFP** | 19 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| sourcePlan | MAL::ObjectRef | No | Reference to the Plan of which the partial plan is a selected subset. |
| domain | MAL::Identifier | Yes | Selection criterion based on the domain of contained ActivityInstances. |
| subPlan | MAL::Identifier | Yes | Selection criterion based on the subPlan of contained ActivityInstances. |
| tags | List <MAL::String> | Yes | Selection criterion based on tags associated with contained ActivityInstances |
| partialPlanStart | Trigger | Yes | Selection criterion indicating the start of a range of time, position or events associated with contained ActivityInstances. |
| partialPlanEnd | Trigger | Yes | Selection criterion indicating the end of a range of time, position or events associated with contained ActivityInstances. |

### Planning Configuration Data



Figure : Planning Configuration Data

Planning Configuration Data is the set of Identity and Definition objects that together define the set of available data items that can be referenced in planning requests and plans. This configuration data must be available to both communicating parties that exchange planning requests and plans. This includes the definitions for:

* Planning Activities
* Planning Events
* Planning Resources
* Planning Requests
* Functions

In addition to the above, the Planning Configuration Data includes MPS system wide configuration parameters, defined in a singleton MPSSystemConfig MO Object.

MPSSystemConfig

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **MPSSystemConfigDetails** | **Extends** | MAL::Composite | **SFP** | 401 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| version | MAL::Version | No | Version of MPS System Config |
| timeSystem | MAL::String | No | Specifies the time system used by the MPS system. |
| epoch | MAL::String | No | Specifies the epoch used by the MPS system. |
| customConfig | List <MAL::NamedValue> | Yes | Optional set of custom configuration parameters defined as a set of named values. |

### Functions [Optional]



Figure : Functions

Functions are an MPS ancillary data item that allow access to built-in Boolean functions of a planning system, for example in the context of planning constraints (see §3.3.6.1.6 Function Constraint). The function must be pre-defined to be referenced and the MPS Function Definition holds the declaration of an available function.

FunctionDefinitions include a set of ArgDefs that define the set of input arguments for the Function.

Similar to ActivityDetails, the FunctionDetails data type can be embedded in other items, such as a Function Constraint, that specify the invocation of a defined function. This references a FunctionDefinition and provides a set of ArgSpecs that specify the input value for each defined argument.

FunctionDefinition

FunctionDefinition is a data structure that contains static configuration data relating to built-in Boolean functions of an MPS system, each of which has a specified Identifier and optional set of argument definitions. This may change over time, each comprising a separate version of the definition. Function Definitions form part of the Planning Configuration Data.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **FunctionDefinitionDetails** | **Extends** | MAL::Composite | **SFP** | 501 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| functionID | MAL::Identifier | No | ID of the Function |
| version | MAL::Version | No | Version of the Function Definition. |
| description | MAL::String | No | Description of the Function. |
| argDefs | List <ArgDef> | Yes | List of Argument Definitions. |

FunctionDetails

Contains the information required to invoke a defined Function, including the specification of argument values.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **FunctionDetails** | **Extends** | MAL::Composite | **SFP** | 502 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| function | MAL::Identifier | No | ID of a specific Function Definition. |
| argSpecs | List <ArgSpec> | Yes | Set of Argument Specifications for each Argument Definition contained in the referenced Function Definition. These supply a value for each argument, or an expression to enable the value to be derived. |

## MPS Data Types

### MPS Base Data Types



Figure : MPS Base Data Types

The MPS information model is defined in terms of a set of base data types. As MPS services are defined as abstract services in terms of the MO service framework, these data types must also be compatible with the attribute types defined in the MO Message Abstraction Layer (MAL). The MAL attribute types (shown in Figure 27 above in purple) are as follows:

* Boolean
* Float *32-bit floating point number*
* Double *64-bit floating point number*
* Octet *8-bit signed integer*
* UOctet *8-bit unsigned integer*
* Short *16-bit signed integer*
* UShort *16-bit unsigned integer*
* Integer *32-bit signed integer*
* UInteger *32-bit unsigned integer*
* Long *64-bit signed integer*
* ULong *64-bit unsigned integer*
* Duration *Length of time in seconds (may include a fractional component)*
* Time *Absolute date and time to millisecond resolution*
* FineTime *Absolute date and time to picosend resolution*
* String *Text as a variable-length, unbounded, Unicode string*
* Blob *Used to store binary objects, it is a variable-length, unbounded, octet array*
* Identifier *Used to store Identifiers, it is a variable-length, unbounded, Unicode string*
* URI *Used to store URI addresses, it is a variable-length, unbounded, Unicode string*

It is also assumed that three additional MAL attribute types will become available in the next version of the MAL (shown in red):

* ObjectID *Unique Identifier for an MO Object*
* Version *Version number for an MO Object*
* ObjectRef *Reference to an MO Object (ID and version)*

The MAL also defines NamedValue as an extension of MAL::Composite that allows the specification of a name-value pair.

The MPS Information Model optionally extends this set of MAL attribute types with the following additional MAL composite data types:

* Position *Coordinates defining a physical location.*
* Direction *Coordinates defining a target pointing angle.*

A number of enumerations associated with the base data types are also defined:

MAL::AttributeType

MAL::AttributeType is defined in the MAL standard and allows specification of the type of a MAL Attribute.

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **MAL::AttributeType** | **SFP** | 0 |

| Status | Value | Description |
| --- | --- | --- |
| BLOB | 1 | Binary object |
| BOOLEAN | 2 | Boolean value (True or False) |
| DURATION | 3 | Length of time in seconds |
| FLOAT | 4 | Floating point number (32 bits) |
| DOUBLE | 5 | Double precision floating point number (64 bits) |
| IDENTIFIER | 6 | The Identifier structure is used to store an identifier and can be used for indexing. It is a variable-length, unbounded, Unicode string. |
| OCTET | 7 | Signed 8 bit Integer |
| UOCTET | 8 | Unsigned 8 bit Integer |
| SHORT | 9 | Signed 16 bit Integer |
| USHORT | 10 | Unsigned 16 bit Integer |
| INTEGER | 11 | Signed 32 bit Integer |
| UINTEGER | 12 | Unsigned 32 bit Integer |
| LONG | 13 | Signed 64 bit Integer |
| ULONG | 14 | Unsigned 64 bit Integer |
| STRING | 15 | Text. It is a variable length, unbounded, Unicode string. |
| TIME | 16 | Absolute date-time to millisecond resolution. |
| FINETIME | 17 | Absolute date-time to picosecond resolution. |
| URI | 18 | Uniform Resource Identifier (address). It is a variable-length, unbounded Unicode string. |
| OBJECTID | 19 | Object Identifier |
| OBJECTREF | 20 | Object Reference (Domain, ID and Version) |
| VERSION | 21 | Object Version |

ArgTypeEnum

ArgTypeEnum is an MPS extension of the above that also allows specification of the data type as Position or Direction.

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **ArgTypeEnum** | **SFP** | 1 |

| Status | Value | Description |
| --- | --- | --- |
| BLOB | 1 | Binary object |
| BOOLEAN | 2 | Boolean value (True or False) |
| DURATION | 3 | Length of time in seconds |
| FLOAT | 4 | Floating point number (32 bits) |
| DOUBLE | 5 | Double precision floating point number (64 bits) |
| IDENTIFIER | 6 | The Identifier structure is used to store an identifier and can be used for indexing. It is a variable-length, unbounded, Unicode string. |
| OCTET | 7 | Signed 8 bit Integer |
| UOCTET | 8 | Unsigned 8 bit Integer |
| SHORT | 9 | Signed 16 bit Integer |
| USHORT | 10 | Unsigned 16 bit Integer |
| INTEGER | 11 | Signed 32 bit Integer |
| UINTEGER | 12 | Unsigned 32 bit Integer |
| LONG | 13 | Signed 64 bit Integer |
| ULONG | 14 | Unsigned 64 bit Integer |
| STRING | 15 | Text. It is a variable length, unbounded, Unicode string. |
| TIME | 16 | Absolute date-time to millisecond resolution. |
| FINETIME | 17 | Absolute date-time to picosecond resolution. |
| URI | 18 | Uniform Resource Identifier (address). It is a variable-length, unbounded Unicode string. |
| OBJECTID | 19 | Object Identifier |
| OBJECTREF | 20 | Object Reference (Domain, ID and Version) |
| VERSION | 21 | Object Version |
| DIRECTION | 129 | MPS Direction |
| POSITION | 130 | MPS Position |

TimeReferenceEnum

TimeReference is an MPS enumeration that allows specification the Time reference used as the default for all Time attributes within an MPS system. The set of Time references is currently TBD.

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **TimeReferenceEnum** | **SFP** | 2 |

| Enumeration | Value | Description |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### MPS Position and Direction Data Types [Optional]

This section defines MPS Position and Direction data types and support types required in the definition of pointing constraints. These are consistent with those used within CCSDS Navigation data format standards, and specifically the Pointing Request Message (PRM) [PRM], but for MPS, to enable use of the MO Framework, they are defined explicitly in terms of MAL Attributes.

MPS Position and Direction data types are only required in the context of the following MPS data structures:

* Geometric Constraints (see §3.3.6.1.7)
* Triggers of type PositionTrigger and PointingTrigger (see §3.3.7)
* Repetitions of type PositionRepetition and PointingRepetition (see 3.3.8)

As all of these are considered optional elements of the MPS Information Model, MPS Position and Direction Data Types are themselves optional.

#### Position Data Type



Figure : Position Data Type

The Position data type is used to specify a physical location.

The Position type is defined in [PRM] §3.3.2.11 (where it is called the “Orbit Entity” type). Only the Ephemeris object and Orbit file representations are supported in PRM template parameters and as such in Pointing Constraint attributes.

For MPS it is possible to define a Position using one of the following coordinate types:

* **Cartesian**: a set of explicitly provided x,y and z coordinates.
* **Orbit**: a reference to a file containing a CCSDS Orbit Data Message [ODM] defining the orbital ephemeris.
* **Object**: a reference to a named target object.

The coordinate type attributes (Cartesian, Orbit and Object) are optional and only one should be present, consistent with the PositionType.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **Position** | **Extends** | MAL::Composite | **SFP** | 3 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| ref | MAL::String | No | Name of a reusable Position definition. If provided, the other Position attributes will be ignored. |
| positionType | PositionTypeEnum | No | Enumeration: one of {Cartesian, Orbit, Object} indicating the type of coordinates used. |
| cartesian | **C**artesianCoords | Yes | Mandatory for PositionType “Cartesian”. |
| orbit | OrbitalCoords | Yes | Mandatory for PositionType “Orbit”. |
| object | MAL::String | Yes | Mandatory for PositionType “Object”.  Name or identifier of an ephemeris object (see [PRM] reference #7) or a mission specific object. |
| frame | MAL::String | Yes | Mandatory for PositionType “Cartesian”. The coordinate frame name, as defined in [PRM] annex B2, or a mission specific frame. |
| units | MAL::String | Yes | Only applicable for PositionType “Cartesian”, ignored for other coordinate types. The distance unit name, as defined in [PRM] annex D.  Default = “km”. |

PositionTypeEnum

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **PositionTypeEnum** | **SFP** | 4 |

| Status | Value | Description |
| --- | --- | --- |
| CARTESIAN | 1 | Position defined using Cartesian Coordinates |
| ORBIT | 2 | Position defined in terms of Orbital Coordinates |
| OBJECT | 3 | Position defined in terms of a named object |

CartesianCoords

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **CartesianCoords** | **Extends** | MAL::Composite | **SFP** | 5 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| x | MAL::Double | No | Cartesian x coordinate defined in the given Frame and with values of the given Unit. |
| y | MAL::Double | No | Cartesian y coordinate defined in the given Frame and with values of the given Unit. |
| z | MAL::Double | No | Cartesian z coordinate defined in the given Frame and with values of the given Unit. |

OrbitalCoords

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **OrbitalCoords** | **Extends** | MAL::Composite | **SFP** | 6 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| orbitFile | MAL::String | No | Name of or reference to a file containing an Orbit Data Message [ODM]. |

#### Direction Data Type



Figure : Direction Data Type

The Direction data type is used to specify a pointing direction or attitude.

The Direction type is defined in [PRM] §3.3.2.9. Only the Coordinates representation is supported in PRM template parameters and as such in Pointing Constraint attributes.

A direction is either defined in the base frame (e.g. an inertial frame) and any sub-frame of the base frame, or in a secondary frame (i.e. the pointing frame, e.g. a spacecraft frame) or any sub-frame of the secondary frame (e.g. an instrument boresight).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **Direction** | **Extends** | MAL::Composite | **SFP** | 7 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| ref | MAL::String | Yes | Name of a reusable Direction definition. If provided, the other Direction attributes will be ignored. |
| directionType | DirectionTypeEnum | No | Enumeration: one of {Cartesian, Spherical, RADec, NamedTarget} indicating the type of coordinates used. |
| cartesian | **C**artesianCoords | Yes | Mandatory for DirectionType “Cartesian”. Dimensionless unit vector. Either a direction in the base frame or in a secondary frame may be defined. |
| spherical | SphericalCoords | Yes | Mandatory for DirectionType “Spherical”. The unit may be defined here. Typically used to define a direction in a secondary frame. When used to specify a surface coordinate, this actually represents a {longitude, latitude} pair |
| raDec | RADecCoords | Yes | Mandatory for DirectionType “RADec”. The unit may be defined. |
| namedTarget | MAL::String | Yes | Mandatory for DirectionType “NamedTarget”.  Name or identifier of a catalogued celestial object or a mission specific object. |
| frame | MAL::String | No | Mandatory for all DirectionTypes. The coordinate frame name, as defined in [PRM] annex B2, or a mission specific frame. |
| units | MAL::String | Yes | Only applicable for DirectionType “Spherical” and “RADec”, ignored for other coordinate types. To be one of the Angle units as defined in [PRM] annex D.  Default = “deg”. |

For MPS it is possible to define a Direction using one of the following coordinate types:

* **Cartesian**: a set of explicitly provided x,y and z coordinates.
* **Spherical**: a pair of coordinates corresponding to Azimuth and Elevation.
* **RADec**: a pair of coordinates typically used for astronomical observations corresponding to Right Ascension and Declination.
* **NamedTarget**: a reference to a named target object.

The coordinate type attributes (Cartesian, Spherical, RADec and NamedTarget) are optional and only one should be present, consistent with the DirectionType. Note that the data structure for CartesianCoords is the same as that defined under Position Data Type above.

DirectionTypeEnum

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **DirectionTypeEnum** | **SFP** | 8 |

| Status | Value | Description |
| --- | --- | --- |
| CARTESIAN | 1 | Direction defined using Cartesian Coordinates |
| SPHERICAL | 2 | Direction defined using Spherical Coordinates |
| RADEC | 3 | Direction defined using Right Ascension and Declination |
| NAMEDTARGET | 4 | Direction defined by a named Target |

SphericalCoords

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **SphericalCoords** | **Extends** | MAL::Composite | **SFP** | 9 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| azimuth | MAL::Double | No | Angular coordinate. May also represent Longitude. |
| elevation | MAL::Double | No | Angular coordinate. May also represent Latitude. |

RADecCoords

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RADecCoords** | **Extends** | MAL::Composite | **SFP** | 10 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| ra | MAL::Double | No | Right Ascension: Celestial angular coordinate, measured eastward along the celestial equator. |
| dec | MAL::Double | No | Declination: Celestial angular coordinate, north or south of the celestial equator. |

#### Physical Value Data Types



Figure : Physical Value Data Types

Physical Value is an abstract base type for the specific value types defined below. Only specific value types are used in the Pointing Constraint definitions below.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***PhysicalValue*** | **Extends** | MAL::Composite | **SFP** | Abstract |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| value | MAL::Double | No | Physical value. |
| units | MAL::String | Yes | Optional unit. The unit type depends on the specific value type, as defined in [PRM] annex D. |

For MPS, three specific physical value types (as defined in [PRM] annex D) are used in the context of geometric constraints on position or pointing:

Angle: has units of type Angle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **Angle** | **Extends** | *PhysicalValue* | **SFP** | 11 |

AngularVelocity: has units of type AngularVelocity

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **AngularVelocity** | **Extends** | *PhysicalValue* | **SFP** | 12 |

Distance: has units of type Distance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **Distance** | **Extends** | *PhysicalValue* | **SFP** | 13 |

### Expressions



Figure : MPS Expression Types

When entering MPS data, it is often not possible to provide an absolute value for a required attribute. Instead, it is necessary to provide a calculation to be performed at run time that supplies the value. These calculations are defined as expressions of a specified data type. The data type can be any defined ArgType [see §3.3.1], which may be any MAL Attribute type, Position or Direction.

Within the MPS Information Model, derived sub-types of Expression are used to constrain the result of an expression is of a specific data type. These are shown in grey in Figure 31. The attribute set for all types of expression is the same as that of the base class.

The expressions are themselves text strings which comprise a sequence of operands and operators. Operands may be literals or references to objects and their attributes or arguments, as defined within the MPS information model.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **Expression** | **Extends** | MAL::Composite | **SFP** | 14 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| type | ArgTypeEnum | No | Enumeration specifying the data type of the result of the expression. |
| value | MAL::Attribute | No | Providing the ArgType is a MAL Attribute type, this field may be used to hold a simple literal value or the evaluated result of the expression. |
| expressionLanguage | MAL::String | No | Defines the expression language used to specify the expression. |
| expression | MAL::String | No | The text of the expression. |

The Value that the expression provides may be specified in three ways:

* As a literal Value of the appropriate type (in the Value field)
* As a simple Reference to an argument or attribute of an MO Object, or to an MO Object itself, of the appropriate data type (in the Expression field). The referenced item contains the Value at run-time.
* As an Expression comprising multiple operands (specified as literals or references as above) together with appropriate arithmetic, logical or other operators (in the Expression field). Evaluation of the expression at run-time delivers a Value result of the appropriate data type.

As there is no equivalent MAL::Attribute type for Position or Direction, values of these types are represented as a MAL::String containing a literal in the defined expression format for these types.

References and Expressions are provided as a text string in the Expression attribute. The expression language itself is not specified as part of the standard. However, there are specific requirements which must be fulfilled in the following areas:

* Formats for the representation of literal values of all data types
* Object References
* Time and Duration Expressions

If there is no native language for the specification of expressions in the target deployment, then it is suggested that one could be defined based on the XPath syntax [D10].

The Expression Language attribute is used to specify which syntax is used in the Expression attribute. It is itself a string rather than an enum to allow extensibility and the use of user defined expression languages. There must be a service agreement between Service Provider and Service User on the language(s) to be used.

SFPs are reserved for expression subtypes as follows (although the data structure is identical):

* Object Expression – SFP 15
* Position Expression – SFP 16
* Direction Expression – SFP 17
* Duration Expression – SFP 18
* Time Expression – SFP 19
* Boolean Expression – SFP 20
* Integer Expression – SFP 21
* Real Expression – SFP 22

#### Object References

The syntax for Object References must support the following:

* References to planning events, planning activities, planning requests and planning resources
* References to any attribute of planning events, planning activities, planning requests and planning resources
* References to any argument (by name) of planning events, planning activities and planning requests

References may be via:

* Name (ObjectID)
* The current object (by context) "Me"
* An Object referenced in an argument or attribute of another Object
* A Child Object of another Object by Name
* A Sibling Object (another child of the parent [source] object) by Name

Note that Child and Sibling relationships apply only to planning events and planning activities.

Note that Name identifies a Planning Resource explicitly, but only the Definition class of Planning Activities and Planning Events. These references must be resolvable at run time to a specific Instance, based on context.

#### Time and Duration Expressions

The syntax for Time (T) and Duration (D) expressions must support the following constructs, which may include a Numeric (N) value or reference:

T = T±D add or subtract a Duration to/from a Time to give another Time.

D = Ta-Tb subtract two Times to give a Duration

D = Da±Db add or subtract two Durations to give another Duration

D = D\*/N multiply or divide a Duration by a numeric factor to give another Duration. Note this may substitute for a simple duration in the previous cases, for example T = T±D\*/N.

### Additional MPS Data Types



Figure : MPS Additional Data Types

These correspond to structures used repeatedly within the MPS Information Model.

Slider

Used to indicate a relative position with respect to an MPS object, such as a planning activity where 0 represents the start and 1 the end of the activity. The slider is a real number that can represent any point between these two extremes.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **Slider** | **Extends** | MAL::Composite | **SFP** | 23 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| position | MAL::Float | No | Relative point between the start and end of an MPS object, where 0 represents the start and 1 represents the end. |

A slider **s** is a floating point value. It converts the *startTime* and *endTime* of an Activity Instance into a *referenceTime*:

*referenceTime* = *startTime* + **s** \* (*endTime* - *startTime*)

Sliders are often associated with an offset. An offset **o** is a duration. It converts a referenceTime into an applicableTime:

*applicableTime* = *referenceTime* + **o**

StateDef

Status values may be represented as enumerated Integers, but the enumeration is not defined by the standard, but in the context of Planning Configuration data. StateDefs hold the definitions of the text labels associated with specific status values.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **StateDef** | **Extends** | MAL::Composite | **SFP** | 24 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| value | MAL::Integer | No | Enumerated value of the Status |
| state | MAL::String | No | Text label associated with the enumerated value. |

TimeWindow

Represents a specific period of time, specified as two Expressions of type Time defining the Start and End of the TimeWindow.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **TimeWindow** | **Extends** | MAL::Composite | **SFP** | 25 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| start | TimeExpression | No | Start time of the Time Window. |
| end | TimeExpression | No | End time of the Time Window. |

EventWindow

Represents a specific period relative to two events that mark the start and end of the EventWindow.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **EventWindow** | **Extends** | MAL::Composite | **SFP** | 26 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| startEvent | ObjectExpression | No | The start of the Event Window is relative to the referenced StartEvent. |
| startOffset | DurationExpression | No | The start of the Event Window is offset by the defined time period from the StartEvent. |
| endEvent | ObjectExpression | No | The end of the Event Window is relative to the referenced EndEvent. |
| endOffset | DurationExpression | No | The end of the Event Window is offset by the defined time period from the EndEvent. |

DefListEntry

Used in the context of the MPS Plan Information Management service, this holds a list of definitions for a specified type of MPS Data Item, together with their definitions.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **DefListEntry** | **Extends** | MAL::Composite | **SFP** | 27 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| definitionID | MAL::ObjectRef | No | Item Definition ID and Version |
| description | MAL::String | No | Description of the Item |

### Arguments



Figure : Arguments

Arguments are a common feature for MPS Data Items that follow the MO Instance Object pattern described in §3.4.3.3 below. This includes planning events, planning activities and planning requests that have both definitions and instances.

A mission-specific set of arguments may be associated with each defined planning event, planning activity or planning request. These hold additional information specific to the defined data item and can be used to parameterise the data item. Each argument has an identifying ArgName and an associated value of any defined ArgType (see §3.3.1) and may correspond to an array of values.

Arguments are not themselves MO objects, but are contained within them, and follow a similar pattern to the MO Instance Object, comprising definitions, instances and details.

ArgDef

The definition of an argument is an ArgDef, a set of which may be contained within the definition MO object of a planning event, planning activity or planning request. This defines the name and data type of the argument. Depending on the data type, the ArgDef may require additional type specific attributes to support data validation.  SubTypes are identified for Numeric, String and Status arguments.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ArgDef** | **Extends** | MAL::Composite | **SFP** | 28 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| argName | MAL::Identifier | No | Name of the argument |
| description | MAL::String | No | Extended description of the argument |
| argType | ArgTypeEnum | No | Enumeration specifying the data type of the argument. |
| argUnits | MAL::String | No | Units that the argument value is expressed in. |
| isArray | MAL::Boolean | No | If True, indicates that the argument is an array of values of type ArgType. |

NumericArgDef

Extended sub-type of ArgDef that provides additional attributes to support data validation for numeric data types.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **NumericArgDef** | **Extends** | ArgDef | **SFP** | 29 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| min | MAL::Double | No | Minimum value of the argument |
| max | MAL::Double | No | Maximum value of the argument |
| precision | MAL::Short | No | Precision of the argument. |

StringArgDef

Extended sub-type of ArgDef that provides additional attributes to support data validation for the string data type.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **StringArgDef** | **Extends** | ArgDef | **SFP** | 30 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| maxLength | MAL::Integer | No | Maximum length of the string (characters). |
| regex | MAL::String | No | A “regular expression” or sequence of characters defining a character pattern that the string value must match. |

StatusArgDef

Extended sub-type of ArgDef that provides additional attributes to support data validation and interpretation for integer type arguments that are effectively enumerated Statuses.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **StatusArgDef** | **Extends** | ArgDef | **SFP** | 31 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| allowedValues | List <StateDef> | No | Set of allowed State definitions (see §3.3.4), comprising the enumerated value and an associated text label. |

Argument

The instance of an argument is an Argument, a set of which may be contained within the instance MO object of a planning event or planning activity or within a planning request. This comprises the name and value of the argument, corresponding to the set of arguments defined in the ArgDef. Argument values are represented as a MAL Attribute of appropriate data type. As there is no equivalent MAL::Attribute type for Position or Direction, values of these types are represented as a MAL::String containing a literal in the defined expression format for these types.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **Argument** | **Extends** | MAL::Composite | **SFP** | 32 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| argName | MAL::Identifier | No | Name of the argument |
| count | MAL::Integer | Yes | If argument is an array, count of the number of elements in the array. |
| argValue | List <MAL::Attribute> | No | Argument value (or values if it is an array). MAL Attribute type must match the ArgType of the ArgDef. Position and Direction values are represented as a MAL::String. |

ArgSpec

In the case of the planning activity, there is also an ArgSpec, a set of which may be contained within the Activity Details structure embedded within a planning request or parent planning activity definition. The ArgSpec defines how to derive the value of an Argument when instantiating it at run-time. The ArgSpec attribute is an Expression, the result of which must be a value matching the defined ArgType.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ArgSpec** | **Extends** | MAL::Composite | **SFP** | 33 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| argName | MAL::Identifier | No | Name of the argument |
| count | MAL::Integer | Yes | If argument is an array, count of the number of elements in the array. |
| argValue | Expression | No | Expression that can be evaluated at run-time to provide argument value(s) of appropriate data type. |

### Constraints



Figure : Planning Constraints

Planning Constraints describe the relationships between planning activities and other entities represented in the MPS Information Model, including:

* Time, Position and pointing Direction
* Planning events
* Planning resources
* Other planning activities

Planning constraints are not free-standing MO objects within the model, but are attached to either planning requests or planning activities.

There are two main sub-types of Planning Constraint: Conditional Constraints and Effects.

Conditional Constraints specify conditions that must be satisfied when placing a planning activity within a plan.

Effects specify the impact that executing a planning activity will have on planning resources. These may be used to predict the evolution of the values of planning resources over the period of a plan. This in turn enables the verification that sufficient resource is available for execution of the plan and that all explicit resource constraints are satisfied. As for Resources, Effects are an optional element of the MPS information model.

Conditional Constraints and Effects are detailed in the following subsections.

*Constraint*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***Constraint*** | **Extends** | MAL::Composite | **SFP** | Abstract |

ConstraintNode

Multiple Planning Constraints can be combined using a Constraint Node. The Constraint Node specifies the logical operation (AND or OR) to be used when combining a set of Constraints together. As the Constraint Node is itself defined as a sub-type of Constraint, it is possible to construct a tree of Constraint Nodes using different logical operators.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ConstraintNode** | **Extends** | *Constraint* | **SFP** | 34 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| operator | LogicOpenum | No | Enumeration specifying the logic for combining multiple Boolean conditions together. One of {AND, OR}.  Default = AND |
| negate | MAL::Boolean | No | Specifies whether the result of combining the Constraints is to be inverted (NOT function).  Default = False |
| constraints | List <Constraint> | No | The set of Constraints to be combined. |

LogicOpEnum

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **LogicOpEnum** | **SFP** | 35 |

| Enumeration | Value | Description |
| --- | --- | --- |
| AND | 1 | Logical AND |
| OR | 2 | Logical OR |

#### Conditional Constraints



Figure : Conditional Constraints

A wide range of conditional constraint sub-types are defined to support different classes of condition. These are shown in Figure 35 above, except for geometric constraints which are shown in Figure 36.

Each of the following sub-types of conditional constraint is described in a separate sub-section below:

* Constraint Expression (a Boolean expression that evaluates to True if the constraint is met)
* Temporal Constraints (when a planning activity can be planned)
* Sequential Constraints (which order planning activities must be executed in)
* Exclusion Constraints (identifying planning activities that cannot be executed concurrently)
* Resource Constraints (restrictions based on the value of planning resources)
* Argument Constraints (restrictions based on the value of an argument)
* Function Constraints (restrictions based on the result of a function)
* Geometric Constraints (restrictions based on position or pointing direction).

Of these, only the Constraint Expression is required to be supported for compliance of an MPS system to the MPS services standard. All other conditional constraint types are optional.

Where a constraint is associated with a planning activity, this may be by reference to an ActivityDefinition, in which case it applies to all instances of that definition, or to a specific ActivityInstance, in which case it only applies to that instance.

*Conditional Constraint*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***ConditionalConstraint*** | **Extends** | *Constraint* | **SFP** | Abstract |

##### Constraint Expression

All types of constraint can be considered conditions that are either met or not met when a planning activity is placed in a plan. They can therefore be specified as a potentially complex Boolean expression that combines references to the arguments and attributes of objects in the MPS Information Model using operators of various types (arithmetic, comparative, logical, string, temporal and geometric). The expression must evaluate to TRUE for the constraint to be met.

As introduced in §3.3.3, this standard does not define a full expression language capable of supporting such complex Boolean expressions. It does, however, support the use of externally defined expression languages. The ConstraintExpression type allows for the use of such an expression language to define any type of constraint, providing communicating entities all have the capability to evaluate that expression language.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ConstraintExpression** | **Extends** | *ConditionalConstraint* | **SFP** | 36 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| constraint | BooleanExpression | No | Potentially complex conditional expression that must evaluate to TRUE for the constraint to be met. |

##### Temporal Constraints [Optional]

Temporal constraints impose a restriction on when a planning activity can appear in a plan. The abstract type *TemporalConstraint* identifies the planning activity that is subject to the constraint, while concrete sub-types allow the specification of three different types of temporal constraint:

* Time Constraint: the time at which the planning activity is to be planned
* Time Window Constraint: a time window within which the planning activity is to be planned
* Duration Constraint: a restriction on the duration of the planning activity in the plan

*TemporalConstraint*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***TemporalConstraint*** | **Extends** | *ConditionalConstraint* | **SFP** | Abstract |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| activityRef | ObjectExpression | No | Identifies the constrained planning activity |

This attribute is common to all sub-types.

TimeConstraint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **TimeConstraint** | **Extends** | *TemporalConstraint* | **SFP** | 37 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| time | TimeExpression | No | The Time at which the planning activity must be planned. |
| timeRef | Slider | No | The point in the duration of the planning activity that is time constrained. 0: the start of the planning activity 1: the end of the planning activity |

The use of a Time Expression allows the time constraint to be specified in terms of a planning event or an argument of a planning request or planning activity.

The Slider construct (see §3.3.4) may be used to express any point in the duration of the planning activity between its start (0) and end (1) that is constrained to the specified Time.

TimeWindowConstraint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **TimeWindowConstraint** | **Extends** | *TemporalConstraint* | **SFP** | 38 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| startRef | Slider | No | The point in the duration of the Activity that is constrained to be after the start time of the Time Window. Although typically the start of the Activity (0), this can be any point up to the end of the Activity (1). |
| endRef | Slider | No | The point in the duration of the Activity that is constrained to be before the end time of the Time Window. Although typically the end of the Activity (1), this can be any point up to the start of the Activity (0). |
| timeWindows | List <TimeWindow> | No | The [set of] TimeWindows within which the Activity must be placed on the Plan. |

The use of the Sliders to specify the start and end time references for the planning activity with respect to the specified TimeWindow[s] allows a range of overlap conditions to be expressed, for example:

* StartRef = Start[0] and EndRef = End[1] means that the planning activity must be fully contained within the specified TimeWindow.
* StartRef = Start[0] and EndRef = Start[0] means that the planning activity must start within the specified TimeWindow, but can continue beyond the end of the TimeWindow.
* StartRef = End[1] and EndRef = Start[0] means that the planning activity can overlap both the start and end of the TimeWindow.

Multiple TimeWindows can be specified. This indicates that the planning activity may be placed within any of the specified TimeWindows, not that it should be placed multiple times.

DurationConstraint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **DurationConstraint** | **Extends** | *TemporalConstraint* | **SFP** | 39 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| minDuration | DurationExpression | No | Specifies the minimum duration of the planning activity |
| maxDuration | DurationExpression | No | Specifies the maximum duration of the planning activity |

##### Sequential Constraint [Optional]

Sequential constraints impose a restriction on the order of planning activities in a plan with respect to both other planning activities and planning events.

Two objects are identified: the Predecessor which must be followed in the plan by the Successor. While either the Predecessor or Successor may be a planning event, it is not possible to specify a sequential constraint between two planning events: one or both must be a planning activity.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **SequentialConstraint** | **Extends** | *ConditionalConstraint* | **SFP** | 40 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| predecessor | ObjectExpression | No | Identifies the planning activity or planning event that must occur first on the plan. |
| successor | ObjectExpression | No | Identifies the planning activity or planning event that must follow the predecessor on the plan. |
| predecessorRef | Slider | No | Point on the Predecessor that must be followed by the Successor |
| successorRef | Slider | No | Point on the Successor that must follow the Predecessor |
| minOffset | DurationExpression | No | Minimum period between the specified points on the Predecessor and Successor. |
| maxOffset | DurationExpression | No | Maximum period between the specified points on the Predecessor and Successor. |

As with the Time Window Constraint, the Slider construct is used to specify the point on the duration of the Predecessor object that the specified point on the Successor object is constrained to follow. This allows various overlap conditions to be expressed. For example, if the Start of the Successor must follow the End of the Predecessor, then the PredecessorRef is End[1] and the SuccessorRef is Start[0].

The constraint may also specify an offset, or interval, between the Predecessor and Successor objects. This is expressed as a minimum and maximum duration between the specified points on the Predecessor and Successor objects.

##### Exclusion Constraint [Optional]

An Exclusion constraint specifies a set of 2 or more planning activities or planning events that cannot occur concurrently in a Plan. As only planning activities can be excluded, at least one of the set must be a planning activity. Excluded objects are specified by definition [class] rather than instance, the exclusion applying to all instances of the class. Exclusion implies no overlap between the excluded items.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ExclusionConstraint** | **Extends** | *ConditionalConstraint* | **SFP** | 41 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| classRef | List <MAL::ObjectRef> | No | Specifies the definition (class) of excluded planning activities and planning events. |

##### Resource and Argument Constraints [Optional]

Resource and Argument Constraints allow the value of a Resource or an Argument (of any MAL::Attribute type) to be compared against a specified value.

Note that all MAL Attribute data types can be supported by a single subtype that has the Value attribute of type MAL Attribute. Argument Constraints cannot be used for Arguments of type Position or Direction as the values are not MAL::Attributes.

ArgumentConstraint

An Argument Constraint may be associated with a planning activity to restrict when it can be planned, based on the value of an argument of the planning activity itself or a related planning event.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ArgumentConstraint** | **Extends** | *ConditionalConstraint* | **SFP** | 42 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| activityRef | ObjectExpression | No | Identifies the planning activity for which the Argument Constraint applies. |
| objectRef | ObjectExpression | No | Identifies the Object (planning activity or planning event) whose argument is to be referenced. |
| argName | MAL::Identifier | No | Identifies the specific argument of the referenced Object whose value is to be compared |
| comparator | ExpressionOperatorEnum | No | Comparisson Operator, which may be one of:  =, !=, >, >=, <, <=, contains, icontains  The contains operator only applies to Strings and may be case sensitive or insensitive. |
| value | MAL::Attribute | No | Value (of same type as the referenced Argument) to be compared against. |

ExpressionOperatorEnum

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **ExpressionOperatorEnum** | **SFP** | 43 |

| Enumeration | Value | Description |
| --- | --- | --- |
| EQUAL | 1 | = |
| DIFFER | 2 | != |
| GREATER | 3 | > |
| GREATER\_OR\_EQUAL | 4 | >= |
| LESS | 5 | < |
| LESS\_OR\_EQUAL | 6 | <= |
| CONTAINS | 7 | Case sensitive containment (Strings only) |
| ICONTAINS | 8 | Case insensitive containment (Strings only) |

ResourceConstraint

The [simple] Resource Constraint must be satisfied for the duration of the referenced planning activity.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ResourceConstraint** | **Extends** | *ConditionalConstraint* | **SFP** | 44 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| activityRef | ObjectExpression | No | Identifies the planning activity for which the Resource Constraint applies. |
| resourceRef | MAL::ObjectRef | No | Identifies the planning resource that is constrained for the duration of the planning activity. |
| comparator | ExpressionOperatorEnum | No | COM Comparisson Operator, which may be one of:  =, !=, >, >=, <, <=, contains, icontains  The contains operator only applies to Strings and may be case sensitive or insensitive. |
| value | MAL::Attribute | No | Value (of same type as the referenced Resource) to be compared against. |

ComplexResourceConstraint

In the [simple] Resource Constraint, the value of the referenced planning resource is constrained against a single value for the entire duration of the referenced planning activity.

With the Complex Resource Constraint, the period over which the constraint applies can be customised relative to the referenced planning activity; and the value against which the referenced planning resource is constrained can be specified as a Relative Resource Profile which evolves over time.

The attributes of the Complex Resource Constraint extend or modify those of the [simple] Resource Constraint as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ComplexResourceConstraint** | **Extends** | ResourceConstraint | **SFP** | 45 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| startRef | Slider | No | Identifies the point in the duration of the referenced planning activity to which the start of the constraint period relates. |
| endRef | Slider | No | Identifies the point in the duration of the referenced planning activity to which the end of the constraint period relates. |
| startOffset | DurationExpression | No | Offset from StartRef that specifies the start of the constraint period. |
| endOffset | DurationExpression | No | Offset from EndRef that specifies the end of the constraint period. |
| value | RelResourceProfile {redefines Value} | No | Resource Profile specifying an evolving value over time against which the value of the planning resource is to be compared.  See §3.2.4.2 |

The period over which the Resource Constraint applies is specified as StartRef+StartOffset to EndRef+EndOffset.

##### Function Constraint [Optional]

Function Constraints make use of an external function to determine whether or not a constraint is satisfied. Available functions must be pre-defined (see §3.2.8) to allow them to be referenced in a Function Constraint.

As for Complex Resource Constraints, the period over which the Function Constraint applies is specified relative to the referenced planning activity.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **FunctionConstraint** | **Extends** | *ConditionalConstraint* | **SFP** | 46 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| activityRef | ObjectExpression | No | Identifies the planning activity for which the Function Constraint applies. |
| startRef | Slider | No | Identifies the point in the duration of the referenced planning activity to which the start of the constraint period relates. |
| endRef | Slider | No | Identifies the point in the duration of the referenced planning activity to which the end of the constraint period relates. |
| startOffset | DurationExpression | No | Offset from StartRef that specifies the start of the constraint period. |
| endOffset | DurationExpression | No | Offset from EndRef that specifies the end of the constraint period. |
| function | FunctionDetails | No | Specifies the Function to be applied and its set of input arguments. |

##### Geometric Constraints [Optional]



Figure : Geometric Constraints

Geometric Constraints impose a restriction on a planning activity appearing in a plan, based on the position or pointing direction of a physical object, such as a spacecraft or instrument.

The abstract type *Geometric Constraint* identifies the planning activity that is subject to the constraint, and the period over which the constraint is applicable, relative to the start and end of that planning activity. Concrete sub-types allow the specification of different types of geometric constraint:

* Position Constraint: expressed in terms of a specified Position and a tolerance. Different sub-types support the specification of Position using different coordinate systems.
* Pointing Constraint: expressed in terms of the pointing templates defined for use within CCSDS Navigation data format standards.
* Revolution Constraint: expressed in terms of revolution angle and a tolerance.
* Distance Constraint: expressed in terms of the distance between Observer and Target objects.
* Angle Constraint: expressed in terms of the angle subtended by three objects.

*GeometricConstraint*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***GeometricConstraint*** | **Extends** | *ConditionalConstraint* | **SFP** | Abstract |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| activityRef | ObjectExpression | No | Identifies the planning activity for which the Geometric Constraint applies. |
| startRef | Slider | No | Identifies the point in the duration of the referenced planning activity to which the start of the constraint period relates. |
| endRef | Slider | No | Identifies the point in the duration of the referenced planning activity to which the end of the constraint period relates. |
| startOffset | Duration Expression | No | Offset from StartRef that specifies the start of the constraint period. |
| endOffset | Duration Expression | No | Offset from EndRef that specifies the end of the constraint period. |

These attributes are common to all sub-types of Geometric Constraint (including Pointing Constraints).

The period over which the Geometric Constraint applies is specified relative to the referenced planning activity as StartRef+StartOffset to EndRef+EndOffset.

*LocationConstraint*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***LocationConstraint*** | **Extends** | *GeometricConstraint* | **SFP** | Abstract |

Location constraints are expressed in terms of a specified Position and a tolerance. Concrete sub-types are defined to support positions expressed using different co-ordinate systems.

PositionConstraint

A concrete sub-type of Position Constraint that can be used to specify the constraint in terms of a tolerance sphere around the specified position, expressed as a distance. Note that the position itself can be expressed as

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PositionConstraint** | **Extends** | *LocationConstraint* | **SFP** | 47 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| position | PositionExpression | No | Specifies the required position expressed as cartesian co-ordinates, orbital co-ordinates, or a named target. |
| tolerance | RealExpression | No | Specifies the maximum distance from the required position that satisfies the constraint, effectively defining a sphere around the required position. |
| units | MAL::String | Yes | Optional. The tolerance unit name, as defined in [PRM] annex D.  Default = “km”. |

OrbitalPositionConstraint

A concrete sub-type of Position Constraint that can be used to specify a range of orbital positions, expressed in terms of orbit number and orbit angle. This is particularly relevant for earth observation satellites with a repetitive ground track and on-board position based scheduler.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **OrbitalPositionConstraint** | **Extends** | *LocationConstraint* | **SFP** | 48 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| orbitNumber | IntegerExpression | No | Orbit Number. Depending on the RelativeOrbit flag, the Orbit Number may be absolute (since start of mission) or relative (to the orbital repeat cycle). |
| relativeOrbit | MAL::Boolean | No | Flag indicating if the Orbit Number is absolute or relative to the orbital repeat cycle. |
| orbitAngle | RealExpression | No | Specifies the required Angle within orbit |
| tolerance | RealExpression | No | Specifies a tolerance in the required Angle within orbit, effectively defining a range of orbit angles: orbitAngle±tolerance. |
| units | List <MAL::String> | Yes | Optional. The angular unit name, as defined in [PRM] annex D.  Default = “deg”. |

PointingConstraint

Pointing Constraints impose a restriction on a planning activity appearing in a plan, based on the pointing direction of a physical object, such as a spacecraft or instrument.

As with the Direction data types [see §3.3.2.2], Pointing Constraints are consistent with the pointing templates defined for use within CCSDS Navigation data format standards, and specifically the Pointing Request Message (PRM) [D7]. PointingConstraint is a concrete sub-type of *Geometric Constraint* that includes attributes common to all pointing templates. The pointing template itself is then identified as an attribute and any additional arguments applicable to the template are provided as a list of name-value pairs.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PointingConstraint** | **Extends** | *GeometricConstraint* | **SFP** | 49 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| pointingFrame | MAL::String | No | Optional. Frame to which the Pointing Constraint applies. Default frame is the spacecraft frame or any other mission specific default frame. |
| boresight | Direction | No | Direction in any spacecraft frame. |
| boresightMargin | Angle | No | Defines an optional cone region around the boresight, allowing a margin for application of the pointing constraint.  Default = 0.0 |
| phaseAngleMargin | Angle | No | Defines an optional rotation around the boresight, w.r.t. the default phase angle, allowing a margin for application of the pointing constraint. |
| unconstrainedPhaseAngle | MAL::Boolean | No | If TRUE no constraint will apply to the phaseAngle. The phaseAngleMargin attribute will be ignored in this case.  Default = FALSE |
| pointingTemplate | MAL::String | No | Corresponds to one of those defined in the NAV Pointing Request Message standard. A MAL::String is used to represent the pointing template type to allow for future extension. |
| pointingArguments | List <MAL::NamedValue> | Yes | The argument list is consistent with the referenced template by name. Physical Values are represented as a pair of arguments containing the value and units respectively. Position and Direction type arguments are represented as strings containing the literal value. |

The following table summarises currently defined pointing templates and their additional arguments. Not all templates require additional arguments.

| Pointing Template | Argument | Type |
| --- | --- | --- |
| Inertial Pointing | target  phaseAngle  offsetAngle  angularRate | Direction  Angle  Angle  AngularVelocity |
| Sun Pointing | phaseAngle  offsetAngle  angularRate | Angle  Angle  AngularVelocity |
| Track with Inertial Direction Yaw Steering | targetBody  phaseAngle | Position  Angle |
| Track with Power Optimized Yaw Steering | targetBody | Position |
| Nadir with Power Optimized Yaw Steering |  |  |
| Nadir with Ground Track Aligned Yaw Steering |  |  |
| Nadir with Orbital Pole Aligned Yaw Steering |  |  |
| Limb Pointing with Power Optimized Yaw Steering | surface  dirVector  height | MAL::String  Direction  Distance |
| Limb Pointing with Inertial Direction Yaw Steering | surface  dirVector  height  phaseAngle | MAL::String  Direction  Distance  Angle |
| Velocity Pointing with Orbital Pole Yaw Steering | phaseAngle | Angle |

RevolutionConstraint

Specifies a range of revolution angles for a rotating spacecraft.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RevolutionConstraint** | **Extends** | *GeometricConstraint* | **SFP** | 50 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| revolutionAngle | RealExpression | No | Angle of revolution |
| tolerance | RealExpression | No | Tolerance in the angle of revolution |
| units | MAL::String | Yes | Optional. The angular unit name, as defined in [PRM] annex D.  Default = “deg”. |

DistanceConstraint

Specifies a range of distances between two physical objects (the Observer and the Target).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **DistanceConstraint** | **Extends** | *GeometricConstraint* | **SFP** | 51 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| observer | PositionExpression | No | Position of the Observer [Object1] |
| target | PositionExpression | No | Position of the Target [Object2] |
| minDistance | RealExpression | No | Minimum Distance between Observer and Target |
| maxDistance | RealExpression | No | Maximum Distance between Observer and Target |
| units | MAL::String | Yes | Optional. The distance unit name, as defined in [PRM] annex D.  Default = “km”. |

AngleConstraint

Specifies a range of values for the angle subtended between three physical objects. The constrained angle is that subtended at the central object by target objects 1 and 2.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **AngleConstraint** | **Extends** | *GeometricConstraint* | **SFP** | 52 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| centreObject | PositionExpression | No | Position of the central object. |
| targetObject1 | PositionExpression | No | Position of target object 1. |
| targetObject2 | PositionExpression | No | Position of target object 2. |
| minAngle | RealExpression | No | Minimum Angle subtended at the central object by target objects 1 and 2.. |
| maxAngle | RealExpression | No | Maximum Angle subtended at the central object by target objects 1 and 2. |
| Units | MAL::String [0..1] | Yes | Optional. The angular unit name, as defined in [PRM] annex D.  Default = “deg”. |

#### Effects [Optional]



Figure : Effects

Effects are an optional element of the MPS information model that may be used in conjunction with planning resources. They specify the impact that executing a planning activity will have on planning resources. These may be used to predict the evolution of the values of planning resources over the period of a plan. This in turn enables the verification that sufficient resource is available for execution of the plan and that all explicit resource constraints are satisfied.

The abstract type Effectidentifies the planning activity that causes the effect and the planning resource to which the effect is applied. The planning activity may be identified by ActivityDefinition, in which case it applies to all instances of that definition, or by a specific ActivityInstance. There are two concrete sub-types:

* Simple Effect
* Complex Effect

*Effect*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***Effect*** | **Extends** | *Constraint* | **SFP** | Abstract |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| activityRef | ObjectExpression | No | Identifies the planning activity for which the Resource Constraint applies. May be either an ActivityDefinition or an ActivityInstance. |
| resourceRef | MAL::ObjectRef | No | Identifies the planning resource that is constrained for the duration of the planning activity. |

These attributes are common to both sub-types.

Simple Effect

A Simple Effect applies the defined operation on the specified planning resource at the time relative to the planning activity defined by TimeRef+TimeOffset.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **SimpleEffect** | **Extends** | *Effect* | **SFP** | 53 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| timeRef | Slider | No | The point in the duration of the planning activity to which the time of the Effect is relative. 0: the start of the planning activity 1: the end of the planning activity |
| timeOffset | DurationExpression | No | Offset from TimeRef that specifies the time at which the Effect is to be applied. |
| operator | EffectOperationEnum | No | Operation to be performed on the planning resource. One of: SET, INCREMENT, DECREMENT.  Increment and Decrement are only applicable to numeric data types. |
| value | MAL::Attribute | No | The value that the planning resource is to be set to if the EffectOperation is SET; or to be incremented/decremented by if it is INCREMENT or DECREMENT. |

EffectOperationEnum

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **EffectOperationEnum** | **SFP** | 54 |

| Status | Value | Description |
| --- | --- | --- |
| SET | 1 | Set to specified value |
| INCREMENT | 2 | Increment by specified value |
| DECREMENT | 3 | Decrement by specified value |

ComplexEffect

In the Simple Effect, the value of the impacted planning resource is set to the specified value at a single point in time.

With the Complex Effect, the value of the impacted planning resource can be evolved over a specified time period in accordance with a defined Relative Resource Profile.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **ComplexEffect** | **Extends** | *Effect* | **SFP** | 55 |

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute | Type | Nullable | Description |
| startRef | Slider | No | Identifies the point in the duration of the referenced planning activity to which the start of the effect period relates. |
| endRef | Slider | No | Identifies the point in the duration of the referenced planning activity to which the end of the effect period relates. |
| startOffset | Duration Expression | No | Offset from StartRef that specifies the start of the effect period. |
| endOffset | Duration Expression | No | Offset from EndRef that specifies the end of the effect period. |
| operator | EffectOperationEnum | No | Operation to be performed on the planning resource. One of: SET, INCREMENT, DECREMENT.  Increment and Decrement are only applicable to numeric data types. |
| Value | RelResourceProfile | No | Resource Profile specifying an evolving value to which the value of the planning resource is to be set.  See §3.2.4.2 |

### Triggers



Figure : Triggers

A Trigger is a construct that allows specification of the specific condition or event that marks the start or end of something. It is used in the context of both planning activities and plans to specify when an activity should start.

The following sub-types of Trigger are supported:

* Time Trigger: the trigger event is defined by time.
* Position Trigger: the trigger event is defined by position.
* Pointing Trigger: the trigger event is defined by pointing
* Event Trigger: the trigger event is defined in terms of a planning event.

Position and Pointing Triggers are optional elements of the MPS Information Model.

*Trigger*

All sub-classes of Trigger include the time at which they are predicted to occur (in advance of execution); and, where applicable, the time at which they actually occurred (post execution).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***Trigger*** | **Extends** | MAL::Composite | **SFP** | Abstract |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| time | MAL::Time | No | Predicted or Actual Time of Trigger. The predicted Time may evolve during the planning process up to the time of execution. The actual Time is only available post execution, and hence can only be provided by a Plan Execution function. |

#### Temporal Triggers

TimeTrigger

Sub-type of Trigger based on Time. The Trigger Time is the specified constraint, and will usually match the predicted Time on the base class during the planning process, but the actual Time could still be slightly different post-execution.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **TimeTrigger** | **Extends** | *Trigger* | **SFP** | 56 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| trigger Time | MAL::Time | No | Planned Time of Trigger. |

#### Location Triggers [Optional]

*LocationTrigger*

Optional sub-type of Trigger based on Location. Separate concrete sub-types provide for the trigger based on position and orbital position.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***LocationTrigger*** | **Extends** | *Trigger* | **SFP** | Abstract |

PositionTrigger

Sub-type of Location Trigger for the general case of a specified Position.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PositionTrigger** | **Extends** | *LocationTrigger* | **SFP** | 57 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| triggerPosition | Position | No | Planned Position of Trigger. |
| distanceMargin | Distance | No | Defines a sphere around the trigger position within which a position is considered to meet the trigger condition. |

OrbitalPositionTrigger

Sub-type of Position Trigger based on orbital repeat cycle.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **OrbitalPositionTrigger** | **Extends** | *LocationTrigger* | **SFP** | 58 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| orbitNumber | MAL::Integer | No | Orbit Number. Depending on the RelativeOrbit flag, the Orbit Number may be absolute (since start of mission) or relative (to the orbital repeat cycle). |
| relativeOrbit | MAL::Boolean | No | Flag indicating if the Orbit Number is absolute or relative to the orbital repeat cycle. |
| orbitAngle | MAL::Double | No | Angle within Orbit |

#### Pointing Triggers [Optional]

*PointingTrigger*

Sub-type of Trigger based on Pointing. Separate concrete sub-types provide for the specification of the trigger based on direction and revolution angle.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***PointingTrigger*** | **Extends** | *Trigger* | **SFP** | Abstract |

DirectionTrigger

Sub-type of Pointing Trigger for the general case of a specified Direction.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **DirectionTrigger** | **Extends** | *PointingTrigger* | **SFP** | 59 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| triggerDirection | Direction | No | Planned Direction of Trigger. |
| angleMargin | Angle | No | Defines a circle around the trigger direction within which a direction is considered to meet the trigger condition. |

RevolutionTrigger

Sub-type of Pointing Trigger based on the angle of revolution of a rotating spacecraft.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RevolutionTrigger** | **Extends** | *PointingTrigger* | **SFP** | 60 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| revolutionAngle | MAL::Double | No | Angle within Revolution |

#### Angle Trigger [Optional]

Angle Trigger

Sub-type of Trigger based on the angle subtended between three physical objects. The trigger angle is that subtended at the central object by target objects 1 and 2.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **AngleConstraint** | **Extends** | *Trigger* | **SFP** | 61 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| centreObject | PositionExpression | No | Position of the central object. The trigger angle is that subtended at the central object by target objects 1 and 2. |
| targetObject1 | PositionExpression | No | Position of target object 1. |
| targetObject2 | PositionExpression | No | Position of target object 2. |
| angleMargin | Angle | No | The trigger occurs if the angle is within ± angleMargin of the trigger angle. |

#### Event Triggers

Event Trigger

Sub-type of Trigger based on Planning Event.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **EventTrigger** | **Extends** | *Trigger* | **SFP** | 62 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| triggerEvent | MAL::ObjectRef | No | Reference to a Planning Event Instance |
| timeOffset | MAL::Duration | No | Time offset from the Planning Event Instance |

### Repetitions



Figure : Repetitions

*Repetition*

A Repetition is used to specify the repeated instantiation of a [set of] Planning Activities. Multiple sub-types of Repetition are defined to support the specification of repeat cycles by different criteria. It can be used in the context of a Planning Request to specify a standing order for repeated execution of the [set of] Planning Activities.

In the context of an ActivityNode embedded within a Planning Request (see 3.2.2.3), it is possible to nest one Repetition inside another, enabling the specification of complex repetitive sequences of activities.

All sub-types have the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***Repetition*** | **Extends** | MAL::Composite | **SFP** | Abstract |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| count | MAL::Integer | Yes | Maximum number of repeat cycles/instances [optional].  If not specified there is no limit to the number of repetitions. |
| timeWindow | TimeWindow | Yes | Time period over which the repetition is applicable [optional].  If not specified repetition continues indefinitely. |
| separationType | SeparationTypeEnum | No | Specifies whether the repetition interval is **Relative** to the previous occurrence, or **Absolute** for all occurrences. |

For Repetitions, the interval between occurrences [the cadence] is expressed as a Separation±Tolerance.

If the SeparationType is Relative, then this defines the required interval between successive occurrences: Tn+1 = Tn+Separation±Tolerance. Consequently, the average interval over multiple occurrences may deviate from the specified separation.

If the SeparationType is Absolute, then the Tolerance relates to a multiple of Separation from the initial occurrence, and is not directly related to the interval between successive occurrences: Tn = T0+n\*Separation±Tolerance.

SeparationTypeEnum

|  |  |  |  |
| --- | --- | --- | --- |
| Name | **SeparationTypeEnum** | **SFP** | 63 |

| Enumeration | Value | Description |
| --- | --- | --- |
| RELATIVE | 1 | Tolerance on separation is only considered between any two occurrences |
| ABSOLUTE | 2 | Tolerance on separation applies to a multiple of the separation from the initial occurrence. |

#### Temporal Repetition

TemporalRepetition

A sub-type of Repetition based on Time.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **TemporalRepetition** | **Extends** | *Repetition* | **SFP** | 64 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| initialTime | TimeExpression | No | Nominal time of first occurrence. |
| separation | DurationExpression | No | The required time interval between occurrences. |
| tolerance | DurationExpression | No | The allowed tolerance (+/-) in the required time between occurrences, the interpretation of which is dependent on the SeparationType. |

#### Location Repetition [Optional]

*LocationRepetition*

A sub-type of Repetition based on Position. Separate concrete sub-types provide for repetitions based on generic position and orbital position.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***LocationRepetition*** | **Extends** | *Repetition* | **SFP** | Abstract |

PositionRepetition

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **PositionRepetition** | **Extends** | *LocationRepetition* | **SFP** | 65 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| initialPosition | PositionExpression | No | Nominal position of first occurrence. |
| repetitionDirection | DirectionExpression | No | Direction of repetition. |
| separation | RealExpression | No | The required Distance between occurrences. |
| tolerance | RealExpression | No | The allowed tolerance (+/-) in the required distance between occurrences, the interpretation of which is dependent on the SeparationType. |
| units | MAL::String | Yes | The units used for Separation and Tolerance |

OrbitalRepetition

A sub-type of Repetition based on the Orbital cycle.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **OrbitalRepetition** | **Extends** | *LocationRepetition* | **SFP** | 66 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| orbitNumber | IntegerExpression | No | Orbit number for the first occurrence. Depending on the RelativeOrbit flag, the Orbit Number may be absolute (since start of mission) or relative (to the orbital repeat cycle). |
| orbitAngle | RealExpression | No | The required position of the first occurrence within the orbit expressed as an angle. |
| relativeOrbit | MAL::Boolean | No | Flag indicating if the Orbit Number is absolute or relative to the orbital repeat cycle. |
| orbitSeparation | IntegerExpression | No | The required number of orbits separation between occurrences. If OrbitNumber is Relative and the required repetition is once per repeat cycle, this is the number of orbits in the repeat cycle, but the value 0 may also be used. |
| angularSeparation | RealExpression | No | The required angular separation between occurrences. This allows for multiple repetitions within an orbit. The value 0 indicates only one occurrence within the orbit. |
| tolerance | RealExpression | No | The allowed tolerance (+/-) in the required orbital angle. |
| units | MAL::String | Yes | The units used for OrbitAngle, AngularSeparation and Tolerance |

Note that the SeparationType is irrelevant in this case.

#### Pointing Repetition [Optional]

*PointingRepetition*

A sub-type of Repetition based on Pointing. Concrete sub-types provide for repetition based on direction and revolutions.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | ***PointingRepetition*** | **Extends** | *Repetition* | **SFP** | Abstract |

DirectionRepetition

A sub-type of Repetition based on direction, which supports the specification of astronomical surveys

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **DirectionRepetition** | **Extends** | *PointingRepetition* | **SFP** | 67 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| initialDirection | DirectionExpression | No | Nominal direction of first occurrence. |
| targetDirection | DirectionExpression | No | Specifies the direction of repetition as line connecting the initial and target directions. |
| separation | RealExpression | No | The required angle between occurrences. |
| tolerance | RealExpression | No | The allowed tolerance (+/-) in the required angle between occurrences, the interpretation of which is dependent on the SeparationType. |
| units | MAL::String | Yes | The units used for Separation and Tolerance |

RevolutionRepetition

A sub-type of Repetition based on the Revolutions of a rotating spacecraft or instrument.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **RevolutionRepetition** | **Extends** | *PointingRepetition* | **SFP** | 68 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| revsSeparation | IntegerExpression | No | The required number of revolutions between occurrences. |
| revsTolerance | IntegerExpression | No | The allowed tolerance (+/-) in the required number of revolutions between occurrences, the interpretation of which is dependent on the SeparationType. |
| revAngle | RealExpression | Yes | Specifies the angle within a revolution. |
| units | MAL::String | Yes | The units used for RevAngle |

#### Angle Repetition [Optional]

AngleRepetition

A sub-type of Repetition based on the angle subtended between three physical objects. The repetition angle is that subtended at the central object by target objects 1 and 2.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **AngleRepetition** | **Extends** | *Repetition* | **SFP** | 69 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| centreObject | PositionExpression | No | Position of the central object. |
| targetObject1 | PositionExpression | No | Position of target object 1. |
| targetObject2 | PositionExpression | No | Position of target object 2. |
| initialAngle | RealExpression | No | Initial Angle subtended at the central object by target objects 1 and 2. |
| separation | RealExpression | No | The required Angle between occurrences.  If this is zero, this implies that repetition is between multiple occurrences of the initialAngle. |
| tolerance | RealExpression | No | The allowed tolerance (+/-) in the required angle between occurrences, the interpretation of which is dependent on the SeparationType. |
| units | MAL::String | Yes | The units used for Separation and Tolerance |

The count attribute inherited from the abstract *Repetition* class can be used to specify how many repetitions should be planned. If the separation angle is zero, then repetition is based on each occurrence of the specified initialAngle. If the separation angle is non-zero, then this is used to indicate repetition at different subtended angles. For example, for an initial angle of 20° and a count of 5:

* if the separation is 2° then the activity is planned when the initial angle of 20° occurs, and then with 4 further repetitions at 2° intervals up to 28°.
* if the separation is 0° then the activity is planned for the next 5 occurrences of the initial angle of 20°

Note that repetitions can be nested to allow repetition over both occurrences and offset angles.

#### Event Repetition

Event Repetition

A sub-type of Repetition based on Planning Events.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | **EventRepetition** | **Extends** | *Repetition* | **SFP** | 70 |

| Attribute | Type | Nullable | Description |
| --- | --- | --- | --- |
| eventRef | ObjectExpression | No | Reference to a Planning Event Definition (type of Event) |
| separation | IntegerExpression | No | Number of occurrences of the Planning Event required between occurrences of the Planning Activity. |
| tolerance | IntegerExpression | No | The allowed tolerance (+/-) in the number of occurrences of the Planning Event between occurrences of the Planning Activity, the interpretation of which is dependent on the SeparationType. |

## MO Framework

This section gives a brief introduction to elements of the MO framework relevant to the MPS Information Model, organised in the following subsections:

* Message Abstraction Layer (MAL)
* MO Objects
* MO Object Patterns

For a full description of the MAL, the reader is referred to the corresponding CCSDS standard document.

The MPS Information Model is not defined in terms of the MO Common Object Model [COM], as it is anticipated that this will be deprecated in the next version of the MO framework. Instead the structure of MPS Objects is fully defined within this document, together with their relationships.

### Message Abstraction Layer (MAL)

For information to be carried by an MO compliant service, it must be defined in terms of the data types specified by the Message Abstraction Layer (MAL) to enable encoding of MAL messages in accordance with multiple MO Technology Bindings.

The MAL Attribute is the simplest MAL element; it cannot be decomposed into smaller elements and is used to build more complex structures. There is a non-extensible set of MAL Attribute types defined by the MAL, corresponding to common data types. These types are detailed in §3.3.1 above and directly referenced in the MPS information model using the form MAL::<AttributeType>. The MAL also allows the use of the type MAL::Attribute as a generic for any supported MAL Attribute type, effectively supporting polymorphism at this level.

The MPS Information Model assumes the following data types will be directly supported by the MAL:

* Object ID
* Version
* Object Reference (including both Object ID and Version)

MAL Composites are compound data structures comprising multiple MAL Attributes. The MAL can transport any fixed data structure defined as a MAL Composite, but does not allow for polymorphism within these structures.

### MO Objects



Figure : MO Objects

An MO Object is an entity defined within the information model of an MO compliant service specification that has a unique identity enabling it to be referenced by other MO Objects and in the body of MO service messages.

The identity of an MO Object is defined by its Object ID and optionally by a Version.

The Object ID includes the domain of the object, which allows for the concept of hierarchical namespacing.

MO Objects may have both static attributes that do not change and dynamic attributes that can change over time. For some types of object, it may be occasionally required to change the value of the static attributes, while maintaining the same Object ID for continuity. In this case, the MO Object should be defined with a Version. The combination of Object ID and Version provides a unique identity for a specific version of the object and its static attributes. This approach is typically used for definition objects that may be occasionally updated.

Relationships with other MO Objects can be defined within an MO Object by including attributes of type ObjectRef. An ObjectRef can specify both the ObjectID and a specific Version of the referenced MO Object. Examples of types of relationships that can be defined include:

* **Definition**: MO Objects that are dynamically instantiated based on an existing definition may reference the corresponding definition object. An example is the relationship between and ActivityInstance and the corresponding ActivityDefinition.
* **Source**: MO Objects that are dynamically instantiated may reference another object responsible for its creation. An example is the relationship between an ActivityInstance and its source planning RequestInstance.
* **Parent/Child**: MO Objects that are hierarchically organised may reference their parent or child objects. Examples include hierarchical ActivityInstances and EventInstances.
* **Other**: special relationships that are specific to a class of MO Objects. Examples include the relationship of an ActivityInstance to an EventInstance that governs its timing and/or input arguments.

The MPS Information Model defines the following nine classes of MO Object:

* ActivityDefinition
* ActivityInstance
* EventDefinition
* EventInstance
* Resource
* RequestDefinition
* RequestInstance
* Plan
* MPSSystemConfig

### MO Object Patterns

The information objects associated with MO compliant services are often implemented as a compound set of objects, each of which is derived from the MO Object. These compound objects often follow one of a number of common object patterns.

Three such MO Object Patterns, relevant to MPS, are illustrated in Figure 41:

* MO Static Item
* MO State
* MO Instance

These share the following common elements:

* A unique Identity that may be used to reference all occurrences of the information object (compound object) throughout the mission lifetime. This is a combination of the domain and a unique name within the domain. The Identity forms part of the Definition object below.
* A Definition that comprises the statically declared information associated with the information object. This may, for example, include a description, set of defined arguments or any other information that applies to all occurrences of the information object. There may be multiple Versions of the Definition over the mission lifetime associated with the same Identity. Definitions are typically contained in configuration databases that are maintained off-line under version control and deployed for use in the on-line environment.
* An Instance that is dynamically created for each new occurrence of the information object. This includes the unique Instance ID of the occurrence and any unchanging data associated with it as a set of static attributes. It also includes the current status of the object as a set of dynamic attributes.

An Instance has a reference to its Definition.

* An Update is a data structure used to report the changing status of the information object or a specific occurrence of it at a specific point in time. This may include a current value, current processing state, or a current set of values for defined arguments. Updates may be generated periodically, or only when there is a change of status. Updates may be used to disseminate changing status and to record the detailed status history of the information object.

An Update has a reference to its Instance.







Figure : MO Object Patterns

#### MO Static Item Object Pattern

An MO Static Item is a single element information object that only comprises statically declared information with no evolving status. An MPS example is the MPSSystemConfig object that contains configuration parameters for an MPS system.

Static Items comprise only the Definition object described above, with no corresponding Update data structure.

#### MO State Object Pattern

An MO State is a single element information object representing a status: it is a persistent object for which there is only one set of dynamic status values at any given time (although this may not be known). MPS examples are Planning Resources, and Plans.

MO States comprise two of the elements described above: a Definition object and Update data structure. As it is persistent rather than instantiated, status Updates relate directly to the Definition object. Note that for Plans the corresponding Definition object is created dynamically as part of the planning process, and is not normally considered part of the planning configuration data.

#### MO Instance Object Pattern

An MO Instance is a dual element compound information object representing any type of operation that is repeatable and extends over a measurable period of time. MPS examples include Planning Requests, Planning Activities and Planning Events.

MO Instance comprises all three of the elements described above: Definition and Instance objects and Update data structure. As an MO Instance may be invoked multiple times, there may be multiple Instance objects created from the same Definition object. Updates relate to a specific Instance object.

A Details data structure may also be required to specify the information needed to create an Instance from a Definition. For example, this may include how to derive any argument values, or any specific constraints to be applied. The Details do not themselves form part of the information object to which they relate, but may be embedded within another information object, typically the parent or source object responsible for creation of the instance.

For MPS, only Planning Activities have a Details data structure defined, which may be embedded within a Planning Request or the Definition of a parent activity to specify its children.

# MPS Service Specifications

## General

*Introduction to Service Specification chapter. List services. Summarise context in terms of MAL and MO Objects. Note that data structures for service message bodies are either defined in the Information Model, or simple structures may be expanded within the operation specification.*

This chapter contains the service specifications for the MPS Services. An overview of the the services has been given previously in section 2.5 above. Each of the following services is defined in a separate section below:

* Planning Request Service
* Plan Distribution Service
* Plan Execution Control Service
* Plan Information Management Service
* Plan Edit Service

There is no requirement to implement all services. Any subset of the services may be supported by an MPS deployment.

Each service specification comprises the following parts:

1. Summary: contains a table listing the service operations and grouping them into capability sets, and UML sequence diagrams illustrating the service operations.
2. MO Objects: identifies the set of MO Objects (defined in chapter 3) that are operated on by the service or referenced by service operations.
3. High-Level Requirements: such as the set of configuration data required by the service.
4. Functional Requirements: specific requirements on the behaviour of the service provider and consumer.
5. Operations: specification of each service operation.

All services defined in this document are part of the MPS Area, which has the Area number 42.

## Service: Planning Request

### Summary

The Planning Request Service, introduced in §2.5.2, is provided by a planning function and enables its consumers to manage the submission of planning requests and to receive feedback on their status. It comprises the following operations, of which only those in capability set 1 are mandatory.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Area Identifier | Service Identifier | Area Number | Service Number | Area Version |
| MPS | PlanningRequest | 42 | 1 | 1 |

| Interaction Pattern | Operation Identifier | Operation Number | Capability Set |
| --- | --- | --- | --- |
| REQUEST | submitRequest | 1 | 1 |
| REQUEST | getRequestSummaries | 2 |
| PROGRESS | getRequestStatus | 3 |
| SUBMIT | cancelRequest | 4 | 2 |
| REQUEST | updateRequest | 5 | 3 |
| PUBSUB | monitorRequestStatus | 6 | 4 |
| PROGRESS | getRequest | 7 | 5 |



Figure : Planning Request Submission Operations

Three of the operations are concerned with the submission and subsequent management of planning requests, enabling a service consumer to submit a planning request, and (where supported) to update or cancel that request. The interaction sequence for these operations is illustrated in Figure 42 above.

The submitRequest operation results in the creation of a new PlanningRequestInstance, returning its identity in the response message. The updateRequest operation results in a new version of an existing PlanningRequestInstance, returning its identity (ID and version) in the response message. The cancelRequest operation stops the referenced PlanningRequestInstance being considered in the generation of future Plans, but does not imply that it is immediately deleted by the provider.



Figure : Planning Request Feedback Operations

The remaining operations are concerned with obtaining feedback on the status or content of planning requests. The interaction sequence for these operations is illustrated in Figure 43 above.

The getRequestSummaries operation requests a list of available planning requests based on a supplied filter. It returns a list of RequestSummaryStatuses that contain the identity, header information and status for each available RequestInstance that matches the filter.

A consumer may already holds the identity (and static content) of RequestInstances, either because it has submitted planning requests, or previously performed a getRequestSummaries operation. It can then request an update of their dynamic status using the getRequestStatus operation. The request lists references to RequestInstances and the response provides a corresponding list of RequestStatusUpdates.

Where supported, consumers may also subscribe to receive RequestStatusUpdates as they become available via the monitorRequestStatus . This uses the standard MAL publish-subscribe pattern and notifies the consumer with RequestStatusUpdates corresponding to the specified subscription keys as they are published by the provider.

The getRequest operation, where supported, enables a consumer to retrieve the full content of one or more planning requests. This is similar to the getRequestStatus operation, but instead of returning RequestStatusSummaries it returns RequestInstances. Note that this is not an archive service, only planning requests currently being managed by the provider can be returned.

### MO Objects

MO Objects relevant to the planning request service and their relationships are defined within the MPS Information Model in section 3.2.

The following MO Objects are directly applicable to the service (see Figure 19):

* RequestDefinition
* RequestInstance

RequestDefinitions are configuration data that provide re-usable templates for planning requests, but are not required for the submission of an ad-hoc planning request. Their identity comprises both ID and version.

RequestInstances are created in response to the submission of a planning request and contain both static data and dynamic status information. As planning requests can be updated, their identity comprises both ID and version assigned by the service provider. The planning request submitted by the service consumer contains only the static data needed to specify the planning request in the form of a PlanningRequestDetails structure. If the planning request is derived from a RequestDefinition, this is referenced in the PlanningRequestDetails and the RequestInstance created from it.

As the RequestInstance is unknown at the time of submitting a planning request, the consumer may provide a user reference. This is returned by the provider together with the identity of the RequestInstance in the response to the planning request submission.

Updates to the dynamic status information associated with a RequestInstance are reported by the service provider to the service consumer using the RequestStatusUpdate structure. The RequestSummaryStatus structure is used to provide the identity, descriptive header fields and current status of available RequestInstances.

The following MO Objects may be referenced in the context of the planning request service:

* PlanningUser: the user responsible for submitting the planning request
* ActivityDefinition: the activities specified to be planned in the form of ActivityDetails structures in the body of the planning request.
* EventDefinition and EventInstance: references to planning events can be contained within ActivityDetails and Constraints contained in the body of the planning request.
* Resource [Optional]: references to planning resources can be contained within the Constraints contained in the body of the planning request.
* Plan: a Plan or reference to a Plan can be used as the body of a planning request. Once the planning request has been planned, a reference to the resulting output Plan may also be included in the RequestInstance.

### High-Level Requirements

**Req\_4.2.3.H.1** The following set of mission planning configuration data shall be available to both provider and consumers in a any deployment of the planning request service:

1. Planning Request Definitions (as RequestDefinition objects [§3.2.5.1] )
2. Planning Activity Definitions (as ActivityDefinition objects [§3.2.2.1])
3. Planning Event Definitions (as EventDefinition objects [§3.2.3.1])
4. Planning Resource Definitions (as Resource objects [§3.2.4.1]) [Optional]
5. MPS System Configuration Data (as an MPSSysConfig object [§3.2.7])

### Functional Requirements

**Req\_4.2.4.F.2** In response to a submitRequest operation, the service provider shall create a corresponding RequestInstance object, set its creationDate and return its identity (ID and version) to the consumer.

**Req\_4.2.4.F.3** In response to an updateRequest operation, if supported, the service provider shall create a new version of the referenced RequestInstance object, set its creationDate and return its identity (ID and version) to the consumer.

**Req\_4.2.4.F.4** The service provider shall only consider the latest version of a RequestInstance in the generation of future Plans, following a successful updateRequest operation.

**Req\_4.2.4.F.5** In response to a cancelRequest operation, if supported, the service provider shall set the requestStatus of the referenced RequestInstance object to “CANCELLED” and stops it being considered in the generation of future Plans.

**Req\_4.2.4.F.6** In response to internal planning and feedback from external plan execution processes, the service provider shall model the status of RequestInstance objects in accordance with the planning request state model (§3.2.5.2).

Note: following a successful updateRequest operation, it is implementation dependent what the status of the previous version of the RequestInstance is set to. Previous versions may already have been incorporated into Plans.

**Req\_4.2.4.F.7** If a service consumer generates a planning request based on an an existing planning request definition, then the PlanningRequestDetails submitted shall:

1. Reference the source RequestDefinition (ID and version) in the definition field;
2. Contain a matching set of arguments (name and type) to the RequestDefinition in the arguments field;
3. Have a matching value to the RequestDefinition in the standingOrder field.

Note: while typically the PlanningRequestDetails will also have matching content to the RequestDefinition in the activities and constraints fields it is allowed to add and remove individual activities and constraints.

**Req\_4.2.4.F.8** Following successful inclusion of a planning request in a generated Plan, the service provider shall update the outputPlanRef attribute of the RequestInstance with the identity of the Plan (ID and version).

Note: the consumer may then use the reference to the output Plan to retrieve the Plan or its status using the PlanDistributionService. Where the planning request has been incorporated into multiple alternate plans, these will be listed in the outputPlanRef attribute.

### Operation: submitRequest

#### Overview

The submitRequest operation sends a planning request to the provider, which then creates a corresponding RequestInstance object and returns its identity to the consumer.

|  |  |
| --- | --- |
| **Operation Identifier** | submitRequest |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | requestDetails : (PlanningRequestDetails) |
| OUT | RESPONSE | requestResponse : (PlanningRequestResponse) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getRequestSummaries

#### Overview

The getRequestSummaries operation allows consumers to obtain a filtered list of currently available RequestInstances. The request uses the RequestFilter structure to select the set of planning requests of interest, using the following keys:

* Domain of the RequestInstance
* Instance ID (and version) of the RequestInstance
* Creation date-time of the Request Instance version (as a time range)
* Definition ID (and version) of the RequestInstance (the RequestDefinition from which it was created)
* User ID of the User who initated the RequestInstance
* User Reference supplied by the User when submitting the RequestInstance

The response returns a list of RequestSummaryStatus structures containing the identity (ID and version), descriptive header fields and status of the RequestInstances that match the filter.

|  |  |
| --- | --- |
| **Operation Identifier** | getRequestSummaries |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | requestFilter : (RequestFilter) |
| OUT | RESPONSE | requestSummaries : (List <RequestSummaryStatus)>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getRequestStatus

#### Overview

The getRequestStatus operation is used to obtain the current status of one or more known RequestInstances. The operation uses the Progress interaction pattern, to allow the response to be spread across multiple messages.

|  |  |
| --- | --- |
| **Operation Identifier** | getRequestStatus |
| **Interaction Pattern** | PROGRESS |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | PROGRESS | requestRefs : (List <MAL::ObjectRef[RequestInstance]>) |
| OUT | ACK | Empty |
| OUT | UPDATE | updateStatuses : (List <RequestStatusUpdate>) |
| OUT | RESPONSE | responseStatuses : (List <RequestStatusUpdate>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: cancelRequest

#### Overview

The cancelRequest operation is used by a consumer to cancel a previously submitted planning request. The service provider acknowledges the cancellation of the RequestInstance or returns an error.

|  |  |
| --- | --- |
| **Operation Identifier** | cancelRequest |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | requestRef : (MAL::ObjectRef[RequestInstance]) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* CANCEL\_FAILED

If it was not possible to cancel the RequestInstance, for example because the resultant activities have already been executed or activated within a plan execution function, then the CANCEL\_FAILED error is returned.

### Operation: updateRequest

#### Overview

The updateRequest operation may be used to modify the PlanningRequestDetails associated with a previously submitted planning request. This results in the creation of a new version of the RequestInstance (with the same ID) by the service provider, which returns the identity (ID and version) of the new version to the consumer.

|  |  |
| --- | --- |
| **Operation Identifier** | updateRequest |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | requestRef : (MAL::ObjectRef[RequestInstance])  requestDetails : (PlanningRequestDetails) |
| OUT | RESPONSE | requestResponse : (PlanningRequestResponse) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* UPDATE\_FAILED

If it was not possible to update the RequestInstance, for example because the resultant activities have already been executed or activated within a plan execution function, then the UPDATE\_FAILED error is returned.

### Operation: monitorRequestStatus

#### Overview

The monitorRequestStatus operation is used to subscribe to status updates for a filtered set of planning RequestInstances. The operation uses the Publish-Subscribe interaction pattern, with the body of the notification message comprising a RequestStatusUpdate for a subscribed RequestInstance.

|  |  |
| --- | --- |
| **Operation Identifier** | monitorRequestStatus |
| **Interaction Pattern** | PUBLISH-SUBSCRIBE |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| OUT | PUBLISH/NOTIFY | requestStatusUpdate : (RequestStatusUpdate) |

Other messages of the Publish-Subscribe pattern are fully defined by the MAL.

#### Structures

**Req\_4.2.10.S.9** The monitorRequestStatus subscription shall be based on the provision of the following keys of the required RequestInstances in the Register message, all of which are nullable:

1. subDomain = domain of subscribed RequestInstances
2. entityKeys.firstSubKey = instanceID of subscribed RequestInstances
3. entityKeys.secondSubKey = definitionID of subscribed RequestInstances
4. entityKeys.thirdSubKey = userID of subscribed RequestInstances
5. entityKeys.fourth SubKey = userReference of subscribed RequestInstances

Note: this assumes the current MAL limit of four entity keys. It is hoped that in the future, the publish-subscribe pattern subscription will allow the specification of an arbitrary list of key field-value pairs. Should this be extended the following additional subscription keys should be supported:

1. status of subscribed RequestInstance
2. outputPlanRef of subscribed RequestInstance

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getRequest

#### Overview

The getRequest operation is used to obtain the full content of one or more known RequestInstances. The operation uses the Progress interaction pattern, to allow the response to be spread across multiple messages.

|  |  |
| --- | --- |
| **Operation Identifier** | getRequest |
| **Interaction Pattern** | PROGRESS |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | PROGRESS | requestRefs : (List <MAL::ObjectRef[RequestInstance]>) |
| OUT | ACK | Empty |
| OUT | UPDATE | updateRequestInstances : (List <RequestInstance>) |
| OUT | RESPONSE | responseRequestInstances : (List<RequestInstance>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

## Service: Plan Distribution Service

### Summary

The Plan Distribution Service, introduced in §2.5.3, is provided by a planning function and enables its consumers to access generated plans and to receive updates on their status. It comprises the following operations, of which only those in capability set 1 are mandatory.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Area Identifier | Service Identifier | Area Number | Service Number | Area Version |
| MPS | PlanDistribution | 42 | 2 | 1 |

| Interaction Pattern | Operation Identifier | Operation Number | Capability Set |
| --- | --- | --- | --- |
| REQUEST | getPlanSummaries | 1 | 1 |
| PROGRESS | getPlan | 2 |
| REQUEST | getPlanStatus | 3 |
| PUBSUB | monitorPlanStatus | 4 | 2 |
| PUBSUB | monitorPlan | 5 | 3 |
| PROGRESS | queryPlan | 6 | 4 |
| REQUEST | getPartialPlan | 7 | 5 |

Note: the getPlanStatus, with the exception of the service number, is identical to the operation of the same name in the Plan Execution Control Service.



Figure : Plan Distribution Mandatory Operations

The mandatory operations of capability set 1 allow a service consumer to access plans, or the status of plans, generated by a planning function.

To retrieve a plan, the consumer needs to have the identity of that plan (ID and optionally version). A reference to the output plan associated with a planning request may have been received through planning request service feedback. Otherwise, the consumer must use the getPlanSummaries operation to discover available plans.

The getPlanSummaries operation returns PlanSummaries for the set of currently available plans that meet the specified filter criteria. These give the identity of the plans, the associated plan information (context and descriptive fields) and the current status of the plan, but do not include the full content of the plans.

The getPlan operation returns the full content of the referenced Plan(s).

The getPlanStatus operation returns only the current status of the referenced plan(s) as PlanUpdates.



Figure : Plan Distribution Monitoring Operations

Where supported, the monitorPlanStatus operation enables the consumer to subscribe to automatic notification of changes in status of plans as PlanUpdates. Similarly the monitorPlan operation forwards new Plans matching the subscription to the consumer.



Figure : Plan Distribution Special Operations

Two further non-mandatory operations allow more complex selection of plans.

The queryPlan operation allows the consumer to request plans based on multiple query criteria, including various header attributes and on whether the plan includes specific planning activities or events.

The getPartialPlan operation allows the consumer to request a subset of a plan, based on the domain, subPlan allocation or tags associated with the contained planning activities, as well as a period of the plan based on time, position or events.

### MO Objects

MO Objects relevant to the plan distribution service and their relationships are defined within the MPS Information Model in section 3.2.

The following MO Objects are directly applicable to the service (see Figure 21):

* Plan

The identity of Plans comprises both ID and version. Plans are created by a planning function as an output that may be passed to a plan execution function, or to another planning function in a distributed or hierarchical planning system. Where a Plan is updated due to replanning, a new version of the Plan with the same ID may be created.

Plans may be stand-alone or reference a defined pre-decessor with which they may overlap. In the latter case, a patch plan may be created which only contains the differences from the predecessor plan, and includes a reference to the target Plan which results from applying these changes to the predecessor Plan.

A selected subset of a Plan can be extracted as a PartialPlan. This is specified as a shorter period covered by the plan, or by the domain, SubPlan or tags associated with its contained planning activities.

The following MO Objects may be referenced in the context of the planning request service:

* ActivityDefinition and ActivityInstance: the ActivityInstances contained within a plan may be referenced in service operations by their associated ActivityDefinition.
* EventDefinition and EventInstance: the EventInstances contained within a plan may be referenced in service operations by their associated EventDefinition.
* Resources may be contained within a plan.
* RequestInstance: the ActivityInstances contained within a Plan reference their source planning request.

### High-Level Requirements

**Req\_4.3.3.H.10** The following set of mission planning configuration data shall be available to both provider and consumers in a any deployment of the plan distribution service:

1. Planning Activity Definitions (as ActivityDefinition objects [§3.2.2.1])
2. Planning Event Definitions (as EventDefinition objects [§3.2.3.1])
3. Planning Resource Definitions (as Resource objects [§3.2.4.1]) [Optional]
4. MPS System Configuration Data (as an MPSSysConfig object [§3.2.7])

### Functional Requirements

**Req\_4.3.4.F.11** If no Plan version is specified in the getPlan, getPlanStatus, and monitorPlanStatus operations, then the service provider shall assume the latest version of the Plan is required.

**Req\_4.3.4.F.12** In response to internal planning and feedback from external plan execution processes, the service provider shall model the status of Plan objects in accordance with the plan state model (§3.2.6.2).

### Operation: getPlanSummaries

#### Overview

The getPlanSummaries operation allows consumers to obtain a filtered list of currently available Plans. The request uses the PlanFilter structure to select the set of plans of interest, using the following keys:

* Domain of the Plan
* planID (and version) of the Plan
* precursorPlan of the Plan
* status of the Plan
* originator of the Plan
* validity period of the Plan as a time window

The response returns a list of PlanSummaryStatus structures containing the identity (ID and version), descriptive header fields and status of the Plans that match the filter.

|  |  |
| --- | --- |
| **Operation Identifier** | getPlanSummaries |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | planFilter : (PlanFilter) |
| OUT | RESPONSE | planSummaries : (List <PlanSummaryStatus>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getPlan

#### Overview

The getPlan operation is used to obtain the full content of one or more known Plans. The operation uses the Progress interaction pattern, to allow the response to be spread across multiple messages.

|  |  |
| --- | --- |
| **Operation Identifier** | getPlan |
| **Interaction Pattern** | PROGRESS |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | PROGRESS | planRefs : (List <MAL::ObjectRef[Plan]>) |
| OUT | ACK | Empty |
| OUT | UPDATE | updatePlans : (List <Plan>) |
| OUT | RESPONSE | responsePlans : (List <Plan>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getPlanStatus

#### Overview

The getPlanStatus operation is used to obtain the current status of one or more known Plans. The operation uses the Request interaction pattern.

|  |  |
| --- | --- |
| **Operation Identifier** | getPlanStatus |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | planRefs : (List <MAL::ObjectRef[Plan]>) |
| OUT | RESPONSE | responsePlans : (List <PlanUpdate>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: monitorPlanStatus

#### Overview

The monitorPlanStatus operation is used to subscribe to status updates for a filtered set of Plans. The operation uses the Publish-Subscribe interaction pattern, with the body of the notification message comprising a PlanUpdate for a subscribed Plan.

|  |  |
| --- | --- |
| **Operation Identifier** | monitorPlanStatus |
| **Interaction Pattern** | PUBLISH-SUBSCRIBE |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| OUT | PUBLISH/NOTIFY | planUpdate : (PlanUpdate) |

Other messages of the Publish-Subscribe pattern are fully defined by the MAL.

#### Structures

**Req\_4.3.8.S.13** The monitorPlanStatus subscription shall be based on the provision of the following keys of the required Plans in the Register message, all of which are nullable:

1. subDomain = domain of subscribed Plans
2. entityKeys.firstSubKey = planID of subscribed Plans
3. entityKeys.secondSubKey = precursorPlan of subscribed Plan
4. entityKeys.thirdSubKey = status of subscribed Plan
5. entityKeys.fourth SubKey = originator of subscribed Plan

Note: this assumes the current MAL limit of four entity keys. It is hoped that in the future, the publish-subscribe pattern subscription will allow the specification of an arbitrary list of key field-value pairs. Should this be extended the following additional subscription keys should be supported:

1. validityPeriod of subscribed Plan

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: monitorPlan

#### Overview

The monitorPlan operation is used by a consumer to subscribe to receive new Plans, or new versions of Plans, as they published. The operation uses the Publish-Subscribe interaction pattern, with the body of the notification message comprising a Plan.

|  |  |
| --- | --- |
| **Operation Identifier** | monitorPlan |
| **Interaction Pattern** | PUBLISH-SUBSCRIBE |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| OUT | PUBLISH/NOTIFY | plan : (Plan) |

#### Structures

**Req\_4.3.9.S.14** The monitorPlan subscription shall be based on the provision of the following keys of the required Plans in the Register message, all of which are nullable:

1. subDomain = domain of subscribed Plans
2. entityKeys.firstSubKey = planID of subscribed Plans
3. entityKeys.secondSubKey = precursorPlan of subscribed Plan
4. entityKeys.thirdSubKey = status of subscribed Plan
5. entityKeys.fourth SubKey = originator of subscribed Plan

Note: this assumes the current MAL limit of four entity keys. It is hoped that in the future, the publish-subscribe pattern subscription will allow the specification of an arbitrary list of key field-value pairs. Should this be extended the following additional subscription keys should be supported:

1. validityPeriod of subscribed Plan

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: queryPlan

#### Overview

The queryPlan operation enables a consumer to retrieve a filtered set of plans, based on an extended set of filter criteria, including relevant fields of the plan information sections of the plan, as well as the type of planning activities and planning events contained within the plan.

|  |  |
| --- | --- |
| **Operation Identifier** | queryPlan |
| **Interaction Pattern** | PROGRESS |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | PROGRESS | query : (PlanQuery) |
| OUT | ACK | Empty |
| OUT | UPDATE | updatePlans : (List <Plan>) |
| OUT | RESPONSE | responsePlans : (List <Plan>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getPartialPlan

#### Overview

The getPartialPlan operation enables a consumer to extract a subset of a Plan that meets the supplied partialPlanFilter. The filter can select the partial plan content based on:

1. A shorter period than that covered by the plan, specified by time, position or events.
2. A subset of contained ActivityInstances, based on their domain, associated SubPlan or tags.

The PartialPlan returned includes the filter criteria and a version of the plan containing only the ActivityInstances that match those criteria. It is implementation dependent what is returned in terms of Events and Resources, but it may be assumed that any related Events and Resources would be included in the returned partial plan.

|  |  |
| --- | --- |
| **Operation Identifier** | getPartialPlan |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | partialPlanFilter : (PartialPlanFilter) |
| OUT | RESPONSE | partialPlan : (PartialPlan) |

#### Structures

**Req\_4.3.11.S.15** The PartialPlan returned shall include all ActivityInstances contained in the source Plan that pass the specified PartialPlanFilter criteria.

**Req\_4.3.11.S.16** The PartialPlan returned should include all EventInstances and ResourceProfiles in the source Plan that lie within the specified period for the partial plan and which are related to the included ActivityInstances.

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

## Service: Plan Execution Control Service

### Summary

The Plan Execution Control Service, introduced in §2.5.4, is provided by a plan execution function and enables its consumers to submit (and revoke) Plans for execution; to control their execution at Plan, Sub-Plan and Activity levels; and to receive feedback on their execution status.

It comprises the following operations, of which only those in capability set 1 are mandatory.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Area Identifier | Service Identifier | Area Number | Service Number | Area Version |
| MPS | PlanExecutionControl | 42 | 3 | 1 |

| Interaction Pattern | Operation Identifier | Operation Number | Capability Set |
| --- | --- | --- | --- |
| SUBMIT | submitPlan | 1 | 1 |
| SUBMIT | revokePlan | 2 |
| REQUEST | getPlanStatus | 3 |
| REQUEST | activatePlan | 4 | 2 |
| REQUEST | deactivatePlan | 5 |
| PUBSUB | monitorPlanExecution | 6 | 3 |
| PUBSUB | monitorPlanExecutionDetail | 7 | 4 |
| REQUEST | activateSubPlan | 8 | 5 |
| REQUEST | deactivateSubPlan | 9 |
| REQUEST | getSubPlanStatus | 10 |
| PUBSUB | monitorSubPlanExecution | 11 | 6 |
| REQUEST | suspendActivity | 12 | 7 |
| REQUEST | resumeActivity | 13 |
| REQUEST | getActivityStatus | 14 | 8 |

Note: the getPlanStatus, with the exception of the service number, is identical to the operation of the same name in the Plan Distribution Service.

#### Plan Level Execution Control Operations

Four of the service operations are concerned with submission and subsequent management of plans, submitPlan and revokePlan being mandatory operations in capability set 1.

The submitPlan operation delivers a Plan to the service provider, making it available for execution. The revokePlan operation makes a previously submitted Plan unavailable for exection. Typically the service provider deletes any local copy of the Plan.

Execution of a Plan is normally a two-stage operation: first the Plan is submitted, then once it has been received by the service provider it can be activated. If the service implementation is restricted to capability set 1, then there is effectively no activation step before a plan is executed: either the plan is activated locally or is immediately activated on submission by the service provider. If an activation step is required, then capability set 2 should also be implemented.

The activatePlan operation enables execution of one or more Plans by the service provider, subject to the scheduling constraints (time, position or event-based) associated with contained planning activities in each plan.

The deactivatePlan operation disables the execution of the specified Plans, specifying a deactivation mode for the case where execution has already started. Deactivated Plans remain available to the service provider, and can be re-activated using the activatePlan operation.



Figure : Plan Execution Control Operations



Figure : Plan Execution Feedback Operations

Three service operations provide feedback on the execution of Plans, of these only the getPlanStatus operation is mandatory in capability set 1. In order to ensure provision of feedback on the execution of a plan at a sufficiently detailed level to enable feedback for planning requests, it is recommended that capability sets 2 and 3 are implemented.

The getPlanStatus operation returns the current status of the referenced plan(s) as PlanUpdates. It is equivalent to the service operation of the same name in the Plan Distribution Service, but only reports those plan statuses relevant to the plan execution function (see Figure 23).

Where supported, the monitorPlanExecution operation enables the consumer to subscribe to automatic notification of changes in status of plans as PlanUpdates. It is equivalent to the monitorPlanStatus operation of the Plan Distribution Service.

The monitorPlanExecutionDetail operation enables the consumer to subscribe to automatic notification of changes in status of the ActivityInstances, EventInstances and Resources contained within Plans, provided as ActivityUpdates, EventUpdates and ResourceUpdates respectively. Note that as resource profiles are an optional element of a Plan, ResourceUpdates are only provided where they are supported.

#### SubPlan Level Execution Control Operations

Support for SubPlans is optional, but where supported an additional 4 service operations enable control at the level of SubPlans.

Planning ActivityInstances contained within a Plan may be associated with a single SubPlan ID. This can be used as a mechanism to identify multiple subplans within plans, for example to support individual spacecraft within a constellation, or separate payloads. SubPlan IDs are not unique to an individual Plan, but apply globally to a mission planning system. SubPlan operations apply to all activated Plans managed by the service provider. Individual ActivityInstances are only executed if both their container Plan and associated SubPlan are in the ACTIVATED state.

The activateSubPlan operation enables execution of one or more SubPlans by the service provider. It is implementation dependent whether it is initially assumed that all SubPlans are active, in which case the operation would only be needed to reenable execution following a deactivateSubPlan operation.

The deactivateSubPlan operation disables execution of one or more SubPlans by the service provider.

The getSubPlanStatus operation returns the current status of the referenced SubPlans as SubPlanUpdates.

Where supported, the monitorSubPlanExecution operation enables the consumer to subscribe to automatic notification of changes in status of SubPlans as SubPlanUpdates.



Figure : SubPlan Execution Control Operations

#### Activity Level Execution Control Operations



Figure : Activity Execution Control Operations

Optional support for execution control at the level of ActivityInstances is provided by an additional 3 service operations.

Selected ActivityInstances are identified by Plan, instance ID, and/or tag. The use of tags[[1]](#footnote-1) allows arbitrary (and overlapping) groups of ActivityInstances to be managed together.

The suspendActivity operation requests suspension of the execution of selected activities, in one or more plans, without changing the state of those plans. The response gives the resulting ActivitySuspensionStatus of each referenced ActivityInstance.

The resumeActivity operation requests the resumption of previously suspended activities in one or more plans without changing the state of those plans. The response gives the resulting ActivitySuspensionStatus of each referenced ActivityInstance.

The getActivityStatus operation returns the status of ActivityInstances, as ActivityUpdates, at activity, subplan or tag level.

### MO Objects

MO Objects relevant to the plan execution control service and their relationships are defined within the MPS Information Model in section 3.2.

The following MO Objects are directly applicable to the service (see Figure 21):

* Plan
* ActivityInstance
* EventInstance
* Resource

The identity of Plans comprises both ID and version. Plans are submitted to a plan execution function for execution.

Plans contain ActivityInstances and EventInstances, the same instance of which may occur in multiple overlapping Plans or versions of Plans. Plans may also optionally contain ResourceProfiles referencing Resources.

The plan execution control service does not result in the creation of new MO Objects.

The following MO Objects may be referenced by the ActivityInstances and EventInstances contained within a Plan:

* ActivityDefinition
* EventDefinition
* RequestInstance

### High-Level Requirements

**Req\_4.4.3.H.17** The following set of mission planning configuration data shall be available to both provider and consumers in a any deployment of the plan execution control service:

1. Planning Activity Definitions (as ActivityDefinition objects [§3.2.2.1])
2. Planning Event Definitions (as EventDefinition objects [§3.2.3.1])
3. Planning Resource Definitions (as Resource objects [§3.2.4.1]) [Optional]
4. MPS System Configuration Data (as an MPSSysConfig object [§3.2.7])

### Functional Requirements

**Req\_4.4.4.F.18** In response to a submitPlan operation, the service provider shall make the submitted Plan available for execution.

**Req\_4.4.4.F.19** If the service does not support plan activation (capability set 2), the service provider shall provide an internal mechanism to activate submitted Plans.

Note: this may be as simple as to automatically activate Plans on submission.

**Req\_4.4.4.F.20** In response to a revokePlan operation, the service provider shall make the submitted Plan unavailable for execution. If this is not possible (for example, if the plan has already executed), then a REVOKE\_FAILED error shall be returned.

**Req\_4.4.4.F.21** In response to internal plan execution processes, the service provider shall model the status of Plans in accordance with the plan state model (§3.2.6.2).

**Req\_4.4.4.F.22** In response to an activatePlan operation, or internal plan activation where not supported, the service provider shall enable the execution of the referenced Plans and the ActivityInstances contained within them, subject to the scheduling constraints specified within the Plans.

**Req\_4.4.4.F.23** In response to an activatePlan operation, if a referenced Plan overlaps with its already activated predecessor Plan, then the service provider should merge plan revisions into the currently active Plan.

Note: it is implementation dependent whether overlapping Plans are supported and how this is managed internally by the plan execution function. However, it is common for successive iterations of a Plan to overlap, for example with a Plan being generated daily for the coming week. In this case, the same ActivityInstance may appear in the overlap period of both Plans, and may be unchanged, modified or deleted in the successor Plan. New ActivityInstances may also be inserted in the overlap period or in the extended period covered by the successor Plan. It is anticipated that when the successor Plan is activated, then its predecessor is superseded from the start point of the successor Plan with any revisions applicable to the overlap period being applied. Only the latest revision of the ActivityInstance is executed.

**Req\_4.4.4.F.24** In response to an activatePlan operation, if a referenced Plan is a Patch Plan, then the service provider shall merge the plan revisions it contains with its predecessor Plan to reconstitute the target Plan prior to its activation.

Note: if the predecessor Plan is already activated, then the Patch Plan can be mergered into the currently active Plan. If the predecessor Plan is not available, then the operation cannot be performed.

**Req\_4.4.4.F.25** In response to a deactivatePlan operation, if supported, the service provider shall disable the execution of the referenced Plans and the ActivityInstances contained within them, subject to the specified deactivationMode.

Note: supported deactivationModes are specific to the implementation of the service provider.

**Req\_4.4.4.F.26** If no Plan version is specified in the getPlanStatus, monitorPlanExecution and monitorPlanExecutionDetail operations, then the service provider shall assume the latest version of the Plan is required.

**Req\_4.4.4.F.27** If the monitorPlanExecutionDetail operation (or activity level operations) are supported, then in response to internal plan execution processes, the service provider shall model the status of ActivityInstances and EventInstances in accordance with their respective state models (§3.2.2.2 and §3.2.3.2).

**Req\_4.4.4.F.28** If the monitorPlanExecutionDetail operation is supported, the service provider may model the evolving value of planning Resources in accordance with the ResourceProfiles (§3.2.4.2) defined within Plans and any Effects (§3.3.6.2) associated with ActivityInstances.

**Req\_4.4.4.F.29** If SubPlans are supported, the service provider shall maintain the current status of SubPlans as ACTIVATED or DEACTIVATED.

**Req\_4.4.4.F.30** In response to an activateSubPlan operation, if supported, the service provider shall activate the referenced SubPlans and enable the execution of ActivityInstances that are contained in activated Plans and allocated to activated SubPlans.

Note: it is implementation dependent whether SubPlans are initially ACTIVATED and therefore do not require activation unless previously deactivated.

**Req\_4.4.4.F.31** In response to a deactivateSubPlan operation, if supported, the service provider shall deactivate the referenced SubPlans and disable the execution of ActivityInstances that are contained in activated Plans and allocated to deactivated SubPlans, subject to the specified deactivationMode.

Note: supported deactivationModes are specific to the implementation of the service provider.

**Req\_4.4.4.F.32** In response to a suspendActivity operation, if supported, the service provider shall suspend the execution of referenced ActivityInstances, subject to the specified suspensionMode.

Note: supported suspensionModes are specific to the implementation of the service provider.

**Req\_4.4.4.F.33** In response to a resumeActivity operation, if supported, the service provider shall resume the execution of the referenced ActivityInstances where it is safe to do so.

### Operation: submitPlan

#### Overview

The submitPlan operation is used to send a plan to a plan execution function (the service provider), making it available for execution. The service provider acknowledges the reception of the plan or returns an error.

Note: the submitted plan may be a full plan or a patch plan.

|  |  |
| --- | --- |
| **Operation Identifier** | submitPlan |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | plan : (Plan) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: revokePlan

#### Overview

The revokePlan operation is used to request a plan execution function to revoke a previously submitted Plan, making it unavailable for execution. The service provider acknowledges the revocation of the Plan or returns an error.

|  |  |
| --- | --- |
| **Operation Identifier** | revokePlan |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | planRef : (MAL::ObjectRef[Plan]) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* REVOKE\_FAILED

### Operation: getPlanStatus

#### Overview

The getPlanStatus operation is used to obtain the current status of one or more known Plans that have been previously submitted to a plan execution function.

|  |  |
| --- | --- |
| **Operation Identifier** | getPlanStatus |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | planRefs : (List <MAL::ObjectRef[Plan]>) |
| OUT | RESPONSE | planStatus : (List <PlanUpdate>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: activatePlan

#### Overview

The activatePlan operation is used to request the execution of specified Plans that have previously been submitted to a plan execution function. The service provider enables the execution of the referenced Plans and the ActivityInstances contained within them, subject to the scheduling constraints specified within the Plans.

Note: Multiple plans with a common predecessor may have been submitted to a plan execution function. Usually only one of these is considered the nominal plan, the other alternative or contingency plans having the isAlternate flag set. It is implementation dependent whether the service provider will allow activation of Plans that have the isAlternate flag set, but this may be blocked for operational safety. Where this is the case, the plan edit service can be used to change the state of the isAlternate flag prior to activation (see §4.6.5).

If a specified Plan is a patch plan, then the service provider merges the plan revisions it contains with its predecessor Plan to reconstitute the target Plan. If the predecessor plan is already active, then the changes can be merged into the active plan, but if it is not active then the the reconstitution of the target Plan must take place prior to activation. If the predecessor plan has not previously been submitted to the service provider (or has been revoked), then it is not possible to activate the patch plan.

|  |  |
| --- | --- |
| **Operation Identifier** | activatePlan |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | planRefs : (List <MAL::ObjectRef[Plan]>) |
| OUT | RESPONSE | activationStatus : (List <PlanActivationStatus>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: deactivatePlan

#### Overview

The deactivatePlan operation is used to request deactivation of specified Plans that have previously been activated. The service provider disables the execution of the referenced Plans and the ActivityInstances contained within them, where it is possible to do so.

The deactivationMode argument allows selection of the deactivation behaviour. For example:

* Orderly (ceases execution of any new Activities, but allows those already initiated to complete)
* Rapid (ceases execution of the Plan, but allows Activities already initiated to continue until their next defined breakpoint)
* Immediate (ceases execution of the Plan and all Activities currently in progress).

Note that it is dependent on the service provider implementation which deactivationModes are supported, and that the above list is not exhaustive.

The service provider returns a list of PlanActivationStatus data structures comprising Plan status and activationInfo as a String for each Plan in the deactivation list. The activationInfo allows the return of deployment specific details on the deactivation, such as the deactivation mode applied or reasons for a failure to deactivate.

|  |  |
| --- | --- |
| **Operation Identifier** | deactivatePlan |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | planRefs : (List <MAL::ObjectRef[Plan]>)  deactivationMode : (MAL::String) |
| OUT | RESPONSE | activationStatus : (List <PlanActivationStatus>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: monitorPlanExecution

#### Overview

The monitorPlanExecution operation is used to subscribe to status updates for a filtered set of Plans that have been submitted to a plan execution function. The operation uses the Publish-Subscribe interaction pattern, with the body of the notification message comprising a PlanUpdate for a subscribed Plan.

The operation is equivalent to the monitorPlanStatus operation of the Plan Distribution Service, but only reports the status of plans currently being managed by a plan execution function.

|  |  |
| --- | --- |
| **Operation Identifier** | monitorPlanExecution |
| **Interaction Pattern** | PUBLISH-SUBSCRIBE |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| OUT | PUBLISH/NOTIFY | planUpdate : (PlanUpdate) |

#### Structures

**Req\_4.4.10.S.34** The monitorPlanExecution subscription shall be based on the provision of the following keys of the required Plans in the Register message, all of which are nullable:

1. subDomain = domain of subscribed Plans
2. entityKeys.firstSubKey = planID of subscribed Plans
3. entityKeys.secondSubKey = precursorPlan of subscribed Plan
4. entityKeys.thirdSubKey = status of subscribed Plan
5. entityKeys.fourth SubKey = originator of subscribed Plan

Note: this assumes the current MAL limit of four entity keys. It is hoped that in the future, the publish-subscribe pattern subscription will allow the specification of an arbitrary list of key field-value pairs. Should this be extended the following additional subscription keys should be supported:

1. validityPeriod of subscribed Plan

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: monitorPlanExecutionDetail

#### Overview

The monitorPlanExecutionDetail operation is used to subscribe to updates that report changes in the detailed execution status for a filtered set of Plan contents at the level of planning activities, events and resources. A planning function requires feedback at the level of planning activities and events to be able to reconstitute the status of planning requests, as well to support re-planning. The operation uses the Publish-Subscribe interaction pattern.

It is implementation dependent which details are reported on, but this may be any combination of planning activities, events and resources. The changing status of each of these items is reported using its own dedicated notification structure.

|  |  |
| --- | --- |
| **Operation Identifier** | monitorPlanExecutionDetail |
| **Interaction Pattern** | PUBLISH-SUBSCRIBE |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| OUT | PUBLISH/NOTIFY | activityUpdate : (ActivityUpdate) |
| OUT | PUBLISH/NOTIFY | eventUpdate : (EventUpdate) |
| OUT | PUBLISH/NOTIFY | resourceUpdate : (ResourceUpdate) |

#### Structures

**Req\_4.4.11.S.35** The monitorPlanExecutionDetail subscription shall be based on the provision of the following keys of the required Plans in the Register message, all of which are nullable:

1. subDomain = domain of subscribed Plans
2. entityKeys.firstSubKey = planID of subscribed Plans
3. entityKeys.secondSubKey = subPlan of subscribed ActivityInstances
4. entityKeys.thirdSubKey = tags of subscribed ActivityInstances
5. entityKeys.fourth SubKey = not used

**Req\_4.4.11.S.36** The service provider shall publish a combination of ActivityUpdates, EventUpdates and ResourceUpdates.

Note: it is implementation dependent which types of update are supported by the service provider.

**Req\_4.4.11.S.37** If the subscription includes subPlan or tags keys, then the consumer shall only be notified of updates to ActivityInstances associated with the specified subPlan or keys. If the service provider supports EventUpdates and/or ResourceUpdates then these should be notified irrespective of subscription by subPlan or tag.

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: activateSubPlan

#### Overview

The activateSubPlan operation is used to request that the service provider activates the referenced SubPlans and enables the execution of ActivityInstances that are contained in activated Plans and allocated to activated SubPlans.

Note: it is implementation dependent whether SubPlans are initially ACTIVATED and therefore do not require activation unless previously deactivated.

|  |  |
| --- | --- |
| **Operation Identifier** | activateSubPlan |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | subPlanIDs : (List <MAL::Identifier[SubPlan]>) |
| OUT | RESPONSE | activationStatus : (List <SubPlanActivationStatus>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: deactivateSubPlan

#### Overview

The deactivateSubPlan operation is used to request that the service provider deactivates the referenced SubPlans and disables the execution of ActivityInstances that are contained in activated Plans and allocated to the deactivated SubPlans, where it is possible to do so.

The deactivationMode argument allows selection of the deactivation behaviour. For example:

* Orderly (ceases execution of any new Activities, but allows those already initiated to complete)
* Rapid (ceases execution of the Sub-plan, but allows Activities already initiated to continue until their next defined breakpoint)
* Immediate (ceases execution of the Sub-plan and all Activities currently in progress).

Note that it is dependent on the service provider implementation which deactivationModes are supported, and that the above list is not exhaustive.

The service provider returns a list of SubPlanActivationStatus data structures comprising sub-plan status and activationInfo as a String for each sub-plan in the deactivation list. The activationInfo allows the return of deployment specific details on the deactivation, such as the deactivation mode applied or reasons for a failure to deactivate.

|  |  |
| --- | --- |
| **Operation Identifier** | deactivateSubPlan |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | subPlanIDs : (List <MAL::Identifier[SubPlan]>)  deactivationMode : (MAL::String) |
| OUT | RESPONSE | activationStatus : (List <SubPlanActivationStatus>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getSubPlanStatus

#### Overview

The getSubPlanStatus operation is used to obtain the current status of one or more SubPlans.

|  |  |
| --- | --- |
| **Operation Identifier** | getPlanStatus |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | subPlanIDs : (List <MAL::Identifier[SubPlan]>) |
| OUT | RESPONSE | subPlanStatus : (List <SubPlanUpdate>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: monitorSubPlanExecution

#### Overview

The monitorSubPlanExecution operation is used to subscribe to status updates for a filtered set of SubPlans. The operation uses the Publish-Subscribe interaction pattern, with the body of the notification message comprising a SubPlanUpdate for a subscribed sub-plan.

|  |  |
| --- | --- |
| **Operation Identifier** | monitorSubPlanExecution |
| **Interaction Pattern** | PUBLISH-SUBSCRIBE |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| OUT | PUBLISH/NOTIFY | subPlanUpdate : (SubPlanUpdate) |

#### Structures

**Req\_4.4.15.S.38** The monitorSubPlanExecution subscription shall be based on the provision of the following keys of the required SubPlans in the Register message, all of which are nullable:

1. subDomain = domain of subscribed SubPlans
2. entityKeys.firstSubKey = subPlanID of subscribed Plans
3. entityKeys.secondSubKey = not used
4. entityKeys.thirdSubKey = not used
5. entityKeys.fourth SubKey = not used

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: suspendActivity

#### Overview

The suspendActivity operation is used to request suspension of the execution of selected activities in one or more plans, without changing the state of the plan(s).

The suspentionMode argument allows selection of the suspension behaviour. For example:

* Orderly (suspends execution of any new Activities, but allows those already initiated to complete)
* Rapid (suspends execution of any new Activities, but allows any Activities and their Sub-activities already initiated to continue until their next defined breakpoint)
* Immediate (suspends execution of all Activities, including those currently in progress).

Note that it is dependent on the service provider implementation which deactivationModes are supported, and that the above list is not exhaustive.

The service provider responds with a list of ActivitySuspensionStatus data structures comprising activity status and suspensionInfo (as a String) for each Activity subject to the suspension request.

The suspensionInfo allows the return of deployment specific details on the suspension, such as the suspension mode applied or reasons for a failure to suspend.

|  |  |
| --- | --- |
| **Operation Identifier** | suspendActivity |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | planRefs : (List <MAL::ObjectRef[Plan]>)  activityRefs : (List <MAL::ObjectRef[ActivityInstance]>)  tags : (List <MAL::String>)  suspensionMode : (MAL::String) |
| OUT | RESPONSE | suspensionStatus : (List <ActivitySuspensionStatus>) |

#### Structures

**Req\_4.4.16.S.39** The ActivityInstances to be suspended shall be specified in the request message of the suspendActivity operation, by the following fields, each of which is nullable:

1. planRefs
2. activityRefs
3. tags (associated with ActivityInstances to be suspended).

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: ResumeActivity

#### Overview

The resumeActivity operation is used to request resumption of the execution of selected activities in one or more plans, without changing the state of the plan(s).

The service provider responds with a list of ActivitySuspensionStatus data structures comprising activity status and suspensionInfo (as a String) for each Activity subject to the resumption request.

The suspensionInfo allows the return of deployment specific details on the resumption, such as the reasons for a failure to resume.

|  |  |
| --- | --- |
| **Operation Identifier** | resumeActivity |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | planRefs : (List <MAL::ObjectRef[Plan]>)  activityRefs : (List <MAL::ObjectRef[ActivityInstance]>)  tags : (List <MAL::String>) |
| OUT | RESPONSE | suspensionStatus : (List <ActivitySuspensionStatus>) |

#### Structures

**Req\_4.4.17.S.40** The ActivityInstances to be resumed shall be specified in the request message of the resumeActivity operation, by the following fields, each of which is nullable:

1. planRefs
2. activityRefs
3. tags (associated with ActivityInstances to be resumed).

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getActivityStatus

#### Overview

The getActivityStatus operation is used to request a detailed report from the service provider on the current status of ActivityInstances, selected at activity, sub-plan or tag levels.

|  |  |
| --- | --- |
| **Operation Identifier** | getActivityStatus |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | planRefs : (List <MAL::ObjectRef[Plan]>)  activityRefs : (List <MAL::ObjectRef[Activity]>)  subPlans : (List <MAL::Identifier[SubPlan]>)  tags : (List <MAL::String>) |
| OUT | RESPONSE | activityStatus : (List <ActivityUpdate>) |

#### Structures

**Req\_4.4.18.S.41** The ActivityInstances whose status is to be reported shall be specified in the request message of the getActivityStatus operation, by the following fields, each of which is nullable:

1. planRefs
2. activityRefs
3. subPlans (associated with ActivityInstances to be reported)
4. tags (associated with ActivityInstances to be reported).

Note: it is implementation dependent what is reported if none of the above are provided (all ActivityInstances or none).

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

## Service: Plan Information Management Service

### Summary

The Plan Information Management Service, introduced in §2.5.5, is provided by a planning function and enables its consumers to list and retrieve available MPS configuration data. This includes definitions for planning requests, planning activities, planning events and planning resources, and also MPS system configuration data. The service may also be provided by a plan execution function (excluding planning request definitions). It comprises the following operations, none of which are mandatory.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Area Identifier | Service Identifier | Area Number | Service Number | Area Version |
| MPS | PlanInformationManagement | 42 | 4 | 1 |

| Interaction Pattern | Operation Identifier | Operation Number | Capability Set |
| --- | --- | --- | --- |
| PROGRESS | listRequestDefs | 1 | 1 |
| REQUEST | getRequestDef | 2 |
| PROGRESS | listEventDefs | 3 | 2 |
| REQUEST | getEventDef | 4 |
| PROGRESS | listActivityDefs | 5 | 3 |
| REQUEST | getActivityDef | 6 |
| PROGRESS | listResourceDefs | 7 | 4 |
| REQUEST | getResourceDef | 8 |
| REQUEST | getSystemConfig | 9 | 5 |



Figure : Plan Information Management Operations for Generic Data Item

Each of the first four capability sets corresponds to a particular type of MPS data item and comprises two operations:

1. listDefs: request a list of available definitions, filtered by domain and/or ID;
2. getDef: obtain the full definitions for a specified set of definition IDs.

The first enables a consumer to discover which definitions are available, and the second enables their retrieval.

The fifth capability set comprises a single operation to retrieve the MPS system configuration data: MPSSystemConfig.

### MO Objects

MO Objects relevant to the plan information management service and their relationships are defined within the MPS Information Model in chapter 3, and specifically identified as planning configuration data in §3.2.7.

The following MO Objects are applicable to the service (see Figure 25):

* RequestDefinition
* ActivityDefinition
* EventDefinition
* Resource [Definition]
* MPSSystemConfig

Each definition has its own ID and version, except for MPSSystemConfig which as a singleton object only has versions.

In the case of planning Resources, the definition may omit the value attribute, although it may also be used to provide a default or initial value.

### High-Level Requirements

**Req\_4.5.3.H.42** The following set of mission planning configuration data shall be available to the provider in a any deployment of the plan information management service:

1. Planning Request Definitions (as RequestDefinition objects [§3.2.5.1] )
2. Planning Activity Definitions (as ActivityDefinition objects [§3.2.2.1])
3. Planning Event Definitions (as EventDefinition objects [§3.2.3.1])
4. Planning Resource Definitions (as Resource objects [§3.2.4.1]) [Optional]
5. MPS System Configuration Data (as an MPSSysConfig object [§3.2.7])

### Functional Requirements

**Req\_4.5.4.F.43** If no version is specified for the definition to be retrieved in a listItem]Defs or operation then the service provider shall list all available versions of the definition.

**Req\_4.5.4.F.44** If no version is specified for the definition to be retrieved in a get[Item]Defs or getSystemConfig operation then the service provider shall return the latest available version of the definition.

### Operation: listRequestDefs

#### Overview

The listRequestDefs operation is used to obtain a list of available RequestDefinitions (ID and version) together with their descriptions. The list can be filtered by domain or restricted to specified definition IDs. All available versions are listed.

|  |  |
| --- | --- |
| **Operation Identifier** | listRequestDefs |
| **Interaction Pattern** | PROGRESS |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | PROGRESS | domains : (List <MAL::Identifier[Domain]>)  requestDefs : (List <MAL::ObjectRef[RequestDefinition]>) |
| OUT | ACK | Empty |
| OUT | UPDATE | updateRequestDefs : (List <DefListEntry>) |
| OUT | RESPONSE | responseRequestDefs : (List <DefListEntry>) |

#### Structures

**Req\_4.5.5.S.45** The RequestDefinitions to be listed shall be specified in the request message of the listRequestDefs operation, by the following fields, each of which is nullable:

1. domains
2. requestDefs..

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getRequestDefs

#### Overview

The getRequestDefs operation is used to retrieve one or more available RequestDefinitions, whose identity is known to the consumer.

|  |  |
| --- | --- |
| **Operation Identifier** | getRequestDefs |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | requestDefs: (List <MAL::ObjectRef[RequestDefinition]>) |
| OUT | RESPONSE | definitions : (List <RequestDefinition>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: listEventDefs

#### Overview

The listEventDefs operation is used to obtain a list of available EventDefinitions (ID and version) together with their descriptions. The list can be filtered by domain or restricted to specified definition IDs. All available versions are listed.

|  |  |
| --- | --- |
| **Operation Identifier** | listEventDefs |
| **Interaction Pattern** | PROGRESS |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | PROGRESS | domains : (List <MAL::Identifier[Domain]>)  eventDefs : (List <MAL::ObjectRef[EventDefinition]>) |
| OUT | ACK | Empty |
| OUT | UPDATE | updateEventDefs : (List <DefListEntry>) |
| OUT | RESPONSE | responseEventDefs : (List <DefListEntry>) |

#### Structures

**Req\_4.5.7.S.46** The EventDefinitions to be listed shall be specified in the request message of the listEventDefs operation, by the following fields, each of which is nullable:

1. domains
2. eventDefs.

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getEventDefs

#### Overview

The getEventDefs operation is used to retrieve one or more available EventDefinitions, whose identity is known to the consumer.

|  |  |
| --- | --- |
| **Operation Identifier** | getEventDefs |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | eventDefs: (List <MAL::ObjectRef[EventDefinition]>) |
| OUT | RESPONSE | definitions : (List <EventDefinition>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: listActivityDefs

#### Overview

The listActivityDefs operation is used to obtain a list of available ActivityDefinitions (ID and version) together with their descriptions. The list can be filtered by domain or restricted to specified definition IDs. All available versions are listed.

|  |  |
| --- | --- |
| **Operation Identifier** | listActivityDefs |
| **Interaction Pattern** | PROGRESS |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | PROGRESS | domains : (List <MAL::Identifier[Domain]>)  activityDefs : (List <MAL::ObjectRef[ActivityDefinition]>)  defaultTags : (List<MAL::String>) |
| OUT | ACK | Empty |
| OUT | UPDATE | updateActivitytDefs : (List <DefListEntry>) |
| OUT | RESPONSE | responseActivityDefs : (List <DefListEntry>) |

#### Structures

**Req\_4.5.9.S.47** The ActivityDefinitions to be listed shall be specified in the request message of the listActivityDefs operation, by the following fields, each of which is nullable:

1. domain
2. activityDefs
3. defaultTags (associated with ActivityDefinitions to be included).

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getActivityDefs

#### Overview

The getActivityDefs operation is used to retrieve one or more available ActivityDefinitions, whose identity is known to the consumer.

|  |  |
| --- | --- |
| **Operation Identifier** | getActivityDefs |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | activityDefs: (List <MAL::ObjectRef[ActivityDefinition]>) |
| OUT | RESPONSE | definitions : (List <ActivityDefinition>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: listResourceDefs

#### Overview

The listResourceDefs operation is used to obtain a list of available Resources (ID and version) together with their descriptions. The list can be filtered by domain or restricted to data types. All available versions are listed.

|  |  |
| --- | --- |
| **Operation Identifier** | listResourceDefs |
| **Interaction Pattern** | PROGRESS |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | PROGRESS | domains : (List <MAL::Identifier[Domain]>)  dataType : (List <MAL::AttributeType>) |
| OUT | ACK | Empty |
| OUT | UPDATE | updateResourceDefs : (List <DefListEntry>) |
| OUT | RESPONSE | responseResourceDefs : (List <DefListEntry>) |

#### Structures

**Req\_4.5.11.S.48** The Resources to be listed shall be specified in the request message of the listResourceDefs operation, by the following fields, each of which is nullable:

1. domains
2. dataType: list of Resource data types to be included.

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getResourceDefs

#### Overview

The getResourceDefs operation is used to retrieve the definition of one or more available Resources, whose identity is known to the consumer.

Note that this operation is designed to retrieve the resource definition and not the current value of the resource (the value field may contain a default value for the resource).

|  |  |
| --- | --- |
| **Operation Identifier** | getResourceDefs |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | resources: (List <MAL::ObjectRef[Resource]>) |
| OUT | RESPONSE | definitions : (List <Resource>) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

### Operation: getSystemConfig

#### Overview

The getSystemConfig operation is used to retrieve system configuration data relating to the MPS System.

|  |  |
| --- | --- |
| **Operation Identifier** | getSystemConfig |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | version: MAL::Version |
| OUT | RESPONSE | systemConfig : (MPSSystemConfig) |

#### Structures

**Req\_4.5.13.S.49** The version field of the getSystemConfig operation request message body shall reference the required version of the MPSSystemConfig object.

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID

## Service: Plan Edit Service

### Summary

The Plan Edit Service, introduced in §2.5.6, is provided by a plan execution function and enables its consumers to modify Plans that have already been submitted for execution. It allows an external user or function to update the status of the Plan; insert, modify or delete its constituent ActivityInstances and EventInstances; update the value of Resources; and apply a time shift to a Plan. It comprises the following operations, of which those in capability sets 1 and 2 are mandatory.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Area Identifier | Service Identifier | Area Number | Service Number | Area Version |
| MPS | PlanEdit | 42 | 5 | 1 |

| Interaction Pattern | Operation Identifier | Operation Number | Capability Set |
| --- | --- | --- | --- |
| SUBMIT | updatePlanStatus | 1 | 1 |
| REQUEST | insertActivity | 2 | 2 |
| REQUEST | insertEvent | 3 |
| SUBMIT | deleteActivity | 4 |
| SUBMIT | deleteEvent | 5 |
| SUBMIT | updateActivity | 6 | 3 |
| SUBMIT | updateEvent | 7 |
| SUBMIT | updateResource | 8 | 4 |
| SUBMIT | updateResourceProfile | 9 | 5 |
| SUBMIT | applyTimeShift | 10 | 6 |

The updatePlanStatus operation allows the service consumer to modify the status of a previously submitted Plan, including the isAlternate flag.



Figure : Plan Edit Operations for Generic Data Item (Activity or Event)

For planning activities and events, three operations are defined for each item type to insert, optionally to update, and to delete an ActivityInstance or EventInstance in a referenced Plan that has previously been submitted to a plan execution function (the service provider). The insert operation results in the creation by the service provider of a new ActivityInstance or EventInstance in the specified Plan. A reference to the new instance (ID and version) is returned in the response message.

For planning resources, if supported, it is only possible to update the value of the Resource. This is supported in two ways, as two distinct operations:

* updateResource: a discrete update to a specified value at a specified instant of time.
* updateResourceProfile: a revised profile covering a period of time.

The applyTimeShift operation is a special operation that allows the timings contained in an entire Plan, or selected SubPlans to be shifted by a specified offset.

### MO Objects

MO Objects relevant to the plan edit service and their relationships are defined within the MPS Information Model in section 3.2.

The following MO Objects are directly applicable to the service (see Figure 21):

* Plan
* ActivityInstance
* EventInstance
* Resource

The identity of Plans comprises both ID and version. Plans must have been previously submitted to a plan execution function for execution (using the plan execution control service).

Plans contain ActivityInstances and EventInstances, the same instance of which may occur in multiple overlapping Plans or versions of Plans. Plans may also optionally contain ResourceProfiles referencing Resources.

The insertActivity and insertEvent operations of the plan edit service result in creation of new ActivityInstances and EventInstances respectively. Deletion of ActivityInstances and EventInstances does not necessarily result in their removal from the plan execution function, but rather their transition to a terminated state.

The following MO Objects may be referenced by the ActivityInstances and EventInstances contained within a Plan and plan edit service operations:

* ActivityDefinition
* EventDefinition

### High-Level Requirements

**Req\_4.6.3.H.50** The following set of mission planning configuration data shall be available to both provider and consumers in a any deployment of the plan edit service:

1. Planning Activity Definitions (as ActivityDefinition objects [§3.2.2.1])
2. Planning Event Definitions (as EventDefinition objects [§3.2.3.1])
3. Planning Resource Definitions (as Resource objects [§3.2.4.1]) [Optional]
4. MPS System Configuration Data (as an MPSSysConfig object [§3.2.7])

### Functional Requirements

**Req\_4.6.4.F.51** In response to an updatePlanStatus operation, the service provider shall update the isAlternate flag of the Plan accordingly and apply any change to Plan status consistently with the plan state model (§3.2.6.2).

Note: it is implementation dependent what the service provider does in the event of a Plan status change when the Plan has executing ActivityInstances. It is recommended that the plan execution control service is used to manage Plan deactivation in an orderly manner.

**Req\_4.6.4.F.52** In response to an insertActivity operation, the service provider shall create a new ActivityInstance in the referenced Plan and return its identity to the consumer.

**Req\_4.6.4.F.53** In response to an insertEvent operation, the service provider shall create a new EventInstance in the referenced Plan and return its identity to the consumer.

**Req\_4.6.4.F.54** In response to a deleteActivity operation, the service provider shall transition the referenced ActivityInstance to the TERMINATED state.

Note: if the ActivityInstance is in the EXECUTING state, then it is implementation dependent what action is taken by the service provider.

**Req\_4.6.4.F.55** In response to a deleteEvent operation, the service provider shall transition the referenced EventInstance to the TERMINATED state.

Note: this may also affect any ActivityInstances whose start or end trigger is linked to the deleted EventInstance as a terminated event will not result in the activity being triggered.

**Req\_4.6.4.F.56** In response to an updateActivity operation, the service provider shall apply the changes contained in the ActivityUpdate to the referenced ActivityInstance.

**Req\_4.6.4.F.57** In response to an updateEvent operation, the service provider shall apply the changes contained in the EventUpdate to the referenced EventInstance.

**Req\_4.6.4.F.58** In response to an updateResource operation, the service provider shall apply the changes contained in the ResourceUpdate to the referenced Resource.

**Req\_4.6.4.F.59** In response to an updateResourceProfile operation, the service provider shall apply the supplied ResourceProfile to the referenced Resource.

**Req\_4.6.4.F.60** In response to an applyTimeShift operation, the service provider shall apply the specified time shift to the unexpired (future) content, or the specified time period of the referenced Plan or its SubPlan(s), including temporal start and end triggers on ActivityInstances.

Note: it is implementation dependent whether any other elements of the Plan are time shifted, particularly with regard to the eventTime of EventInstances and, where supported, the start and end times on resource ProfileSegments and the times on Profile Entries.

### Operation: updatePlanStatus

#### Overview

The updatePlanStatus operation may be used to modify the status of a previously submitted Plan. Directly modifying the status field of a Plan may be used by a third party function to autonomously terminate (or activate) a Plan, but the operation also allows the isAlternate flag to be set or cleared.

It is implementation dependent what action the service provider takes in response to a change of Plan status. The service provider may not permit certain state changes (for example to modify the status of a TERMINATED plan, which is inconsistent with the plan status model), in which case an UPDATE\_FAILED error is returned.

A set of Plans with a common predecessor may be submitted to a plan execution function to cater for alternative or contingency scenarios. All but one of these Plans should have the isAlternate flag set, to inform the plan execution function (and the mission operations team) which is the nominal Plan. It is implementation dependent whether a plan execution control service provider will allow a Plan to be activated with the isAlternate flag set, but for operational safety reasons this may be blocked. In a contingency scenario, the updatePlanStatus operation can be used to set the flag on the nominal Plan, and reset the flag on the required contingency Plan, making it operational.

|  |  |
| --- | --- |
| **Operation Identifier** | updatePlanStatus |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | planRef : (MAL::ObjectRef[Plan])  status : (PlanStatus)  isAlternate : (MAL::Boolean) |

#### Structures

**Req\_4.6.5.S.61** The status and isAlternate fields of the updatePlanStatus submit message shall both be nullable, but one must be present.

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* UPDATE\_FAILED

### Operation: insertActivity

#### Overview

The insertActivity operation sends an InsertedActivityDetails structure (an ActivityDetails structure with Plan reference and start/end triggers) to the provider, which then creates a corresponding ActivityInstance object in the referenced Plan and returns its identity to the consumer.

Insertion may fail if the Plan is already in the TERMINATED state, in which case an INSERT\_FAILED error is returned.

|  |  |
| --- | --- |
| **Operation Identifier** | insertActivity |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | activityDetails: (InsertedActivityDetails) |
| OUT | RESPONSE | activityRef : (MAL::ObjectRef[ActivityInstance]) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* INSERT\_FAILED

### Operation: insertEvent

#### Overview

The insertEvent operation sends an InsertedEventDetails structure, which includes a Plan reference, to the provider, which then creates a corresponding EventInstance object in the referenced Plan and returns its identity to the consumer.

Insertion may fail if the Plan is already in the TERMINATED state, in which case an INSERT\_FAILED error is returned.

|  |  |
| --- | --- |
| **Operation Identifier** | insertEvent |
| **Interaction Pattern** | REQUEST |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | REQUEST | eventDetails: (InsertedEventDetails) |
| OUT | RESPONSE | eventRef : (MAL::ObjectRef[EventInstance]) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* INSERT\_FAILED

### Operation: deleteActivity

#### Overview

The deleteActivity operation requests that a specified ActivityInstance within a Plan is deleted by the service provider. In practice, the activity is not removed, but transitioned to the TERMINATED state with deletion indicated in the terminationInfo field. The ActivityInstance is not subsequently executed by the service provider, but it is implementation dependent what action is taken by the service provider if the ActivityInstance is in the EXECUTING state.

Deletion may fail if the referenced Plan or ActivityInstance is already in the TERMINATED state, in which case the DELETE\_FAILED error is returned.

|  |  |
| --- | --- |
| **Operation Identifier** | deleteActivity |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | planRef : (MAL::ObjectRef[Plan])  activityRef : (MAL::ObjectRef[ActivityInstance]) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* DELETE\_FAILED

### Operation: deleteEvent

#### Overview

The deleteEvent operation requests that a specified EventInstance within a Plan is deleted by the service provider. In practice, the event is not removed, but transitioned to the TERMINATED state with deletion indicated in the terminationInfo field. The EventInstance is not subsequently triggered by the service provider.

Deletion may fail if the referenced Plan or EventInstance is already in the TERMINATED state, in which case the DELETE\_FAILED error is returned.

|  |  |
| --- | --- |
| **Operation Identifier** | deleteEvent |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | planRef : (MAL::ObjectRef[Plan])  eventRef : (MAL::ObjectRef[EventInstance]) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* DELETE\_FAILED

### Operation: updateActivity

#### Overview

The updateActivity operation may be used to modify an ActivityInstance in a Plan that has already been submitted to the service provider. The consumer submits an ActivityUpdate structure which is applied by the service provider to the referenced ActivityInstance.

Update may fail if the referenced Plan or ActivityInstance is already in the TERMINATED state, in which case the UPDATE\_FAILED error is returned.

|  |  |
| --- | --- |
| **Operation Identifier** | updateActivity |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | planRef : (MAL::ObjectRef[Plan])  activityUpdate : (ActivityUpdate) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* UPDATE\_FAILED

### Operation: updateEvent

#### Overview

The updateEvent operation may be used to modify an EventInstance in a Plan that has already been submitted to the service provider. The consumer submits an EventUpdate structure which is applied by the service provider to the referenced EventInstance.

Update may fail if the referenced Plan or EventInstance is already in the TERMINATED state, in which case the UPDATE\_FAILED error is returned.

|  |  |
| --- | --- |
| **Operation Identifier** | updateEvent |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | planRef : (MAL::ObjectRef[Plan])  eventUpdate : (EventUpdate) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* UPDATE\_FAILED

### Operation: updateResource

#### Overview

The updateResource operation may be used to modify the value of a Resource at the specified point in time, in a Plan that has already been submitted to the service provider. The consumer submits an ResourceUpdate structure which is applied by the service provider to the referenced Resource.

Update may fail if the referenced Plan is already in the TERMINATED state, in which case the UPDATE\_FAILED error is returned.

|  |  |
| --- | --- |
| **Operation Identifier** | updateResource |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | planRef : (MAL::ObjectRef[Plan])  resourceUpdate : (ResourceUpdate) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* UPDATE\_FAILED

### Operation: updateResourceProfile

#### Overview

The updateResourceProfile operation may be used to modify the value of a Resource over a period of time, in a Plan that has already been submitted to the service provider. The consumer submits an ResourceProfile structure which is applied by the service provider to the referenced Resource.

Update may fail if the referenced Plan is already in the TERMINATED state, in which case the UPDATE\_FAILED error is returned.

|  |  |
| --- | --- |
| **Operation Identifier** | updateResourceProfile |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | planRef : (MAL::ObjectRef[Plan])  resourceProfile : (ResourceProfile) |

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* UPDATE\_FAILED

### Operation: applyTimeShift

#### Overview

The applyTimeShift operation may be used to request a shift in the timing by a fixed offset of the ActivityInstances, EventInstances and ResourceProfiles contained within a Plan that has previously been submitted to a plan execution function. The operation may also be restricted to one or more SubPlans within the referenced Plan and/or to a specified time period within the Plan. The service provider applies the time shift to the timing of ActivityInstances, EventInstances and ResourceProfiles contained within the Plan or SubPlan(s).

The time shift may fail if the referenced Plan is already in the TERMINATED state, in which case the UPDATE\_FAILED error is returned.

The operation is designed to support backward compatibility with simple time-based on-board schedules, and may not be appropriate for use with plans that include event or position-based triggers and resource profiles. What is shifted within the Plan is implementation dependent, but shall include time-based start and end triggers on ActivityInstances. EventInstances may also be shifted, but it is noted that some EventInstances correspond to predicted orbital events that cannot meaningfully be shifted. Similarly, where supported, resource profiles may reflect the ActivityInstances contained within the Plan and if those are shifted, the corresponding changes in Resource value should also be shifted.

|  |  |
| --- | --- |
| **Operation Identifier** | applyTimeShift |
| **Interaction Pattern** | SUBMIT |

| Pattern Sequence | Message | Body Signature |
| --- | --- | --- |
| IN | SUBMIT | planRef : (MAL::ObjectRef[Plan])  subPlans : (List <MAL::Identifier[SubPlan]>)  timePeriod : (TimeWindow)  offset : (MAL::Duration) |

#### Structures

**Req\_4.6.14.S.62** The subPlans and timePeriod fields of the applyTimeShift submit message shall both be nullable.

#### Errors

In addition to standard MAL Errors, the operation may return the following MPS Errors:

* INVALID
* UPDATE\_FAILED

# Error Codes

Standard error codes defined by the MAL are applicable to the MPS service operations. In particular it is noted that this includes errors associated with delivery issues and authorization failure.

The following error codes shall apply to this specification.

|  |  |  |  |
| --- | --- | --- | --- |
| Error | Error # | Description | ExtraInfo Type |
| INVALID | 80000 | One or more fields in the message contain invalid values.  ExtraInfo comprises a list of structures, each identifying an invalid field, comprising:   1. A String giving a dot separated nested index for the field, to allow for fields that are themselves a structure, of the form “3.2” meaning the 2nd field of the composite structure that is the 3rd field of the message. 2. A UInteger giving a secondary error code that details the reason for invalidity. | List <MAL::Pair> |
| CANCEL\_FAILED | 80001 | The cancelRequest operation failed to cancel the referenced RequestInstance.  ExtraInfo provides additional information on the reason for failure as a free format string. | MAL::String |
| UPDATE\_FAILED | 80002 | The update operation (to Request, PlanStatus, Activity, Event or Resource) failed to update the referenced object.  ExtraInfo provides additional information on the reason for failure as a free format string. | MAL::String |
| REVOKE\_FAILED | 80003 | The revokePlan operation failed to revoke the referenced Plan, for example because it has already started executing.  ExtraInfo provides additional information on the reason for failure as a free format string. | MAL::String |
| INSERT\_FAILED | 80004 | The insertActivity or insertEvent operation failed to insert the requested object.  ExtraInfo provides additional information on the reason for failure as a free format string. | MAL::String |
| DELETE\_FAILED | 80005 | The deleteActivity or deleteEvent operation failed to delete the requested object.  ExtraInfo provides additional information on the reason for failure as a free format string. | MAL::String |

Standard secondary error codes for the INVALID error are as follows:

| Error | Error # | Description |
| --- | --- | --- |
| UNKNOWN | 0 | Referenced MO Object is not available to the service provider. |
| UNDEFINED | 1 | Undefined value for enumeration field. |
| OUT\_OF\_RANGE | 2 | A numeric value is outside the supported range. |
| UNRECOGNIZED | 3 | Value of type MAL::Identifier or MAL::String (referencing a named item) does not correspond to a known item. |
| BAD\_TIME | 4 | A date-time value is outside the supported time period. |
| BAD\_POSITION | 5 | A position value is outside the supported position range. |
| BAD\_DIRECTION | 6 | A direction value is outside the supported direction range. |
| INCONSISTENT | 7 | A value is inconsistent with that of another field within the message. This indicates violation of a constraint rule. |

# Service Specification XML

The use of XML for service specification provides a machine-readable format rather than the text-based document format. The service specification in XML notation as specified in reference [XX] may be accessed at the URLs below.

The published specifications and XML schemas are held in an online SANA registry, located at the following URL:

<http://sanaregistry.org/r/moschemas/>

The normative XML for this specification, validated against the XML schemas, is located at the following URL:

<http://sanaregistry.org/r/moschemas/ServiceDefMPS-v.v.xml>

where the ‘v.v’ part is replaced with the issue number of the corresponding document.

The latest version of any specification may always be directly addressed by removing the ‘-v.v’ part from the URL; for example:

<http://sanaregistry.org/r/moschemas/ServiceDefMPS.xml>

# XML File Formats

Some MPS deployments, including those based on legacy systems, may not be designed to use service-based interaction, relying instead on the transfer of files with a defined data structure. In order to support such deployments, the following standardized file formats are defined based on the XML schema for MPS service specification defined in chapter 6, and the MPS Information Model defined in chapter 3:

* Planning Request
* Plan

## Planning Request XML File Format

## Plan XML File Format

1. Protocol Implementation Conformance   
   Statement (PICS) Proforma  
   (Normative)
   1. INTRODUCTION
      1. OVERVIEW

This annex provides the Protocol Implementation Conformance Statement (PICS) Requirements List (PRL) for an implementation of the Mission Operations MPS Services standard. The PICS for an implementation is generated by completing the PRL in accordance with the instructions below. An implementation claiming conformance must satisfy the mandatory requirements referenced in the PRL.

An implementation’s completed PRL is called the PICS. The PICS states which protocol features have been implemented. The following entities can use the PICS:

* the protocol implementer, as a checklist to reduce the risk of failure to conform to the standard through oversight;
* the supplier and acquirer or potential acquirer of the implementation, as a detailed indication of the capabilities of the implementation, stated relative to the common basis for understanding provided by the standard PICS proforma;
* the user or potential user of the implementation, as a basis for initially checking the possibility of interworking with another implementation (while interworking can never be guaranteed, failure to interwork can often be predicted from incompatible PICSes);
* a protocol tester, as the basis for selecting appropriate tests against which to assess the claim for conformance of the implementation..
  + 1. Notation
       1. Status Column Symbols

The following are used in the PRL to indicate the status of features:

|  |  |
| --- | --- |
| **Symbol** | **Meaning** |
| M | Mandatory |
| O | Optional |

* + - 1. Support Column Symbols

The support of every item as claimed by the implementer is stated by entering the appropriate answer (Y, N, or N/A) in the support column.

|  |  |
| --- | --- |
| **Symbol** | **Meaning** |
| Y | Yes, supported by the implementation |
| N | No, not supported by the implementation |
| N/A | Not applicable |

* 1. General Information
     1. Identification of PICS

|  |  |  |
| --- | --- | --- |
| **Ref** | **Question** | **Response** |
| 1 | Date of Statement (DD/MM/YYYY) |  |
| 2 | CCSDS document number containing the PICS |  |
| 3 | Date of CCSDS document containing the PICS |  |

* + 1. Identification of implementation under test (IUT)

|  |  |  |
| --- | --- | --- |
| **Ref** | **Question** | **Response** |
| 1 | Implementation name |  |
| 2 | Implementation version |  |
| 3 | Machine name |  |
| 4 | Machine version |  |
| 5 | Operating System name |  |
| 6 | Operating System version |  |
| 7 | Special Configuration |  |
| 8 | Other Information |  |

* + 1. User Identification

|  |  |
| --- | --- |
| Supplier |  |
| Contact Point for Queries |  |
| Implementation name(s) and Versions |  |
| Other Information Necessary for full identification, e.g., name(s) and version(s) for machines and/or operating systems;  System Name(s) |  |

* + 1. Instructions for Completing the PRL

An implementer shows the extent of compliance to the protocol by completing the PRL; the resulting completed PRL is called a PICS.

* 1. MPS Services PICS

There are 5 separate MPS services defined, each of which has multiple capability sets. The service is shown as a top level item, with subsidiary items for each capability set, using the format <service number>.<capability set number>. All services are optional, but if implemented, some capability sets are mandatory.

Additional items are shown for the standard file formats that may be supported without services.

The MPS services use an information model, which itself has optional elements, which implies some features may not be supported within service messages. Support for optional elements of the information model is shown as a separate item “D”, with subsidiary items for each optional element. This section should be completed in conjunction with both services and file based items.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Protocol Feature** | **Reference** | **Status** | **Support** |
| 1 | Parameter Request Service | 2.6 and 4.2 | O |  |
| 1.1 | Submit Request / Status | 2.6 and 4.2 | M |  |
| 1.2 | Cancel Request | 2.6 and 4.2 | O |  |
| 1.3 | Update Request | 2.6 and 4.2 | O |  |
| 1.4 | Subscribe to Status | 2.6 and 4.2 | O |  |
| 1.5 | Retrieve Request | 2.6 and 4.2 | O |  |
| 2 | Plan Distribution Service | 2.6 and 4.3 | O |  |
| 2.1 | List and Obtain Plans | 2.6 and 4.3 | M |  |
| 2.2 | Subscribe to Status | 2.6 and 4.3 | O |  |
| 2.3 | Subscribe to Plans | 2.6 and 4.3 | O |  |
| 2.4 | Query Plans | 2.6 and 4.3 | O |  |
| 2.5 | Retrieve Partial Plan | 2.6 and 4.3 | O |  |
| 3 | Plan Execution Control Service | 2.6 and 4.4 | O |  |
| 3.1 | Submit Plan / Status | 2.6 and 4.4 | M |  |
| 3.2 | Plan Activation | 2.6 and 4.4 | O |  |
| 3.3 | Subscribe to Status | 2.6 and 4.4 | O |  |
| 3.4 | Subscribe to Detail | 2.6 and 4.4 | O |  |
| 3.5 | SubPlan Activation | 2.6 and 4.4 | O |  |
| 3.6 | Subscribe to SubPlans | 2.6 and 4.4 | O |  |
| 3.7 | Activity Suspension | 2.6 and 4.4 | O |  |
| 3.8 | Activity Status | 2.6 and 4.4 | O |  |
| 4 | Plan Information Management Service | 2.6 and 4.5 | O |  |
| 4.1 | Request Definitions | 2.6 and 4.5 | O |  |
| 4.2 | Event Definitions | 2.6 and 4.5 | O |  |
| 4.3 | Activity Definitions | 2.6 and 4.5 | O |  |
| 4.4 | Resource Definitions | 2.6 and 4.5 | O |  |
| 4.5 | MPSSystemConfig | 2.6 and 4.5 | O |  |
| 5 | Plan Edit Service | 2.6 and 4.6 | O |  |
| 5.1 | Update Plan Status | 2.6 and 4.6 | M |  |
| 5.2 | Insert/Delete Activity/Event | 2.6 and 4.6 | M |  |
| 5.3 | Update Activity/Event | 2.6 and 4.6 | O |  |
| 5.4 | Update Resource | 2.6 and 4.6 | O |  |
| 5.5 | Update Resource Profile | 2.6 and 4.6 | O |  |
| 5.6 | Apply Time Shift |  | O |  |
| 6 | Planning Request File Format | 7.1 | O |  |
| 7 | Plan File Format | 7.2 | O |  |
| D | MPS Information Model | 2.6 and 3 | M |  |
| D.1 | Core Features | 2.6 and 3 | M |  |
| D.2 | Basic Constraints | 2.6, 3.3.6.1.2, 3.3.6.1.3, 3.3.6.1.4 | O |  |
| D.3 | Plan Revisions | 2.6 and 3.2.6.1.3 | O |  |
| D.4 | Resources | 2.6, 3.2.4 and 3.2.6.1.4 | O |  |
| D.5 | Resource Constraints (requires D.4) | 2.6, 3.3.6.1.5 and 3.3.6.2 | O |  |
| D.6 | Position & Direction | 2.6, 3.3.2.1, 3.3.2.2, 3.3.7.2, 3.3.7.3, 3.3.7.4, 3.3.8.2, 3.3.8.3, 3.3.8.4 | O |  |
| D.7 | Geometric Constraints (requires D.6) | 2.6, 3.3.6.1.7 | O |  |
| D.8 | Functions | 2.6, 3.2.8, 3.3.6.1.6 | O |  |

1. Security, SANA, and Patent Considerations  
   (Informative)

*See M&C Service Specification. Can probably adapt this for MPS.*

* 1. Security Considerations

The security considerations of this specification are the same as those of reference [2]. Specifically, authentication and authorisation of a participating consumer or provider is provided by the MAL access control concept and is covered in subsections 3.6, 5.2, and 5.3 of the Reference Model (reference [1]).

Security of a communications link is delegated to the transport layer.

* 1. SANA Considerations

The recommendations of this document request SANA populate the registry specified in reference [2] with the schema and XML detailed in section 6 of this document.

As stated in reference [2], the registration rule for change to this registry requires an engineering review by a designated expert. The expert shall be assigned by the WG Chair, or in absence, Area Director.

* 1. Patent Considerations

The recommendations of this document have no patent issues.

1. Definition of Acronyms  
   (Informative)

| Acronym | Definition |
| --- | --- |
| AOS | Acquisition Of Signal |
| COM | Common Object Model |
| CSS | Cross Support Services |
| LOS | Loss of Signal |
| MAL | Message Abstraction Layer |
| MO | Mission Operations |
| MPS | Mission Planning and Scheduling |
| NAV | CCSDS Navigation Message |
| NEM | Navigation Event Message |
| ODM | Orbit Data Message |
| PDS | Plan Distribution Service |
| PECS | Plan Execution Control Service |
| PES | Plan Edit Service |
| PI | Principal Investigator |
| PICS | Protocol Implementation Conformance Statement |
| PIMS | Plan Information Management Service |
| PRL | (PICS) Requirements List |
| PRM | Pointing Request Message |
| PRS | Planning Request Service |
| SANA | CCSDS Space Assigned Numbers Authority |
| SFN | Short Form Number |
| SFP | Short Form Part |
| TOO | Target Of Opportunity |
| UML | Unified Modelling Language |
| URI | Uniform Resource Identifier |
| URL | Uniform Resource Locator |
| XML | eXtensible Markup Language |

1. Informative References  
   (Informative)
2. *Mission Operations Services Concept*, Issue 3, CCSDS Informational Report (Green Book), CCSDS 520.0-G-3. Washington, D.C.: CCSDS, December 2010
3. *Mission Planning and Scheduling,* CCSDS Informational Report (Green Book), CCSDS 529.0-G-1, Washington, D.C.: CCSDS, June 2018
4. *Mission Operations Common Object Model*, Issue 1, CCSDS Recommended Standard (Blue Book), CCSDS 521.1-B-1, Washington, D.C.: CCSDS, February 2014
5. *Mission Operations – Common Services*, Issue 1, CCSDS Recommended Standard (Blue Book), CCSDS 522.0-B-1, Washington, D.C.: CCSDS, May 2020
6. *Mission Operations Monitoring & Control Services*, Issue 1, CCSDS Recommended Standard (Blue Book), CCSDS 522.1-B-1, Washington, D.C.: CCSDS, October 2017
7. *Navigation Event Message,* Proposed CCSDS Recommended Standard
8. *Pointing Request Message,* Issue 1, CCSDS Recommended Standard (Blue Book), CCSDS-509.0-B-1, Washington, D.C.: CCSDS, February 2018
9. *Cross Support Service Management – Simple Schedule Format Specification*, Issue 1, CCSDS Recommended Standard (Blue Book), CCSDS-902.1-B-1, Washington, D.C.: CCSDS, May 2018
10. *Telemetry and Telecommand Packet Utilization*, ECSS Standard, ECSS-E-ST-70-41C, Nordwijk, The Netherlands: ECSS 15 April 2016
11. *XML Path Language (XPath)*, Issue3.1, W3C Recommendation, 21 March 2017

1. Tags are used in the MPS information model to capture the equivalent concept to subschedules of PUS service 11 in the ECSS Packet Utilisation Standard [D9]. [↑](#footnote-ref-1)