

Recommendation for Space Data System Standards

|  |
| --- |
| XML Specification for Navigation Data Messages |

Revised Standard

CCSDS 505.0-P-2.0.2

Pink Book

September 2022

AUTHORITY

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | Issue: | Revised Standard, Issue 2.0.2 |  |
|  | Date: | September 2022 |  |
|  | Location: | Washington, DC, USA |  |
|  |  |  |  |

This document has been approved for publication by the Management Council of the Consultative Committee for Space Data Systems (CCSDS) and represents the consensus technical agreement of the participating CCSDS Member Agencies. The procedure for review and authorization of CCSDS documents is detailed in *Organization and Processes for the Consultative Committee for Space Data Systems* (CCSDS A02.1-Y-4), and the record of Agency participation in the authorization of this document can be obtained from the CCSDS Secretariat at the email address below.

This document is published and maintained by:

CCSDS Secretariat

National Aeronautics and Space Administration

Washington, DC, USA

Email: secretariat@mailman.ccsds.org

STATEMENT OF INTENT

The Consultative Committee for Space Data Systems (CCSDS) is an organization officially established by the management of its members. The Committee meets periodically to address data systems problems that are common to all participants, and to formulate sound technical solutions to these problems. Inasmuch as participation in the CCSDS is completely voluntary, the results of Committee actions are termed **Recommended Standards** and are not considered binding on any Agency.

This **Recommended Standard** is issued by, and represents the consensus of, the CCSDS members. Endorsement of this **Recommendation** is entirely voluntary. Endorsement, however, indicates the following understandings:

o Whenever a member establishes a CCSDS-related **standard**, this **standard** will be in accord with the relevant **Recommended Standard**. Establishing such a **standard** does not preclude other provisions which a member may develop.

o Whenever a member establishes a CCSDS-related **standard**, that member will provide other CCSDS members with the following information:

-- The **standard** itself.

-- The anticipated date of initial operational capability.

-- The anticipated duration of operational service.

o Specific service arrangements shall be made via memoranda of agreement. Neither this **Recommended Standard** nor any ensuing **standard** is a substitute for a memorandum of agreement.

No later than five years from its date of issuance, this **Recommended Standard** will be reviewed by the CCSDS to determine whether it should: (1) remain in effect without change; (2) be changed to reflect the impact of new technologies, new requirements, or new directions; or (3) be retired or canceled.

In those instances when a new version of a **Recommended Standard** is issued, existing CCSDS-related member standards and implementations are not negated or deemed to be non-CCSDS compatible. It is the responsibility of each member to determine when such standards or implementations are to be modified. Each member is, however, strongly encouraged to direct planning for its new standards and implementations towards the later version of the Recommended Standard.

FOREWORD

This document is a technical Recommended Standard for an XML Specification for Navigation Data Messages. This Recommended Standard has been developed via consensus of the Navigation Working Group of the CCSDS Mission Operations and Information Management Services (MOIMS) area. The XML schema set described in this Recommended Standard represents the baseline concept for exchanging navigation data in XML format between Agencies of the CCSDS.

This Recommended Standard establishes a common framework and provides a common basis for the interchange of navigation data in XML format. It allows implementing organizations within each Agency to proceed coherently with the development of compatible derived standards for the flight and ground systems that are within their cognizance. Derived Agency standards may implement only a subset of the optional features allowed by the Recommended Standard and may incorporate features not addressed by this Recommended Standard.

Through the process of normal evolution, it is expected that expansion, deletion, or modification of this document may occur. This Recommended Standard is therefore subject to CCSDS document management and change control procedures, which are defined in the *Organization and Processes for the Consultative Committee for Space Data Systems* (CCSDS A02.1-Y-4). Current versions of CCSDS documents are maintained at the CCSDS Web site:

https://www.ccsds.org/

Questions relating to the contents or status of this document should be sent to the CCSDS Secretariat at the email address indicated on page i.

At time of publication, the active Member and Observer Agencies of the CCSDS were:

Member Agencies

* Agenzia Spaziale Italiana (ASI)/Italy.
* Canadian Space Agency (CSA)/Canada.
* Centre National d’Etudes Spatiales (CNES)/France.
* China National Space Administration (CNSA)/People’s Republic of China.
* Deutsches Zentrum für Luft- und Raumfahrt (DLR)/Germany.
* European Space Agency (ESA)/Europe.
* Federal Space Agency (FSA)/Russian Federation.
* Instituto Nacional de Pesquisas Espaciais (INPE)/Brazil.
* Japan Aerospace Exploration Agency (JAXA)/Japan.
* National Aeronautics and Space Administration (NASA)/USA.
* UK Space Agency/United Kingdom.

Observer Agencies

* Austrian Space Agency (ASA)/Austria.
* Belgian Science Policy Office (BELSPO)/Belgium.
* Central Research Institute of Machine Building (TsNIIMash)/Russian Federation.
* China Satellite Launch and Tracking Control General, Beijing Institute of Tracking and Telecommunications Technology (CLTC/BITTT)/China.
* Chinese Academy of Sciences (CAS)/China.
* China Academy of Space Technology (CAST)/China.
* Commonwealth Scientific and Industrial Research Organization (CSIRO)/Australia.
* Danish National Space Center (DNSC)/Denmark.
* Departamento de Ciência e Tecnologia Aeroespacial (DCTA)/Brazil.
* Electronics and Telecommunications Research Institute (ETRI)/Korea.
* European Organization for the Exploitation of Meteorological Satellites (EUMETSAT)/Europe.
* European Telecommunications Satellite Organization (EUTELSAT)/Europe.
* Geo-Informatics and Space Technology Development Agency (GISTDA)/Thailand.
* Hellenic National Space Committee (HNSC)/Greece.
* Hellenic Space Agency (HSA)/Greece.
* Indian Space Research Organization (ISRO)/India.
* Institute of Space Research (IKI)/Russian Federation.
* Korea Aerospace Research Institute (KARI)/Korea.
* Ministry of Communications (MOC)/Israel.
* Mohammed Bin Rashid Space Centre (MBRSC)/United Arab Emirates.
* National Institute of Information and Communications Technology (NICT)/Japan.
* National Oceanic and Atmospheric Administration (NOAA)/USA.
* National Space Agency of the Republic of Kazakhstan (NSARK)/Kazakhstan.
* National Space Organization (NSPO)/Chinese Taipei.
* Naval Center for Space Technology (NCST)/USA.
* Netherlands Space Office (NSO)/The Netherlands.
* Research Institute for Particle & Nuclear Physics (KFKI)/Hungary.
* Scientific and Technological Research Council of Turkey (TUBITAK)/Turkey.
* South African National Space Agency (SANSA)/Republic of South Africa.
* Space and Upper Atmosphere Research Commission (SUPARCO)/Pakistan.
* Swedish Space Corporation (SSC)/Sweden.
* Swiss Space Office (SSO)/Switzerland.
* United States Geological Survey (USGS)/USA.

DOCUMENT CONTROL

|  |  |  |  |
| --- | --- | --- | --- |
| **Document** | **Title** | **Date** | **Status** |
| CCSDS 505.0-B-1 | XML Specification for Navigation Data Messages, Recommended Standard, Issue 1 | December 2010 | Original issue, superseded |
| CCSDS 505.0-B-2 | XML Specification for Navigation Data Messages, Recommended Standard, Issue 2 | May 2021 | Current issue:   * applies general improvements and eliminates overlaps with other CCSDS navigation documents (note). |

|  |  |  |  |
| --- | --- | --- | --- |
| CCSDS 505.0-P-2.0.1 | XML Specification for Navigation Data Messages, Revised Standard, Issue 2.0.1 | August 2022 | Revised issue:   * applies general improvements and eliminates overlaps with other CCSDS navigation documents. |
| CCSDS 505.0-P-2.0.2 | XML Specification for Navigation Data Messages, Revised Standard, Issue 2.0.2 | September 2022 | * Detailed changes in preparation for Agency Review. |
|  |  |  |  |

CONTENTS

Section Page

[1 INTRODUCTION 1-1](#_Toc113809570)

[1.1 PURPOSE 1-1](#_Toc113809571)

[1.2 SCope and APPLICABILITY 1-1](#_Toc113809572)

[1.3 Rationale 1-2](#_Toc113809573)

[1.4 STRUCTURE OF THIS DOCUMENT 1-2](#_Toc113809574)

[1.5 CONVENTIONS AND DEFINITIONS 1-3](#_Toc113809575)

[1.6 REferences 1-3](#_Toc113809576)

[2 OVERVIEW 2-1](#_Toc113809577)

[2.1 Navigation Data Messages 2-1](#_Toc113809578)

[3 BASIC StrUCTURE OF THE NDM/XML SCHEMA SET 3-3](#_Toc113809579)

[3.1 NAVIGATION DATA MESSAGES AND THE ASSOCIATED Schema sET 3-3](#_Toc113809580)

[3.2 NDM/XML BASIC STRUCTURE 3-5](#_Toc113809581)

[3.3 Substructure 1: apm, OCM, omm, opm, RDM 3-5](#_Toc113809582)

[3.4 Substructure 2: aem, oem, tdm, and CDM 3-6](#_Toc113809583)

[3.5 NDM/XML Tags 3-7](#_Toc113809584)

[3.6 NDM/XML Text ValueS 3-8](#_Toc113809585)

[4 constructing an ndm/xml instance 4-1](#_Toc113809586)

[4.1 Overview 4-1](#_Toc113809587)

[4.2 XML VERSION 4-1](#_Toc113809588)

[4.3 BEGINNING THE INSTANTIATION: ROOT ELEMENT TAG 4-1](#_Toc113809589)

[4.4 The STANDARD NDM/XML Header SECTION 4-3](#_Toc113809590)

[4.5 The NDM BODY section 4-3](#_Toc113809591)

[4.6 The NDM metadata section 4-4](#_Toc113809592)

[4.7 The NDM data section 4-4](#_Toc113809593)

[4.8 CREATING AN AEM INSTANTIATION 4-4](#_Toc113809594)

[4.9 CREATING AN APM INSTANTIATION 4-9](#_Toc113809595)

[4.10 USER DEFINED PARAMETERS 4-14](#_Toc113809596)

[4.11 CREATING AN NDM COMBINED INSTANTIATION 4-15](#_Toc113809597)

[4.12 Extensible Markup Language 4-1](#_Toc113809598)

[4.13 Special Considerations 4-3](#_Toc113809599)

CONTENTS (continued)

Section Page

ANNEX A IMPLEMENTATION CONFORMANCE STATEMENT (ICS) (Normative) 4-20

ANNEX B VALUES FOR SELECTED KEYWORDS (Normative) 4-22

ANNEX C SECURITY, SANA, AND PATENT CONSIDERATIONS   (Informative) C-1

ANNEX D ABBREVIATIONS AND ACRONYMS   (INFORMATIVE) D-1

ANNEX E RATIONALE FOR XML-FORMAT NAVIGATION DATA MESSAGES (INFORMATIVE) E-1

ANNEX F TECHNICAL MATERIAL AND CONVENTIONS (INFORMATIVE) 4-1

ANNEX G EXAMPLE NDM/XML SCHEMA INSTANTIATIONS   (INFORMATIVE) G-1

ANNEX H InfoRmative References   (Informative) H-1

ANNEX I ITEMS FOR AN INTERFACE CONTROL DOCUMENT (ICD)   (INFORMATIVE) I-1

ANNEX J CHANGES IN NDM/XML VERSION 3   (INFORMATIVE) J-1

Figure

[3-1 NDM/XML Substructure 1 (Single Segment) 3-5](#_Toc113809948)

[3-2 NDM/XML Substructure 2 (Possible Multiplicity of Segments) 3-6](#_Toc113809949)

[3-3 Variant of Substructure 2 for CDM 3-7](#_Toc113809950)

[4-1 Comparison of Single Message NDM with NDM Combined Instantiation 4-16](#_Toc113809951)

[4-2 NDM Combined Instantiation Basic Structure 4-17](#_Toc113809952)

[4-3 NDM Combined Instantiation Showing Use of Attributes 4-18](#_Toc113809953)

[G-1 Sample NDM/XML AEM G-2](#_Toc113809954)

[G-2 Sample NDM/XML AEM with Rotation G-4](#_Toc113809955)

[G-3 Sample NDM/XML APM G-5](#_Toc113809956)

[G-4 Sample Combined Instantiation with elementFormDefault="qualified\ G-8](#_Toc113809957)

Table

[3-1 The NDM/XML Schema Set 3-4](#_Toc113809855)

[4-1 Special Tags Used in the AEM Body 4-5](#_Toc113809856)

[4-2 AEM Rotation Tags 4-6](#_Toc113809857)

[4-3 APM Tags with Units 4-10](#_Toc113809858)

[4-4 Special Tags Used in the APM Body 4-10](#_Toc113809859)

[4-5 APM Rotation Tags 4-11](#_Toc113809860)

[E-1 Primary Requirements E-2](#_Toc113809861)

[E-2 Heritage Requirements E-2](#_Toc113809862)

[E-3 Desirable Characteristics E-2](#_Toc113809863)

# INTRODUCTION

## PURPOSE

This Recommended Standard specifies a format for use in exchanging spacecraft navigation data. Such exchanges are used for distributing navigation-related data between space agencies and other space operators. The Recommended Standard specifies an integrated Extensible Markup Language (XML) schema set that applies to Navigation Data Messages (NDMs) defined in the CCSDS Recommended Standards developed by the CCSDS Navigation Working Group (see references [4]–[8]). This XML schema set is suited to interagency exchanges of any number of NDMs.

## SCope and APPLICABILITY

This Recommended Standard is applicable only to the schema content and layout, and to instantiations of the schema, but not to the *transmission* of any instantiation of the schema. The means of transmission of an XML-formatted NDM between exchange participants is beyond the scope of this document; such arrangements require specification via other arrangements, for example, in an Interface Control Document (ICD). Transmission of an XML-formatted NDM could be based on a future CCSDS real-time data transfer service, a file-based transfer protocol such as the Secure File Transfer Protocol (SFTP), streaming media, email, or services provided via the World Wide Web and XML-compatible Web browsers. The potential for compression/decompression of the message is an aspect of the transmission that is not part of this specification. In general, it is a requirement that the transmission mechanism not place constraints on the technical data content of an NDM.

As noted in the Purpose subsection above, this document applies to the NDMs defined in the CCSDS Recommended Standards developed by the CCSDS Navigation Working Group. Historically, the first few such Recommended Standards contained no XML representation. Given the lack of XML representations in these early Recommended Standards, the first version of this NDM/XML document contained information on how to create instantiations of all the messages documented in the Orbit Data Messages (ODM), Attitude Data Messages (ADM), and Tracking Data Message (TDM). Starting with Conjunction Data Message (CDM) in 2013, the XML representation was directly included in the Recommended Standard. XML representations have been added to other Recommended Standards as they have been produced (the Re-Entry Data Message (RDM) in 2019, the TDM version 2 in 2020, and the ODM version 3 in 2023). As the early Navigation Working Group Recommended Standards are being revised, the strategy is to remove the XML formatting discussion from this NDM/XML document and migrate it into the revised documents; the ADM is the last of these early Navigation Working Group early standards. (Note that the CCSDS Pointing Request Message (PRM) is also a standard created by the CCSDS Navigation Working Group, but it is implemented using a set of XML templates rather than as an XML message that can be validated via the XML schema language.)

The first version of this document only encompassed schemas and messages in which the XML ‘elementFormDefault="unqualified"’ applied. This version of the Recommended Standard encompasses schemas and messages in which the XML ‘elementFormDefault="unqualified"’ and ‘elementFormDefault="qualified"’ both apply. The "qualified" schemas can be included/imported into XML schemas for other CCSDS Recommended Standards that wish to leverage Navigation Working Group data structures.

## Rationale

This document responds to a requirement levied by the CCSDS to produce an XML format for NDMs. Rather than revise several different CCSDS Recommended Standards, the relevant XML format information was consolidated in Version 1 of this document. It includes sets of requirements and criteria that the XML schema set has been designed to meet. The rationale behind the design of the schema set is described in annex E in order to assist the application engineer in constructing a suitable message.

## STRUCTURE OF THIS DOCUMENT

Section 1 (this section) provides an introduction, scope, normative references, and the description of the document structure.

Section 2 provides a very brief overview of the individual messages that constitute an NDM (i.e., references [4]–[8]). It also provides a very brief overview of XML, and the justification for an integrated NDM/XML schema set.

Section 3 provides an overview of the basic structure of the NDM/XML schema set. This structure is external to the internal structure provided by the constituent messages.

Section 4 provides detailed discussion of the differences between the XML-formatted messages and the Keyword Value Notation (KVN) text-formatted messages described in references [4]–[8]. Instructions for how to construct instantiations of the ADM message types and "combined instantiations" are provided.

Annex A explains why this document does not contain an Implementation Conformance Statement (ICS), a component of typical CCSDS Recommended Standards.

Annex B explains why this document does not provide in Annex B the material that is provided in Annex B of other Navigation Working Group standards.

Annex C discusses information security, Space Assigned Numbers Authority (SANA), and patent considerations.

Annex D is a list of abbreviations and acronyms applicable to the NDM/XML.

Annex E lists a set of requirements that were taken into consideration in the design of the NDM/XML schema set.Annex F provides some technical material and conventions relevant to the NDM/XML.

Annex G provides instructions on where to find the schema set referenced in this Recommended Standard on the SANA website. Also provided for illustrative purposes are a number of example instantiations of NDM/XML messages.

Annex H contains a list of informative references.

Annex I lists a number of items that should be covered in interagency ICDs prior to  
exchanging NDMs in XML format on a regular basis.

Annex J lists the changes in this version of the Recommended Standard compared to the previous version.

## CONVENTIONS AND DEFINITIONS

### Nomenclature

The following conventions apply throughout this Recommended Standard:

1. the words ‘shall’ and ‘must’ imply a binding and verifiable specification;
2. the word ‘should’ implies an optional, but desirable, specification;
3. the word ‘may’ implies an optional specification;
4. the words ‘is’, ‘are’, and ‘will’ imply statements of fact.

### Terms

For the purposes of this document, the following definitions apply:

CamelCase: a style of capitalization in which the initial characters of concatenated words are capitalized.

lowerCamelCase: a variant on CamelCase in which the first character of a character string formed from concatenated words is lowercase. In the case of a character string consisting of only a single word, only lowercase characters are used.

ASCII: a text character set defined in reference [H4].

## REferences

The following documents contain provisions which, through reference in this text, constitute provisions of this Recommended Standard. At the time of publication, the editions indicated were valid. All documents are subject to revision, and users of this Recommended Standard are encouraged to investigate the possibility of applying the most recent editions of the documents indicated below. The CCSDS Secretariat maintains a register of currently valid CCSDS Recommended Standards.

[1] Henry S. Thompson, et al., eds. “XML Schema Part 1: Structures.” W3C Recommendation. 2nd ed., 28 October 2004. The World Wide Web Consortium (W3C). https://www.w3.org/TR/2004/REC-xmlschema-1-20041028/.

[2] Paul V. Biron and Ashok Malhotra, eds. “Extensible Markup Language (XML) 1.0.” W3C Recommendation. 3rd ed., February 2004. https://www.w3.org/TR/2004/REC-xmlschema-2-20041028/.

[3] “Navigation Data Messages XML Schema.” Space Assigned Numbers Authority. https://beta.sanaregistry.org/r/ndmxml.

[4] *Attitude Data Messages*. Issue 1. Recommendation for Space Data System Standards (Blue Book), CCSDS 504.0-B-1. Washington, D.C.: CCSDS, May 2008.

[5] *Orbit Data Messages*. Issue 3. Recommendation for Space Data System Standards (Blue Book), CCSDS 502.0-B-3. Washington, D.C.: CCSDS, to be published 2023.

[6] *Tracking Data Message*. Issue 2. Recommendation for Space Data System Standards (Blue Book), CCSDS 503.0-B-2. Washington, D.C.: CCSDS, June 2020.

[7] *Conjunction Data Message*. Issue 1. Recommendation for Space Data System Standards (Blue Book), CCSDS 508.0-B-1. Washington, D.C.: CCSDS, June 2013.

[8] *Re-entry Data Message*. Issue 1. Recommendation for (Blue Book), CCSDS 508.1-B-1. Washington, D.C.: CCSDS, November 2019.

NOTE – Informative references are provided in annex H.

# OVERVIEW

## Navigation Data Messages

### General

This subsection provides a brief overview of the set of NDMs. There are five basic types of NDM that are covered by the schemas described in this document: Attitude Data Messages (reference [4]), Orbit Data Messages (reference [5]), Tracking Data Message (reference [6]), Conjunction Data Message (reference [7]), and Re-entry Data Message (reference [8]). The remainder of this document conveys the structure of the NDMs in an integrated XML schema set.

### Attitude Data Messages

Attitude Data Messages comprise two message types used to convey spacecraft attitude information: the Attitude Parameter Message (APM) and Attitude Ephemeris Message (AEM). The APM consists of an instantaneous attitude state and optional attitude maneuvers. The AEM consists of a history/forecast of the attitude of the object; the history/forecast can be interpolated to obtain the attitude of the spacecraft at times other than those specified in the message. Instructions for creating an XML instantiation of the messages in the ADM are specified in Section 4 of this document. The APM and AEM are specified in reference [4].

### Orbit Data Messages

Orbit Data Messages comprise four message types used to convey trajectory information: the Orbit Parameter Message (OPM), Orbit Mean Elements Message (OMM), Orbit Ephemeris Message (OEM), and Orbit Comprehensive Message. The OPM consists of a single state vector at a given time that can be propagated to generate the trajectory of the spacecraft; specifications of maneuvers are optional. Like the OPM, the OMM also represents an orbit state, but it is calculated on the basis of mean orbital elements instead of osculating elements (there are other differences as well). The OEM represents a history/forecast of state vectors that can be interpolated to obtain the state of the spacecraft at times other than those explicitly specified in the message. The OCM aggregates and extends OPM, OMM, and OEM content in a single comprehensive hybrid message and includes a great deal of additional information about the spacecraft and its environment. Instructions for creating an XML instantiation of the messages in the ODM version 3 are contained in the ODM document itself. The OPM, OMM, OEM, and OCM are specified in reference [5].

### Tracking Data Message

The Tracking Data Message is a single message type for use in exchanging spacecraft tracking data between space agencies. Such exchanges are used for distributing tracking data output from interagency cross supports in which spacecraft missions managed by one agency are tracked from a ground station managed by a second agency. Additionally, the ability to transfer tracking data between space agencies facilitates the allocation of tracking sessions to alternate antenna resources and increases the ability of space agencies to tolerate availability issues with their primary antennas. The TDM supports commonly used ground-based radiometric data types, spacecraft-to-spacecraft Doppler and range, and ancillary information needed to calculate the measurement residuals. Instructions for creating an XML instantiation of the TDM version 2 are contained in the TDM document itself. The TDM is specified in reference [6].

### Conjunction Data Message

The Conjunction Data Message specifies a single message type for use in exchanging spacecraft conjunction information between originators of conjunction assessments and satellite owner/operators and other authorized parties. Such exchanges provide critical information to satellite owner/operators to enable timely collision-avoidance decisions. The CDM is applicable to satellite operations in all environments in which close approaches and collisions among satellites are concerns. Instructions for creating an XML instantiation of the CDM are contained in the CDM document itself. The CDM is specified in reference [7].

### Re-Entry Data Message

The Re-entry Data Message specifies a single message type for use in exchanging spacecraft re-entry information between space situational-awareness data providers and recipients such as satellite operators, civil protection authorities, and/or aviation authorities. The RDM contains information about a single re-entry event, including identification of the re-entering object; basic re-entry information such as remaining orbital lifetime; whether the re-entry is controlled or not, and which celestial body the object is orbiting; and more complex re-entry information such as re-entry and impact windows, impact location and probabilities, state vector, object properties, the orbit determination process, and observations used to predict the re-entry. The information is used by recipients to assess the re-entry risk and plan any needed mitigation measures. The RDM is not limited to man-made objects re-entering the Earth’s atmosphere. It could be used for any entry/impact event by specifying the appropriate center name, reference frame, and object type. Instructions for creating an XML instantiation of the RDM are contained in the RDM document itself. The RDM is specified in reference [8].







# BASIC StrUCTURE OF THE NDM/XML SCHEMA SET

## NAVIGATION DATA MESSAGES AND THE ASSOCIATED Schema sET

The basic element in the NDM/XML is an NDM. An NDM shall consist of at least one of the messages documented in references [4]–[8].

The NDM/XML schema set shall consist of a schema for the most current Blue Book issue[[1]](#footnote-3) of each individual message type (see references [4]–[8]), an ‘NDM combined instantiation’ schema (see 4.11), a namespace schema, a master validator schema, and a schema containing elements common to more than one Navigation Working Group (see table 3‑1).

The NDM/XML schema set shall be available on a CCSDS resource that is internet accessible.

NOTE – The NDM/XML schema set is currently available at:

* https://beta.sanaregistry.org/r/ndmxml for links to the two schema subsets below:
* https://beta.sanaregistry.org/r/ndmxml\_unqualified/[schemaName] for schemas with the attribute ‘elementFormDefault="unqualified"’;
* https://beta.sanaregistry.org/r/ndmxml\_qualified/[schemaName] for schemas with the attribute ‘elementFormDefault="qualified"’.

For schemas directly associated with one of the NDM message types, the components of [schemaName] shall be

ndmxml-[ndmxmlVersionNumber]-[messageType]-[blueBookNumber].xsd

where

* [ndmxmlVersionNumber] is formed via the string M.m.X, where ‘M’ is the Blue Book number of this document (i.e., the NDM/XML standard), ‘m’ is a minor revision number of the NDM/XML Blue Book (usually ‘0’), and ‘X’ is a schema revision indicator (‘0’ for the initial version, then {‘A’, ‘B’, ‘C’,...} for successive revisions (see the SANA Registry for the current NDM/XML version number);
* [messageType] is one of the individual message types described in references [4]–[8] (e.g., APM, CDM, OPM, RDM, TDM, etc.);
* [blueBookNumber] is the most current Blue Book version corresponding to the message (e.g., ‘1.0’ for the AEM and APM).

NOTES

1. There are several test files and example NDM/XML instantiations on the CCSDS Navigation Working Group Collaborative Work Environment (CWE) Web site https://cwe.ccsds.org/moims/docs/MOIMS-NAV/Test-Messages/XML.
2. The following table illustrates the naming convention in the names of the NDM/XML schema set. The ‘Blue Book Supported’ column indicates the message and respective Blue Book to which the schema applies; an asterisk next to the schema name indicates that instructions for creating an instantiation are incorporated in this Blue Book.
3. The naming convention for the auxiliary schemas not directly associated with an NDM (common, master, namespace) is similar to the convention for the message-related schemas, but not identical.
4. As noted above, each schema is available with ‘elementFormDefault="qualified"’ and ‘elementFormDefault="unqualified"’.

Table 3‑1 : The NDM/XML Schema Set

| **Schema** | **Blue Book Supported** | **Root Tag** |
| --- | --- | --- |
| ndmxml-3.0.x-aem-1.0.xsd \* | ADM Attitude Ephemeris Message (reference [4]) | <aem> |
| ndmxml-3.0.x-apm-1.0.xsd \* | ADM Attitude Parameter Message (reference [4]) | <apm> |
| ndmxml-3.0.x-cdm-1.0.xsd | CDM Conjunction Data Message (reference [7]) | <cdm> |
| ndmxml-3.0.x-common-3.n.xsd | Constructs used in more than one NDM schema (‘n’ is a sequence number 0, 1, 2, ...). Supports all references listed in references [4]–[8]. | N/A |
| ndmxml-3.0.x-master-3.n.xsd | NDM/XML master schema, used to validate all instantiations, import NDM/XML namespace, and declare all schema set root elements. Supports all references listed in references [4]–[8]. | N/A |
| ndmxml-3.0.x-namespace-3.n.xsd | Includes each element of the NDM/XML schema set. Supports all references listed in references [4]–[8]. | N/A |
| ndmxml-3.0.x-ndm-3.0.xsd | NDM combined instantiation schema (see 4.11) | <ndm> |
| ndmxml-3.0.x-ocm-3.0.xsd | ODM Orbit Comprehensive Message (reference [5]) | <ocm> |
| ndmxml-3.0.x-oem-3.0.xsd | ODM Orbit Ephemeris Message (reference [5]) | <oem> |
| ndmxml-3.0.x-omm-3.0.xsd | ODM Orbit Mean Elements Message (reference [5]) | <omm> |
| ndmxml-3.0.x-opm-3.0.xsd | ODM Orbit Parameter Message (reference [5]) | <opm> |
| ndmxml-3.0.x-rdm-1.0.xsd | RDM Re-entry Data Message (reference [8]) | <rdm> |
| ndmxml-3.0.x-tdm-2.0.xsd | TDM Tracking Data Message (reference [6]) | <tdm> |

## NDM/XML BASIC STRUCTURE

Each constituent NDM (see messages specified in references [4]–[8]) shall consist of a <header> and a <body>.

The NDM body shall consist of one or more <segment> constructs, depending upon the message type.

Each <segment> shall consist of a <metadata>/<data> pair.

NOTE – The <body> and <segment> constructs are not explicitly specified in some of the constituent message documents (see references [4], [5], [6]); however, they are logically implied, and are necessary in order to enforce the strict ordering of metadata and data sections (see section 4).

## Substructure 1: apm, OCM, omm, opm, RDM

The body of several NDMs (e.g., APM, OCM, OMM, OPM, and RDM) shall consist of a single segment, as shown in figure 3‑1. Generally these NDMs describe a single state; the OCM varies from this pattern.

NOTE – In Substructure 1 the <segment> tag is not structurally necessary; however, it is present for symmetry with Substructure 2 in the ‘body’ of the message, enabling re-use of some schema data types.

|  |  |
| --- | --- |
| <header>  </header>  <body>  <segment>  <metadata>  </metadata>  <data>  </data>  </segment>  </body> |  |

Figure 3‑1 : NDM/XML Substructure 1 (Single Segment)

## Substructure 2: aem, oem, tdm, and CDM

The body of several NDMs (e.g., AEM, OEM, and TDM) shall consist of one or more segments, as shown in figure 3‑2. Generally, these messages describe multiple states or tracking data types.

The CDM is a variant of Substructure 2. It contains exactly two segments, and includes a unique ‘Relative Metadata Section’ prior to the first segment (see figure 3‑3).

1. NOTE - The alternation of associated metadata and data sections is the structural element that necessitates the notion of the segment..

|  |  |
| --- | --- |
| <header>  </header>  <body>  <segment>  <metadata>  </metadata>  <data>  </data>  </segment>  <segment>  <metadata>  </metadata>  <data>  </data>  </segment>  .  .  .  <segment>  <metadata>  </metadata>  <data>  </data>  </segment>  </body> |  |

Figure 3‑2 : NDM/XML Substructure 2 (Possible Segment Multiplicity)

|  |  |
| --- | --- |
| <header>  </header>  <body>  <relativeMetadata>  </relativeMetadata>  <segment>  <metadata>  </metadata>  <data>  </data>  </segment>  <segment>  <metadata>  </metadata>  <data>  </data>  </segment>  </body> |  |

Figure 3‑3 : Variant of Substructure 2 for CDM

## NDM/XML Tags

Within the structure and substructures described in 3.2 through 3.4, the individual NDM/XML tags specific to the various message types shall be defined.

NDM/XML tag names shall be identical to the keywords in the reference documents for the KVN representation, with exceptions as noted below and in section 4.

NOTE

1. There are three exceptions for which there is not a strict correspondence between KVN keywords in a reference document and NDM/XML tags:
2. the ‘CCSDS\_xxx\_VERS’ keyword that is present in each document;
3. keywords associated with rotations in the ADM (see 4.8.2); and
4. keywords associated with user-defined parameters in some of the documents (see 4.10).

In the first two exceptions, the KVN keywords appear as XML attributes rather than as XML elements. In the last case, the KVN keywords appear as a combination of XML elements and attributes. The details of these special cases are described in section 4 of this document, which contains instructions for coding instantiations of the specific messages. The use of <userDefinedParameters> is defined in 4.10.

An NDM/XML tag shall be all uppercase if it corresponds directly to a KVN keyword in one of the reference documents.

References [4]–[8] shall define the contents of the specific KVN keyword related NDM/XML tags.

NDM/XML keywords that do not correspond directly to a KVN keyword in one of the special reference documents (references [4]–[8]) shall be in ‘lowerCamelCase’.

## NDM/XML Text ValueS

Text values in NDM/XML instantiations (i.e., the values between the element begin and end tags and the values between opening and closing quotes for XML attributes) shall consist of either all uppercase or all lowercase characters, with exceptions as noted in 3.6.2.

NOTE – In some of the KVN format NDMs, it is stated that constructing text values using mixed case is permitted, and that case is not significant. However, this complicates checking for valid values in an XML schema. For example, if the word ‘cat’ is expected for a text value, but case is not significant, then the schema necessarily will allow the values ‘cat’, ‘Cat’, ‘cAt’, ‘caT’, ‘CAt’, ‘CaT’, ‘cAT’, and ‘CAT’. This is a 2n problem that is not feasible in schema coding for enumerations longer than a few characters. Thus in the NDM/XML schema set, regardless of whether or not mixed case is allowed in the underlying KVN standard, the requirement associated with this note is established.

An exception is made for values between the <COMMENT> and </COMMENT> tags, which may be in any case desired by the user.

# constructing an ndm/xml instance

## Overview

This section provides more detailed instructions for the user on how to create an XML message based on one of the ASCII-text KVN-formatted messages described in references [4]–[8]. In particular, with the current exception of the Attitude Data Messages (reference [4]), the instructions for creating XML formatted messages are described in references [5]–[8].

## XML VERSION

The first line of each instantiation shall specify the XML version, exactly as follows:

<?xml version="1.0" encoding="UTF-8"?>

## BEGINNING THE INSTANTIATION: ROOT ELEMENT TAG

Each instantiation shall have a ‘root element tag’ that identifies the message type and other information specific to the NDM/XML.

NOTE – ‘Other information’ includes things such as where to find the applicable schema, required attributes, etc.

The root element tag in an NDM/XML instantiation shall be one of those listed in the ‘Root Tag’ column of table 3‑1.

The XML Schema Instance namespace attribute must appear in the root element tag of all NDM/XML instantiations, exactly as shown:

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

NOTE: "https:" is not a valid value in the above string, as it is the name of a namespace, not the name of an internet protocol.

The NDM/XML namespace must next be coded, exactly as shown:

xmlns:ndm="urn:ccsds:schema:ndmxml"

The value that follows the ‘xmlns:’ in the NDM/XML name space (‘ndm’ in this case) is a prefix that must be used on every XML tag if it is desired to create an instantiation in an environment that requires ‘elementFormDefault="qualified"’.

NOTE – The NDM/XML schemas for ‘elementFormDefault="qualified"’ and ‘elementFormDefault="unqualified"’ are identical with the exception of the value for the elementFormDefault parameter.

If it is desired to validate an instantiation against the CCSDS Web-based schema, one of the options for the xsi:noNamespaceSchemaLocation attribute must be coded as a single string of non-blank characters, with no line breaks:

xsi:noNamespaceSchemaLocation="https://beta.sanaregistry.org/r/ndmxml\_unqualified/ndmxml-3.0.X-master-3.0.xsd" (if ‘elementFormDefault="unqualified"’ is desired)

xsi:noNamespaceSchemaLocation="https://beta.sanaregistry.org/r/ndmxml\_qualified/ndmxml-3.0.X-master-3.0.xsd" (if ‘elementFormDefault="qualified"’ is desired)

NOTES

1. The value associated with the xsi:noNamespaceSchemaLocation attribute shown in this document is too long to appear on a single line.
2. In the schema name, the ‘X’ in ‘3.0.X’ is the most current revision of the NDM/XML schema set, which can be determined via the SANA Registry. For the initial schema set, X = 0 (i.e., 3.0.0 is the initial schema set).

For use in a local operations environment, the NDM/XML schema set may be downloaded from the CCSDS Web site to a local server that meets local requirements for operations robustness.

If a local version is used, the value associated with the xsi:noNamespaceSchemaLocation attribute must be changed to a URL that is accessible to the local server.

There are two attributes that are required in the root element tag of an NDM/XML single message instantiation, specifically, the CCSDS\_xxx\_VERS keyword that is also part of the standard KVN header, and the Blue Book issue number.

The CCSDS\_xxx\_VERS keyword shall be supplied via the ‘id’ attribute of the root element tag as noted in table 3‑1. The value ‘xxx’ in the ‘id’ attribute must be in all capital letters.

The issue number of the Blue Book to which the schema applies shall be supplied via the ‘version’ attribute.

NOTE – The following example root element tag for an OPM instantiation combines all the directions in the preceding several subsections for both ‘unqualified’ and ‘qualified’ elementFormDefault:

<?xml version="1.0" encoding="UTF-8"?>

<opm xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xmlns:ndm="urn:ccsds:schema:ndmxml"

xsi:noNamespaceSchemaLocation="https://sanaregistry.org/r/ndmxml\_unqualified/ndmxml-3.0.0-master-3.0.xsd"

id="CCSDS\_OPM\_VERS" version="3.0">

<?xml version="1.0" encoding="UTF-8"?>

<ndm:opm xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xmlns:ndm="urn:ccsds:schema:ndmxml"

xsi:noNamespaceSchemaLocation="https://sanaregistry.org/r/ndmxml\_qualified/ndmxml-3.0.0-master-3.0.xsd"

id="CCSDS\_OPM\_VERS" version="3.0">

## The STANDARD NDM/XML Header SECTION

The NDMs shall share a standard header format, with tags <header> and </header>.

Immediately following the <header> tag, the message may have any number of <COMMENT></COMMENT> tag pairs.

The standard NDM header shall contain the <CREATION\_DATE> and the <ORIGINATOR> tags.

NOTE – The rules for these keywords are specified in references [4]–[8]. An example <header> section is shown immediately below for both ‘unqualified’ and ‘qualified’ elementFormDefault. In some of the recent publications, an optional ‘MESSAGE\_ID’ keyword has been included in the message header; details are in the specific reference.

<header>

<COMMENT>This is the common NDM/XML header</COMMENT>

<COMMENT>I can put as many comments here as I want,</COMMENT>

<COMMENT>including none.</COMMENT>

<CREATION\_DATE>2004-281T17:26:06</CREATION\_DATE>

<ORIGINATOR>AGENCY-X</ORIGINATOR>

</header>

<ndm:header>

<ndm:COMMENT>This is the common NDM/XML header</ndm:COMMENT>

<ndm:COMMENT>I can put as many comments here as I want,</ndm:COMMENT>

<ndm:COMMENT>including none.</ndm:COMMENT>

<ndm:CREATION\_DATE>2004-281T17:26:06</ndm:CREATION\_DATE>

<ndm:ORIGINATOR>AGENCY-X</ndm:ORIGINATOR>

</ndm:header>

## The NDM BODY section

After coding the <header>, the instantiation must include a <body></body> tag pair.

Inside the <body></body> tag pair must appear at least one <segment></segment> tag pair.

Each segment must be made up of one or more <metadata></metadata> and <data></data> tag pairs.

## The NDM metadata section

All NDMs must have a metadata section.

The metadata section shall be set off by the <metadata></metadata> tag combination.

Between the <metadata> and </metadata> tags, the keywords shall be the same as those in the metadata sections in references [4]–[8].

## The NDM data section

All NDMs must have a data section.

The data section shall follow the metadata section and shall be set off by the <data></data> tag combination.

Between the <data> and </data> tags, the keywords shall be the same as those in the data sections in the references [4]–[8], with exceptions as noted in the following subsections that discuss creating instantiations of the specific messages.

## CREATING AN AEM INSTANTIATION

### General

An AEM instantiation shall be delimited with the <aem></aem> root element tags using the standard attributes documented in 4.3.

NOTE – Figures G‑1 and G‑2 in annex G provide example AEM instantiations.

The final attributes of the <aem> tag shall be ‘id’ and ‘version’.

The ‘id’ attribute shall be ‘id="CCSDS\_AEM\_VERS"’.

The ‘version’ attribute for the version of the AEM described in reference [4] shall be ‘version="1.0"’.

The standard NDM header shall follow the <aem> tag.

The AEM <body> shall consist of one or more <segment> constructs (see figure 3‑2).

Each <segment> shall consist of a <metadata> section and a <data> section.

The keywords in the <metadata> and <data> sections shall be those specified in reference [4].

NOTE – The rules for including any of the keyword tags in the instantiation are the same as those specified for the AEM in reference [4].

Tags for keywords specified in reference [4] shall be all uppercase as in reference [4].

### SPECIAL TAGS IN the AEM BODY

NOTE – In addition to the AEM keywords specified in reference [4], there are several special tags associated with the AEM body as described in the next few subsections.

The <attitudeState> tag shall be used to encapsulate the keywords associated with the structure of one of the attitude ephemeris data line types.

The NDM/XML tags used within the <attitudeState> structure shall be drawn from table 4‑1.

Table 4‑1 : Special Tags Used in the AEM Body

|  |  |
| --- | --- |
| **AEM ‘ATTITUDE\_TYPE’ Metadata Value** | **Associated NDM/XML Tag in the <attitudeState>** |
| QUATERNION | <quaternionState> |
| QUATERNION/DERIVATIVE | <quaternionDerivative> |
| QUATERNION/RATE | <quaternionEulerRate> |
| EULER\_ANGLE | <eulerAngle> |
| EULER\_ANGLE/RATE | <eulerAngleRate> |
| SPIN | <spin> |
| SPIN/NUTATION | <spinNutation> |

Between the begin tag and end tag (e.g., between <quaternionState> and </quaternionState>), the user shall place the values required by the specific ephemeris data line type as specified in reference [4].

In the XML representation of the AEM, the components of the <attitudeState> ephemeris data line must be represented with keywords (i.e., a tag).

The <attitudeState> keywords shall be the same as those defined for the same construct in the APM.

NOTE – In the KVN representations of the ephemeris data lines, keywords are not used. Rather, the components of the ephemeris data line appear in an order defined by the specific ephemeris data line type.

The <rotation\*> constructs shall be used to encapsulate the keywords associated with the structure of one of the rotation sequences.

NOTE – Some <attitudeState> entries include angles only, or rates only, or both angles and rates.

The NDM/XML tags used within the <rotation\*> structure shall be drawn from table 4‑2.

Table 4‑2 : AEM Rotation Tags

|  |  |
| --- | --- |
| **<attitudeState> Tag** | **Associated Rotation Tag in the <attitudeState>** |
| <quaternionEulerRate> | <rotationRates> |
| <eulerAngle> | <rotationAngles> |
| <eulerAngleRate> | <rotationAngles> followed immediately by <rotationRates>. |

The <rotationAngles> and <rotationRates> elements shall be composed of three tags: <rotation1>, <rotation2>, and <rotation3>.

NOTE – Depending on whether angles or rates are being described, these <rotation*i* > (i=1,2,3) keywords have different attributes.

For <rotation*i*> tags in the <rotationAngles> element, the attributes shall be ‘angle=’ and ‘units="deg"’.

The ‘angle’ attribute must be coded on the <rotation*i*> tag.

The ‘units’ attribute may be coded on the <rotation*i*> tag.

The value associated with the ‘angle’ attribute must be chosen from the values ‘X\_ANGLE’, ‘Y\_ANGLE’, ‘Z\_ANGLE’.

NOTE – ‘X\_ANGLE’, ‘Y\_ANGLE’, and ‘Z\_ANGLE’ are keywords from the KVN AEM.

For <rotation*i*> tags in the <rotationRates> element, the attributes shall be ‘rate=’ and ‘units="deg/s"’.

The ‘rate’ attribute must be coded on the <rotation*i*> tag.

The ‘units’ attribute may be coded on the <rotation*i* > tag.

The value associated with the ‘rate’ attribute must be chosen from the values ‘X\_RATE’, ‘Y\_RATE’, ‘Z\_RATE’.

NOTE – ‘X\_RATE’, ‘Y\_RATE’, and ‘Z\_RATE’ are keywords from the KVN AEM.

### DISCUSSION

This non-normative subsection discusses and provides examples of the use of quaternion tags in the AEM.

The XML representations of quaternions in the ADM constituent messages share a common quaternion definition. However, there are some differences in those definitions in the underlying KVN definitions of the APM and AEM. As in the KVN representation of the quaternion, it is possible to code the tags for the individual components of the quaternion (Q1, Q2, Q3, QC) in either of the standard orders (i.e., scalar component first or last). The following examples are meant to illustrate the standard for representing quaternions in the AEM.

Here is an example AEM quaternion for a ‘QUATERNION’ ephemeris data line:

<attitudeState>

<quaternionState>

<EPOCH>2004-100T00:00:00</EPOCH>

<quaternion>

<Q1>0.00005</Q1>

<Q2>0.87543</Q2>

<Q3>0.40949</Q3>

<QC>0.25678</QC>

</quaternion>

</quaternionState>

</attitudeState>

Here is an example AEM quaternion for a ‘QUATERNION/DERIVATIVE’ ephemeris data line:

<attitudeState>

<quaternionDerivative>

<EPOCH>2004-100T00:00:00</EPOCH>

<quaternion>

<Q1>0.00005</Q1>

<Q2>0.87543</Q2>

<Q3>0.40949</Q3>

<QC>0.25678</QC>

</quaternion>

<quaternionRate>

<Q1\_DOT>0.002</Q1\_DOT>

<Q2\_DOT>0.003</Q2\_DOT>

<Q3\_DOT>0.004</Q3\_DOT>

<QC\_DOT>0.001</QC\_DOT>

</quaternionRate>

</quaternionDerivative>

</attitudeState>

Here is an example AEM quaternion for a ‘QUATERNION/RATE’ ephemeris data line:

<attitudeState>

<quaternionEulerRate>

<EPOCH>2004-100T00:00:00</EPOCH>

<quaternion>

<Q1>0.00005</Q1>

<Q2>0.87543</Q2>

<Q3>0.40949</Q3>

<QC>0.25678</QC>

</quaternion>

<rotationRates>

<rotation1 rate="X\_RATE">1.0</rotation1>

<rotation2 rate="Y\_RATE">1.1</rotation2>

<rotation3 rate="X\_RATE">1.2</rotation3>

</rotationRates>

</quaternionEulerRate>

</attitudeState>

### DISCUSSION

This non-normative subsection discusses and provides examples of the use of rotation tags in the AEM.

The <aem> is notable in that there are XML attributes used to convey the characteristics of rotations instead of XML elements. The AEM includes a number of rotation-related constructs that are necessitated by the fact that attitude rotations are not of one type. The rotation combinations are complicated by the fact that some rotation sequences are specified with more than one rotation about the same axis (e.g., a ‘131’ rotation, in which the first rotation is about the x-axis, second about the z-axis, and the final rotation again about the x-axis). The rotation constructs are used to encapsulate the keywords associated with the structure of one of the rotation sequences. Some <attitudeState> entries include angles only, or rates only, or both angles and rates. The <rotationAngles> and <rotationRates> elements are composed of three tags: <rotation1>, <rotation2>, and <rotation3>. Depending on whether angles or rates are being described, these <rotation*i*> (*i*=1,2,3) keywords have different attributes. For example, the following shows rotation angles for a 321 rotation sequence:

<rotationAngles>

<rotation1 angle="Z\_ANGLE">1.234</rotation1>

<rotation2 angle="Y\_ANGLE">5.678</rotation2>

<rotation3 angle="X\_ANGLE">9.1011</rotation3>

</rotationAngles>

For example, the following shows rotation rates for a 321 rotation sequence:

<rotationRates>

<rotation1 rate="Z\_RATE" units="deg/s">1.234</rotation1>

<rotation2 rate="Y\_RATE" units="deg/s">5.678</rotation2>

<rotation3 rate="X\_RATE" units="deg/s">9.1011</rotation3>

</rotationRates>

## CREATING AN APM INSTANTIATION

An APM instantiation shall be delimited by the <apm></apm> root element tags using the standard attributes documented in 4.3.

NOTE – Figure G‑3 in annex G provides an example APM instantiation.

The final attributes of the <apm> tag shall be ‘id’ and ‘version’.

The ‘id’ attribute shall be ‘id="CCSDS\_APM\_VERS"’.

The ‘version’ attribute for the version of the APM described in reference [4] shall be ‘version="1.0"’.

The standard NDM header shall follow the <apm> tag.

The APM <body> shall consist of a single <segment> (see figure 3‑1).

The segment shall consist of a <metadata> section and a <data> section.

The keywords in the <metadata> and <data> sections shall be those specified in reference [4].

NOTE – The rules for including any of the keyword tags in the instantiation are the same as those specified for the APM in reference [4].

Tags for keywords specified in reference [4] shall be all uppercase as in reference [4].

Several of the NDM/XML APM keywords may have a unit attribute, if desired by the APM producer.

In all cases, the units shall match those defined in reference [4].

Table 4‑3 illustrates the keyword tags for which units may be specified:

Table 4‑3 : APM Tags with Units

| **Keyword** | **Units** | **Example** |
| --- | --- | --- |
| Q1\_DOT | 1/s | <Q1\_DOT units="1/s">numeric-value</Q1\_DOT> |
| Q2\_DOT | 1/s | <Q2\_DOT units="1/s">numeric-value</Q2\_DOT> |
| Q3\_DOT | 1/s | <Q3\_DOT units="1/s">numeric-value</Q3\_DOT> |
| QC\_DOT | 1/s | <QC\_DOT units="1/s">numeric-value</QC\_DOT> |
| SPIN\_ALPHA | deg | <SPIN\_ALPHA units="deg">numeric-value</SPIN\_ALPHA> |
| SPIN\_DELTA | deg | <SPIN\_DELTA units="deg">numeric-value</SPIN\_DELTA> |
| SPIN\_ANGLE | deg | <SPIN\_ANGLE units="deg">numeric-value</SPIN\_ANGLE> |
| SPIN\_ANGLE\_VEL | deg/s | <SPIN\_ANGLE\_VEL units="deg/s">numeric-value</SPIN\_ANGLE\_VEL> |
| NUTATION | deg | <NUTATION units="deg">numeric-value</NUTATION> |
| NUTATION\_PER | s | <NUTATION\_PER units="s">numeric-value</NUTATION\_PER> |
| NUTATION\_PHASE | deg | <NUTATION\_PHASE units="deg">numeric-value</NUTATION\_PHASE> |
| I11 | kg\*m\*\*2 | <I11 units="kg\*m\*\*2">numeric-value</I11> |
| I22 | kg\*m\*\*2 | <I22 units="kg\*m\*\*2">numeric-value</I22> |
| I33 | kg\*m\*\*2 | <I33 units="kg\*m\*\*2">numeric-value</I33> |
| I12 | kg\*m\*\*2 | <I12 units="kg\*m\*\*2">numeric-value</I12> |
| I13 | kg\*m\*\*2 | <I13 units="kg\*m\*\*2">numeric-value</I13> |
| I23 | kg\*m\*\*2 | <I23 units="kg\*m\*\*2">numeric-value</I23> |
| MAN\_DURATION | s | <MAN\_DURATION units="s">numeric-value</MAN\_DURATION> |
| MAN\_TOR\_1 | N\*m | <MAN\_TOR\_1 units="N\*m">numeric-value</MAN\_TOR\_1> |
| MAN\_TOR\_2 | N\*m | <MAN\_TOR\_2 units="N\*m">numeric-value</MAN\_TOR\_2> |
| MAN\_TOR\_3 | N\*m | <MAN\_TOR\_3 units="N\*m">numeric-value</MAN\_TOR\_3> |

### SPECIAL TAGS IN the APM BODY

NOTE – In addition to the APM keywords specified in reference [4], there are several special tags associated with the APM body as described in the next few subsections. The information content in the APM is separated into constructs described in reference [4] as ‘logical blocks’. Special tags in the APM are used to encapsulate the information in the logical blocks of the APM.

The NDM/XML tags used to delimit the logical blocks of the APM shall be drawn from table 4‑4.

Table 4‑4 : Special Tags Used in the APM Body

|  |  |
| --- | --- |
| **APM Logical Block** | **Associated NDM/XML APM Tag** |
| Quaternion | <quaternionState>, <quaternion>, <quaternionRate> |
| Euler Elements / Three Axis Stabilized | <eulerElementsThree> |
| Euler Elements / Spin Stabilized | <eulerElementsSpin> |
| Spacecraft Parameters | <spacecraftParameters> |
| Maneuver Parameters | <maneuverParameters> |

Between the begin tag and end tag (e.g., between <spacecraftParameters> and </spacecraftParameters>), the user shall place the keywords required by the specific logical block as specified in reference [4].

NOTE – The Quaternion logical block has two primary NDM/XML tags associated with it: <quaternionState> and <quaternionRate>; within the <quaternionState> block, there is a <quaternion> tag that contains the components of the quaternion itself.

The <rotation\*> constructs shall be used to encapsulate the keywords associated with the structure of one of the rotation sequences.

The NDM/XML tags used within the <rotation\*> structure shall be drawn from table 4‑5.

Table 4‑5 : APM Rotation Tags

|  |  |
| --- | --- |
| **APM Tag** | **Associated Rotation Tag in the <eulerElementsThree>** |
| <eulerElementsThree>, after the <RATE\_FRAME> tag | <rotationAngles>  <rotationRates> |

The <rotationAngles> and <rotationRates> elements shall be composed of three tags: <rotation1>, <rotation2>, and <rotation3>.

NOTE – Depending on whether angles or rates are being described, these <rotation*i*> (i=1,2,3) keywords have different attributes.

For <rotation*i*> tags in the <rotationAngles> element, the attributes shall be ‘angle=’ and ‘units="deg"’.

The ‘angle’ attribute must be coded on the <rotation*i*> tag.

The ‘units’ attribute may be coded on the <rotation*i*> tag.

The value associated with the ‘angle’ attribute must be chosen from the values ‘X\_ANGLE’, ‘Y\_ANGLE’, ‘Z\_ANGLE’.

NOTE – ‘X\_ANGLE’, ‘Y\_ANGLE’, and ‘Z\_ANGLE’ are keywords from the KVN APM.

For <rotation*i*> tags in the <rotationRates> element, the attributes shall be ‘rate=’ and ‘units="deg/s"’.

The ‘rate’ attribute must be coded on the <rotation*i*> tag.

The ‘units’ attribute may be coded on the <rotation*i*> tag.

The value associated with the ‘rate’ attribute must be chosen from the values ‘X\_RATE’, ‘Y\_RATE’, ‘Z\_RATE’.

NOTE – ‘X\_RATE’, ‘Y\_RATE’, and ‘Z\_RATE’ are keywords from the KVN APM.

### DISCUSSION

This non-normative subsection discusses and provides examples of the use of quaternion tags in the APM.

The XML representations of quaternions in the ADM constituent messages share a common quaternion definition. However, there are some differences in those definitions in the underlying KVN definitions of the APM and AEM. As in the KVN representation of the quaternion, it is possible to code the tags for the individual components of the quaternion (Q1, Q2, Q3, QC) in either of the standard orders (i.e., scalar component first or last). The following examples are meant to illustrate the standard for representing quaternions in the APM.

Here is an example APM quaternion construct:

<quaternionState>

<EPOCH>2004-100T00:00:00Z</EPOCH>

<Q\_FRAME\_A>ICRF</Q\_FRAME\_A>

<Q\_FRAME\_B>ICRF</Q\_FRAME\_B>

<Q\_DIR>B2A</Q\_DIR>

<quaternion>

<Q1>0.00005</Q1>

<Q2>0.87543</Q2>

<Q3>0.40949</Q3>

<QC>0.25678</QC>

</quaternion>

</quaternionState>

Here is an example APM quaternion construct with the optional derivative:

<quaternionState>

<EPOCH>2004-100T00:00:00Z</EPOCH>

<Q\_FRAME\_A>ICRF</Q\_FRAME\_A>

<Q\_FRAME\_B>ICRF</Q\_FRAME\_B>

<Q\_DIR>B2A</Q\_DIR>

<quaternion>

<Q1>0.00005</Q1>

<Q2>0.87543</Q2>

<Q3>0.40949</Q3>

<QC>0.25678</QC>

</quaternion>

<quaternionRate>

<Q1\_DOT>0.002</Q1\_DOT>

<Q2\_DOT>0.003</Q2\_DOT>

<Q3\_DOT>0.004</Q3\_DOT>

<QC\_DOT>0.001</QC\_DOT>

</quaternionRate>

</quaternionState>

### DISCUSSION

This non-normative subsection discusses and provides examples of the use of rotation tags in the APM.

The APM includes two rotation-related constructs that are used in conjunction with the <eulerElementsThree> tag. The rotation combinations are complicated by the fact that some rotation sequences are specified with more than one rotation about the same axis (e.g., a ‘131’ rotation, in which the first rotation is about the x-axis, second about the z-axis, and the final rotation again about the x-axis). The rotation constructs are used to encapsulate the keywords associated with the structure of one of the rotation sequences. As in the KVN APM, angles can be specified without rates, rates can be specified without angles, or both angles and rates can be specified. The <rotationAngles> and <rotationRates> elements are composed of three tags: <rotation1>, <rotation2>, and <rotation3>. Depending on whether angles or rates are being described, these <rotation*i*> (*i*=1,2,3) keywords have different attributes.

For example, the following shows rotation angles for a 321 rotation sequence:

<rotationAngles>

<rotation1 angle="Z\_ANGLE">1.234</rotation1>

<rotation2 angle="Y\_ANGLE">5.678</rotation2>

<rotation3 angle="X\_ANGLE">9.1011</rotation3>

</rotationAngles>

For example, the following shows rotation rates for a 321 rotation sequence:

<rotationRates>

<rotation1 rate="Z\_RATE" units="deg/s">1.234</rotation1>

<rotation2 rate="Y\_RATE" units="deg/s">5.678</rotation2>

<rotation3 rate="X\_RATE" units="deg/s">9.1011</rotation3>

</rotationRates>



























## USER DEFINED PARAMETERS

NOTE – User-defined parameters have been added to some of the Navigation Data Messages (OPM, OMM, OCM (reference [5]); and RDM (reference [8]). As other Navigation Data Message standards are updated, it is likely that the ability to include user-defined parameters will be added to them. These parameters are situation specific and are not standardized. Accordingly, the use of user-defined parameters is not encouraged. Because these parameters are not known to the schema, there is only one very broad keyword offered in the NDM/XML: <USER\_DEFINED>.

### General

User-defined parameters, if utilized, must be specified in ICDs between the exchange participants.

User-defined parameters shall only appear in instantiations of the navigation data messages which have defined them for the KVN format.

User-defined parameters shall appear in a logical block that is offset with the tag set <userDefinedParameters></userDefinedParameters>.

Specific user-defined parameters in an NDM shall utilize the tag <USER\_DEFINED>.

Following the <userDefinedParameters> tag, any number and order of <USER\_DEFINED> tags may appear.

All information about the user-defined parameters shall be conveyed via one attribute of the <USER\_DEFINED> tag (the attribute ‘parameter’) and the <USER\_DEFINED> element value (which may include the applicable units).

In the NDM/XML, the variable-length value associated with the parameter attribute shall be the string following ‘USER\_DEFINED\_’ in the associated KVN keyword.

The data type for the user-defined value shall be ‘xsd:string’, even if the actual user-defined parameter has a numeric value.

### DISCUSSION

For example, the following KVN parameters might appear in an OMM or OPM:

USER\_DEFINED\_ATMOSPHERE\_MODEL = MSISE90

USER\_DEFINED\_C3 = 29.376 [km\*\*2/s\*\*2]

USER\_DEFINED\_EARTH\_RADIUS = 6378.1 [km]

USER\_DEFINED\_3RD\_BODY\_PERTURBATION = JUPITER

These parameters would appear in an NDM/XML representation as:

<userDefinedParameters>

<USER\_DEFINED parameter="ATMOSPHERE\_MODEL">MSISE90</USER\_DEFINED>

<USER\_DEFINED parameter="C3">29.376 [km\*\*2/s\*\*2]</USER\_DEFINED>

<USER\_DEFINED parameter="EARTH\_RADIUS">6378.1 [km]</USER\_DEFINED>

<USER\_DEFINED parameter="3RD\_BODY\_PERTURBATION">JUPITER</USER\_DEFINED>

</userDefinedParameters>

## CREATING AN NDM COMBINED INSTANTIATION

### OVERVIEW

It is possible to create an XML instance that incorporates any number of NDM messages from references listed in references [4]–[8] in a logical suite called an ‘NDM combined instantiation’. Such combined instantiations may be useful for some situations, for example:

* a constellation of spacecraft in which ephemeris data for all of the spacecraft is combined in a single XML message;
* a spacecraft attitude that depends upon a particular orbital state (an APM and its associated OPM could be conveniently conveyed in a single NDM);
* an ephemeris message with the set of tracking data messages used in the orbit determination.

There are many other possible scenarios that may benefit from the combined instantiation approach.

An NDM combined instantiation shall be delimited with the <ndm></ndm> root element tags instead of one of the individual message tags.

The standard attributes documented in 4.3 shall be used with the <ndm> tag, with the exception that neither ‘id’ nor ‘version’ attributes are associated with the <ndm> tag.

In the NDM combined instantiation, the only attributes that shall appear on the constituent message tags are the ‘id’ and ‘version’ attributes, as described in the subsections 4.3.9 through 4.3.11.

Between the <ndm></ndm> tags, the desired messages described in table 3‑1 may be combined.

Any combination of constituent NDM message types may be used in an NDM combined instantiation.

An NDM combined instantiation should consist of at least one constituent message from the references listed in references [4]–[8].

### DISCUSSION

Figures 4‑1 through 4‑3 illustrate the basic structure of an NDM combined instantiation. Figure 4‑1 has removed all detail to contrast the single message NDM with an NDM combined instantiation. In figure 4‑2, the basic structure of an NDM combined instantiation is graphically illustrated. As shown in figure 4‑3, in an NDM combined instantiation, the individual message tags still have the ‘id’ and ‘version’ attributes, but the namespace attributes and schema location attributes are associated with the <ndm> root element.

|  |  |
| --- | --- |
| **Single Message NDM** | **NDM Combined Instantiation** |
| <opm>  <header>  </header>  <body>  </body>  </opm> | <ndm>  <opm>  <header>  </header>  <body>  </body>  </opm>  <apm>  <header>  </header>  <body>  </body>  </apm>  </ndm> |

Figure 4‑1 : Comparison of Single Message NDM with NDM Combined Instantiation

|  |  |
| --- | --- |
| <ndm>  <COMMENT>Generally, at least one AEM, APM, CDM, OCM, OEM, OMM, OPM, RDM, or TDM. Constituent messages can occur in any quantity (0 or more) or order.</COMMENT>  <aem>  </aem>  <apm>  </apm>  <cdm>  </cdm>  <ocm>  </ocm>  <oem>  </oem>  <omm>  </omm>  <opm>  </opm>  <rdm>  </rdm>  <tdm>  </tdm>  </ndm> |  |

Figure 4‑2 : NDM Combined Instantiation Basic Structure

<?xml version="1.0" encoding="UTF-8"?>

<ndm xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xmlns:ndm="urn:ccsds:schema:ndmxml" xsi:noNamespaceSchemaLocation="https://sanaregistry.org/r/ndmxml\_unqualified/ndmxml-3.0.0-master-3.0.xsd">

<apm id="CCSDS\_APM\_VERS" version="1.0">

<header>

</header>

<body>

</body>

</apm>

<aem id="CCSDS\_AEM\_VERS" version="1.0">

<header>

</header>

<body>

</body>

</aem>

<cdm id="CCSDS\_CDM\_VERS" version="1.0">

<header>

</header>

<body>

</body>

</cdm>

<opm id="CCSDS\_OPM\_VERS" version="3.0">

<header>

</header>

<body>

</body>

</opm>

<omm id="CCSDS\_OMM\_VERS" version="3.0">

<header>

</header>

<body>

</body>

</omm>

<oem id="CCSDS\_OEM\_VERS" version="3.0">

<header>

</header>

<body>

</body>

</oem>

<ocm id="CCSDS\_OCM\_VERS" version="3.0">

<header>

</header>

<body>

</body>

</ocm>

<rdm id="CCSDS\_RDM\_VERS" version="1.0">

<header>

</header>

<body>

</body>

</rdm>

<tdm id="CCSDS\_TDM\_VERS" version="2.0">

<header>

</header>

<body>

</body>

</tdm>

</ndm>

Figure 4‑3 : NDM Combined Instantiation Showing Use of Attributes

1. IMPLEMENTATION CONFORMANCE STATEMENT (ICS)   
     
   (Normative)

: This document does not contain an Implementation Conformance Specification (ICS), which is usually shown in Annex A of Blue Books. This is due to the fact that the material in this document simply reflects a re-formatting of some older documents from KVN to XML. The constituent documents listed in Section 1.6 either now contain an ICS, or will contain an ICS Annex upon publication of updated issues now in progress.

1. VALUES FOR SELECTED KEYWORDS   
     
   (Normative)

: This annex is not applicable to the Navigation   
Data Messages XML, though it does apply to other CCSDS Navigation Working Group Standards, which have a consistent ordering of annexes.

1. SECURITY, SANA, AND PATENT CONSIDERATIONS  
      
   (Informative)
   1. SECURITY CONSIDERATIONS
      1. ANALYSIS OF SECURITY CONSIDERATIONS

This annex presents the results of an analysis of security considerations applied to the technologies specified in this Recommended Standard.

* + 1. CONSEQUENCES OF NOT APPLYING SECURITY TO THE TECHNOLOGY

The consequences of not applying security to the systems and networks on which this Recommended Standard is implemented could include potential loss, corruption, and theft of data. Because it is possible to utilize these messages in orbit determination, in preparing pointing and frequency predicts used during spacecraft commanding, and in collision avoidance studies, the consequences of not applying security to the systems and networks on which this Recommended Standard is implemented could include compromise or loss of the mission if malicious tampering of a particularly severe nature occurs.

* + 1. POTENTIAL THREATS AND ATTACK SCENARIOS

Potential threats or attack scenarios include, but are not limited to, (a) unauthorized access to the programs/processes that generate and interpret the messages, (b) unauthorized access to the messages during transmission between exchange partners, and (c) modification of the messages between partners. Protection from unauthorized access during transmission is especially important if the mission utilizes open ground networks such as the Internet to provide ground station connectivity for the exchange of data formatted in compliance with this Recommended Standard. It is strongly recommended that potential threats or attack scenarios applicable to the systems and networks on which this Recommended Standard is implemented be addressed by the management of those systems and networks.

* + 1. DATA PRIVACY

Privacy of data formatted in compliance with the specifications of this Recommended Standard should be assured by the systems and networks on which this Recommended Standard is implemented.

* + 1. DATA INTEGRITY

Integrity of data formatted in compliance with the specifications of this Recommended Standard should be assured by the systems and networks on which this Recommended Standard is implemented.

* + 1. AUTHENTICATION OF COMMUNICATING ENTITIES

Authentication of communicating entities involved in the transport of data that complies with the specifications of this Recommended Standard should be provided by the systems and networks on which this Recommended Standard is implemented.

* + 1. DATA TRANSFER BETWEEN COMMUNICATING ENTITIES

The transfer of data formatted in compliance with this Recommended Standard between communicating entities should be accomplished via secure mechanisms approved by the Information Technology Security functionaries of exchange participants.

* + 1. CONTROL OF ACCESS TO RESOURCES

Control of access to resources should be managed by the systems upon which originator formatting and recipient processing are performed.

* + 1. AUDITING OF RESOURCE USAGE

Auditing of resource usage should be handled by the management of systems and networks on which this Recommended Standard is implemented.

* + 1. UNAUTHORIZED ACCESS

Unauthorized access to the programs/processes that generate and interpret the messages should be prohibited in order to minimize potential threats and attack scenarios.

* + 1. DATA SECURITY IMPLEMENTATION SPECIFICS

Specific information-security interoperability provisions that apply between agencies and other independent users involved in an exchange of data formatted in compliance with this Recommended Standard should be specified in an ICD.

* 1. SANA CONSIDERATIONS

The following NDM/XML related items are registered with the SANA Operator.

* The NDM/XML schemas (see reference [3]).

The values for certain fields in an XML instantiation are also registered with SANA. The details as to these are incorporated in the ‘Security, SANA, and Patent Considerations’ annexes of references [4]–[8].

NOTE – This annex subsection is not present in older Navigation Working Group standards published prior to 2010.

The general policy for changes to the NDM/XML schemas is Expert Review by the Working Group or Area responsible for the NDM/XML standard. Any NDM/XML schema changes in the future will result in supersession of the older schema versions by the newer versions. Older versions will be available for download at https://cwe.ccsds.org/moims/docs/MOIMS-NAV/NDM-XML-Schema-Archive/.

The registration rule for new entries in the registry is the approval of new requests by the CCSDS Area or Working Group responsible for the maintenance of the NDM/XML at the time of the request. New requests for this registry should be sent to SANA (mailto:info@sanaregistry.org).

* 1. PATENT CONSIDERATIONS

The recommendations of this document have no patent issues.

OCM Orbit Comprehensive Message

ocm Orbit Comprehensive Message tag

1. RATIONALE FOR XML-FORMAT NAVIGATION DATA MESSAGES  
     
   (INFORMATIVE)

Table E‑1 : Primary Requirements

|  |  |
| --- | --- |
| E-1-1 | The NDM/XML data must be provided in digital form (computer file). |
| E-1-2 | The NDM/XML shall be represented by a valid XML format descriptor. |
| E-1-3 | The NDM/XML format descriptor shall be hosted on the SANA Registry, whence it can be shared by all agencies exchanging instantiations of the format descriptor. |
| E-1-4 | The NDM/XML shall allow for the representation of all the fields available in the Navigation Data Messages Recommended Standards.[[2]](#footnote-4) |
| E-1-5 | Files must be readily portable between and useable within ‘all’ computational environments in use by Member Agencies choosing to exchange NDMs via XML. |
| E-1-6 | Files must have means of being uniquely identified and clearly annotated. The file name alone is considered insufficient for this purpose. |
| E-1-7 | File name syntax and length must not violate computer constraints for those computing environments in use by Member Agencies. |
| E-1-8 | The NDM/XML shall use XML elements when there is substructure associated with information, for example, maneuver parameters. |
| E-1-9 | The NDM/XML shall use XML elements when there is data type checking associated with information, for example, maneuver parameters. |

Table E‑2 : Heritage Requirements

|  |  |
| --- | --- |
| E-2-1 | The standard shall be, or must include, an ASCII format. |
| E-2-2 | The standard shall not require software supplied by other agencies to process valid instantiations of the NDM/XML schema. |

Table E‑3 : Desirable Characteristics

|  |  |
| --- | --- |
| E-3-1 | The standard should be extensible with no disruption to existing users/uses. |
| E-3-2 | Keywords, values, and terminology in the NDM/XML should be the same as those in the Navigation Data Messages Recommended Standards, insofar as it is possible. |
| E-3-3 | Structures in the NDM/XML should be re-used across the different message types when practical. |
| E-3-4 | The NDM/XML should minimize the use of tags that do not correspond to keywords in the Navigation Data Messages Recommended Standards. |
| E-3-5 | Units may be specified in the NDM/XML instantiations. The standard should provide for clear specification of units of measure. |
| E-3-6 | The NDM/XML may use XML attributes when there is no substructure associated with information (e.g., units specifications). |

1. TECHNICAL MATERIAL AND CONVENTIONS  
     
   (INFORMATIVE)

This annex

* However, there are specific compressors for XML data (e.g., XMILL and XGRIND—references [H5] and [H6]) that are much more efficient than those used for non-XML-formatted ASCII data.

There are several ways in which XML files can be processed, for example: without validation, with validation via Document Type Definition (DTD), with validation via RELAX NG (reference [H7]), with validation via Schematron (reference [H8]), and with validation via XML schema (references [1] and [2]). [https://www.w3.org/](http://www.w3.org/)).

The integrated NDM/XML schema set is stored in the CCSDS SANA repository (reference [3]), accessible by all interested parties.







An assortment of valid



xsi:noNamespaceSchemaLocation="https://beta.sanaregistry.org/r/ndmxml\_unqualified/ndmxml-3.0.0-master-3.0.xsd"

</ORIGINATOR>

</header>

<body>

<segment>

<metadata>

<COMMENT>This file was produced by M.R. Somebody, MSOO NAV, 2002 OCT 04.</COMMENT>

<COMMENT>It is to be used for attitude reconstruction only. The relative accuracy of these</COMMENT>

<COMMENT>attitudes is 0.1 degrees per axis.</COMMENT>

<OBJECT\_NAME>ST5-224</OBJECT\_NAME>

<OBJECT\_ID>2006224</OBJECT\_ID>

<CENTER\_NAME>EARTH</CENTER\_NAME>

<REF\_FRAME\_A>J2000</REF\_FRAME\_A>

<REF\_FRAME\_B>SC\_BODY\_1</REF\_FRAME\_B>

<ATTITUDE\_DIR>A2B</ATTITUDE\_DIR>

<TIME\_SYSTEM>UTC</TIME\_SYSTEM>

<START\_TIME>2006-090T05:00:00.071</START\_TIME>

<USEABLE\_START\_TIME>2006-090T05:00:00.071</USEABLE\_START\_TIME>

<USEABLE\_STOP\_TIME>2006-090T05:00:00.946</USEABLE\_STOP\_TIME>

<STOP\_TIME>2006-090T05:00:00.946</STOP\_TIME>

<ATTITUDE\_TYPE>SPIN</ATTITUDE\_TYPE>

</metadata>

<data>

<COMMENT>Spin KF ground solution, SPINKF rates</COMMENT>

<attitudeState>

<spin>

<EPOCH>2006-090T05:00:00.071</EPOCH>

<SPIN\_ALPHA>2.6862511e+002</SPIN\_ALPHA>

<SPIN\_DELTA>6.8448486e+001</SPIN\_DELTA>

<SPIN\_ANGLE>1.5969509e+002</SPIN\_ANGLE>

<SPIN\_ANGLE\_VEL>-1.0996528e+002</SPIN\_ANGLE\_VEL>

</spin>

</attitudeState>

<attitudeState>

<spin>

<EPOCH>2006-090T05:00:00.196</EPOCH>

<SPIN\_ALPHA>2.6863990e+002</SPIN\_ALPHA>

<SPIN\_DELTA>6.8432197e+001</SPIN\_DELTA>

<SPIN\_ANGLE>1.4593720e+002</SPIN\_ANGLE>

<SPIN\_ANGLE\_VEL>-1.0996493e+002</SPIN\_ANGLE\_VEL>

</spin>

</attitudeState>

<attitudeState>

<spin>

<EPOCH>2006-090T05:00:00.321</EPOCH>

<SPIN\_ALPHA>2.6864591e+002</SPIN\_ALPHA>

<SPIN\_DELTA>6.8412960e+001</SPIN\_DELTA>

<SPIN\_ANGLE>1.3218766e+002</SPIN\_ANGLE>

<SPIN\_ANGLE\_VEL>-1.0996455e+002</SPIN\_ANGLE\_VEL>

</spin>

</attitudeState>

Figure G‑1 : Sample NDM/XML AEM

<attitudeState>

<spin>

<EPOCH>2006-090T05:00:00.446</EPOCH>

<SPIN\_ALPHA>2.6863697e+002</SPIN\_ALPHA>

<SPIN\_DELTA>6.8392049e+001</SPIN\_DELTA>

<SPIN\_ANGLE>1.1845280e+002</SPIN\_ANGLE>

<SPIN\_ANGLE\_VEL>-1.0996402e+002</SPIN\_ANGLE\_VEL>

</spin>

</attitudeState>

<attitudeState>

<spin>

<EPOCH>2006-090T05:00:00.571</EPOCH>

<SPIN\_ALPHA>2.6861072e+002</SPIN\_ALPHA>

<SPIN\_DELTA>6.8371266e+001</SPIN\_DELTA>

<SPIN\_ANGLE>1.0473305e+002</SPIN\_ANGLE>

<SPIN\_ANGLE\_VEL>-1.0996370e+002</SPIN\_ANGLE\_VEL>

</spin>

</attitudeState>

<attitudeState>

<spin>

<EPOCH>2006-090T05:00:00.696</EPOCH>

<SPIN\_ALPHA>2.6856625e+002</SPIN\_ALPHA>

<SPIN\_DELTA>6.8353279e+001</SPIN\_DELTA>

<SPIN\_ANGLE>9.1030304e+001</SPIN\_ANGLE>

<SPIN\_ANGLE\_VEL>-1.0996339e+002</SPIN\_ANGLE\_VEL>

</spin>

</attitudeState>

<attitudeState>

<spin>

<EPOCH>2006-090T05:00:00.821</EPOCH>

<SPIN\_ALPHA>2.6850631e+002</SPIN\_ALPHA>

<SPIN\_DELTA>6.8340398e+001</SPIN\_DELTA>

<SPIN\_ANGLE>7.7341548e+001</SPIN\_ANGLE>

<SPIN\_ANGLE\_VEL>-1.0996317e+002</SPIN\_ANGLE\_VEL>

</spin>

</attitudeState>

<attitudeState>

<spin>

<EPOCH>2006-090T05:00:00.946</EPOCH>

<SPIN\_ALPHA>2.6843571e+002</SPIN\_ALPHA>

<SPIN\_DELTA>6.8332398e+001</SPIN\_DELTA>

<SPIN\_ANGLE>6.3662262e+001</SPIN\_ANGLE>

<SPIN\_ANGLE\_VEL>-1.0996304e+002</SPIN\_ANGLE\_VEL>

</spin>

</attitudeState>

</data>

</segment>

</body>

</aem>

Figure G‑1: Sample NDM/XML AEM (continued)

<?xml version="1.0" encoding="UTF-8"?>

<aem xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xsi:noNamespaceSchemaLocation="https://beta.sanaregistry.org/r/ndmxml\_unqualified/ndmxml-3.0.0-master-3.0.xsd"

id="CCSDS\_AEM\_VERS" version="1.0">

<header>

<COMMENT>This example shows an AEM with a rotation</COMMENT>

<CREATION\_DATE>2008-071T17:09:49</CREATION\_DATE>

<ORIGINATOR>NASA</ORIGINATOR>

</header>

<body>

<segment>

<metadata>

<COMMENT>The relative accuracy of these</COMMENT>

<COMMENT>attitudes is 0.1 degrees per axis.</COMMENT>

<OBJECT\_NAME>FICTITIOUS</OBJECT\_NAME>

<OBJECT\_ID>2020-224A</OBJECT\_ID>

<CENTER\_NAME>EARTH</CENTER\_NAME>

<REF\_FRAME\_A>J2000</REF\_FRAME\_A>

<REF\_FRAME\_B>SC\_BODY\_1</REF\_FRAME\_B>

<ATTITUDE\_DIR>A2B</ATTITUDE\_DIR>

<TIME\_SYSTEM>UTC</TIME\_SYSTEM>

<START\_TIME>2020-090T05:00:00.071</START\_TIME>

<STOP\_TIME>2020-090T05:00:00.946</STOP\_TIME>

<ATTITUDE\_TYPE>EULER\_ANGLE/RATE</ATTITUDE\_TYPE>

</metadata>

<data>

<attitudeState>

<eulerAngleRate>

<EPOCH>2020-090T05:00:00.071</EPOCH>

<rotationAngles>

<rotation1 angle="X\_ANGLE" units="deg">45</rotation1>

<rotation2 angle="Y\_ANGLE" units="deg">0.9</rotation2>

<rotation3 angle="Z\_ANGLE" units="deg">15</rotation3>

</rotationAngles>

<rotationRates>

<rotation1 rate="X\_RATE">4.5</rotation1>

<rotation2 rate="Y\_RATE">0.123</rotation2>

<rotation3 rate="Z\_RATE">15</rotation3>

</rotationRates>

</eulerAngleRate>

</attitudeState>

<attitudeState>

<eulerAngleRate>

<EPOCH>2020-090T05:00:00.946</EPOCH>

<rotationAngles>

<rotation1 angle="X\_ANGLE" units="deg">50</rotation1>

<rotation2 angle="Y\_ANGLE" units="deg">1.9</rotation2>

<rotation3 angle="Z\_ANGLE" units="deg">1.5</rotation3>

</rotationAngles>

<rotationRates>

<rotation1 rate="X\_RATE">1.0</rotation1>

<rotation2 rate="Y\_RATE">0.123</rotation2>

<rotation3 rate="Z\_RATE">1.5</rotation3>

</rotationRates>

</eulerAngleRate>

</attitudeState>

</data>

</segment>

</body>

</aem>

Figure G‑2 : Sample NDM/XML AEM with Rotation

* 1. SAMPLE NDM/XML APM

The following is a simple sample of an NDM/XML APM:

<?xml version="1.0" encoding="UTF-8"?>

<apm xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xsi:noNamespaceSchemaLocation="https://beta.sanaregistry.org/r/ndmxml\_unqualified/ndmxml-3.0.0-master-3.0.xsd"

id="CCSDS\_APM\_VERS" version="1.0">

<header>

<COMMENT>This example corresponds to ADM Blue Book Figure 3-8</COMMENT>

<CREATION\_DATE>2004-02-14T19:23:57</CREATION\_DATE>

<ORIGINATOR>NASA</ORIGINATOR>

</header>

<body>

<segment>

<metadata>

<OBJECT\_NAME>MARS SPIRIT</OBJECT\_NAME>

<OBJECT\_ID>2004-003A</OBJECT\_ID>

<CENTER\_NAME>EARTH</CENTER\_NAME>

<TIME\_SYSTEM>UTC</TIME\_SYSTEM>

</metadata>

<data>

<COMMENT>GEOCENTRIC, CARTESIAN, EARTH FIXED</COMMENT>

<COMMENT>OBJECT\_ID: 2004-003</COMMENT>

<COMMENT>$ITIM = 2004 JAN 14 22:26:18.400000, original launch 14:36</COMMENT>

<COMMENT>Generated by NASA</COMMENT>

<COMMENT>Current attitude for orbit 20 and attitude maneuver</COMMENT>

<COMMENT>planning data.</COMMENT>

<COMMENT>Attitude state quaternion</COMMENT>

<quaternionState>

<EPOCH>2004-02-14T14:28:15.1172</EPOCH>

<Q\_FRAME\_A>INSTRUMENT\_1</Q\_FRAME\_A>

<Q\_FRAME\_B>ITRF1997</Q\_FRAME\_B>

<Q\_DIR>A2B</Q\_DIR>

<quaternion>

<Q1>0.03123</Q1>

<Q2>0.78543</Q2>

<Q3>0.39158</Q3>

<QC>0.47832</QC>

</quaternion>

</quaternionState>

<eulerElementsThree>

<COMMENT>Attitude specified as Euler elements</COMMENT>

<EULER\_FRAME\_A>INSTRUMENT\_1</EULER\_FRAME\_A>

<EULER\_FRAME\_B>ITRF1997</EULER\_FRAME\_B>

<EULER\_DIR>A2B</EULER\_DIR>

<EULER\_ROT\_SEQ>312</EULER\_ROT\_SEQ>

<RATE\_FRAME>EULER\_FRAME\_A</RATE\_FRAME>

<rotationAngles>

<rotation1 angle="Z\_ANGLE" units="deg">-53.3688</rotation1>

<rotation2 angle="X\_ANGLE" units="deg">139.7527</rotation2>

<rotation3 angle="Y\_ANGLE" units="deg">25.0658</rotation3>

</rotationAngles>

<rotationRates>

<rotation1 rate="Z\_RATE" units="deg/s">0.02156</rotation1>

<rotation2 rate="X\_RATE" units="deg/s">0.1045</rotation2>

<rotation3 rate="Y\_RATE" units="deg/s">0.03214</rotation3>

</rotationRates>

Figure G‑3 : Sample NDM/XML APM

</eulerElementsThree>

<spacecraftParameters>

<COMMENT>Spacecraft Parameters</COMMENT>

<I11 units="kg\*m\*\*2">6080.0</I11>

<I22 units="kg\*m\*\*2">5245.5</I22>

<I33 units="kg\*m\*\*2">8067.3</I33>

<I12 units="kg\*m\*\*2">-135.9</I12>

<I13 units="kg\*m\*\*2">89.3</I13>

<I23 units="kg\*m\*\*2">-90.7</I23>

</spacecraftParameters>

<maneuverParameters>

<COMMENT> Data follows for 1 planned maneuver.</COMMENT>

<COMMENT> First attitude maneuver for: MARS SPIRIT</COMMENT>

<COMMENT> Impulsive, torque direction fixed in body frame</COMMENT>

<MAN\_EPOCH\_START>2004-02-14T14:29:00.5098</MAN\_EPOCH\_START>

<MAN\_DURATION units="s">3</MAN\_DURATION>

<MAN\_REF\_FRAME>INSTRUMENT\_1</MAN\_REF\_FRAME>

<MAN\_TOR\_1 units="N\*m">-1.25</MAN\_TOR\_1>

<MAN\_TOR\_2 units="N\*m">-0.5</MAN\_TOR\_2>

<MAN\_TOR\_3 units="N\*m">0.5</MAN\_TOR\_3>

</maneuverParameters>

</data>

</segment>

</body>

</apm>

Figure G‑3: Sample NDM/XML APM (continued)

* 1. SAMPLE QUALIFIED NDM/XML Instance

The following is a simple sample of a qualified NDM/XML instance:

<?xml version="1.0" encoding="UTF-8"?>

<ndm xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xmlns:ndm="urn:ccsds:schema:ndmxml"

xsi:noNamespaceSchemaLocation="https://beta.sanaregistry.org/r/ndmxml\_qualified/ndmxml-3.0.0-master-3.0.xsd">

<ndm:opm id="CCSDS\_OPM\_VERS" version="3.0">

<ndm:header>

<ndm:COMMENT>In this simple case, there are no Keplerian elements, no maneuver, no S/C parameters, no covariance matrix; this is essentially just the state vector</ndm:COMMENT>

<ndm:CREATION\_DATE>2009-05-18T13:06:00</ndm:CREATION\_DATE>

<ndm:ORIGINATOR>GSFC</ndm:ORIGINATOR>

</ndm:header>

<ndm:body>

<ndm:segment>

<ndm:metadata>

<ndm:OBJECT\_NAME>SOHO</ndm:OBJECT\_NAME>

<ndm:OBJECT\_ID>2009-000A</ndm:OBJECT\_ID>

<ndm:CENTER\_NAME>EARTH</ndm:CENTER\_NAME>

<ndm:REF\_FRAME>EME2000</ndm:REF\_FRAME>

<ndm:TIME\_SYSTEM>UTC</ndm:TIME\_SYSTEM>

</ndm:metadata>

<ndm:data>

<ndm:stateVector>

<ndm:EPOCH>2009-04-28T00:00:00</ndm:EPOCH>

<ndm:X>0.11480770338073E+07</ndm:X>

<ndm:Y>0.50826618901580E+06</ndm:Y>

<ndm:Z>0.32422917889939E+06</ndm:Z>

<ndm:X\_DOT>-0.29736064079430</ndm:X\_DOT>

<ndm:Y\_DOT>0.39070228393147</ndm:Y\_DOT>

<ndm:Z\_DOT>0.19156258887615</ndm:Z\_DOT>

</ndm:stateVector>

</ndm:data>

</ndm:segment>

</ndm:body>

</ndm:opm>

<ndm:opm id="CCSDS\_OPM\_VERS" version="3.0">

<ndm:header>

<ndm:CREATION\_DATE>2009-05-18T13:06:00</ndm:CREATION\_DATE>

<ndm:ORIGINATOR>GSFC</ndm:ORIGINATOR>

</ndm:header>

<ndm:body>

<ndm:segment>

<ndm:metadata>

<ndm:OBJECT\_NAME>SOHO</ndm:OBJECT\_NAME>

<ndm:OBJECT\_ID>2009-000A</ndm:OBJECT\_ID>

<ndm:CENTER\_NAME>EARTH</ndm:CENTER\_NAME>

<ndm:REF\_FRAME>EME2000</ndm:REF\_FRAME>

<ndm:TIME\_SYSTEM>UTC</ndm:TIME\_SYSTEM>

</ndm:metadata>

<ndm:data>

<ndm:stateVector>

<ndm:EPOCH>2009-04-28T00:00:00</ndm:EPOCH>

<ndm:X>0.11480770338073E+07</ndm:X>

<ndm:Y>0.50826618901580E+06</ndm:Y>

<ndm:Z>0.32422917889939E+06</ndm:Z>

<ndm:X\_DOT>-0.29736064079430</ndm:X\_DOT>

<ndm:Y\_DOT>0.39070228393147</ndm:Y\_DOT>

<ndm:Z\_DOT>0.19156258887615</ndm:Z\_DOT>

</ndm:stateVector>

</ndm:data>

</ndm:segment>

</ndm:body>

</ndm:opm>

</ndm>

Figure G‑4 : Sample Combined Instantiation with elementFormDefault="qualified"

1. InfoRmative References  
      
   (Informative)

[H1] *Navigation Data—Definitions and Conventions*. Issue 4. Report Concerning Space Data System Standards (Green Book), CCSDS 500.0-G-4. Washington, D.C.: CCSDS, November 2019.

[H2] Fran Martínez. “XML in CCSDS.” Presented at CCSDS Navigation Working Group meeting (May 2004, Montreal). https://cwe.ccsds.org/moims/docs/MOIMS-NAV/NDM%20XML%20Related%20Material/XML-in-CCSDS-Montreal-2004.ppt.

[H3] *Space Communication Cross Support—Service Management—Service Specification*. Issue 1-S. Recommendation for Space Data System Standards (Historical), CCSDS 910.11-B-1-S. Washington, D.C.: CCSDS, (August 2009) June 2017.

[H4] *Information Technology—8-Bit Single-Byte Coded Graphic Character Sets—Part 1: Latin Alphabet No. 1*. International Standard, ISO/IEC 8859-1:1998. Geneva: ISO, 1998.

[H5] "SourceForge.net: XMill." SourceForge.net: Open Source Software. https://sourceforge.net/projects/xmill.

[H6] "SourceForge.net: XGrind: A Query-Friendly XML Compressor." SourceForge.net: Open Source Software. https://sourceforge.net/projects/xgrind/.

[H7] RELAX NG home page. https://relaxng.org/.

[H8] *Information Technology—Document Schema Definition Languages (DSDL)—Part 3: Rule-Based Validation—Schematron*. 3rd ed. International Standard, ISO/IEC 19757-3:2020. Geneva: ISO, 2020.

NOTE – Normative references appear in 1.6.



|  |  |
| --- | --- |

|  |  |
| --- | --- |

|  |  |
| --- | --- |

1. ITEMS FOR AN INTERFACE CONTROL DOCUMENT (ICD)  
      
   (INFORMATIVE)

This Annex lists a number of items that should be covered in interagency ICDs prior to  
exchanging NDMs on a regular basis. There are some statements in the document  
that refer to the desirability or necessity of such a document; this annex consolidates the  
suggested ICD items in a single list.

* The means of transmission of an XML-formatted NDM between exchange participants (see 1.2)
* User-defined parameters, if utilized (see 4.10.1.1)
* Specific information-security interoperability provisions that apply between agencies and other independent users (see C.1.11)

1. CHANGES IN NDM/XML VERSION 3  
      
   (INFORMATIVE)

1. Detailed material related to creating XML instantiations of the Orbit Data Messages (ODM) has been removed. This material is now described in the ODM version 3, reference [5].

2. The document annexes have been rearranged relative to the previous version to conform to a guideline developed for all of the CCSDS Navigation Working Group documents.

1. In this document, ‘Blue Book version’ is synonymous with ‘Blue Book issue’. [↑](#footnote-ref-3)
2. These are the references listed in references [4]–[8]. [↑](#footnote-ref-4)